../Drivers/STM32H5xx_HAL_Driver/Src/stm32h5xx_hal_uart_ex.c:166:19:HAL_RS485Ex_Init	5
../Drivers/STM32H5xx_HAL_Driver/Src/stm32h5xx_hal_uart_ex.c:274:13:HAL_UARTEx_WakeupCallback	1
../Drivers/STM32H5xx_HAL_Driver/Src/stm32h5xx_hal_uart_ex.c:289:13:HAL_UARTEx_RxFifoFullCallback	1
../Drivers/STM32H5xx_HAL_Driver/Src/stm32h5xx_hal_uart_ex.c:304:13:HAL_UARTEx_TxFifoEmptyCallback	1
../Drivers/STM32H5xx_HAL_Driver/Src/stm32h5xx_hal_uart_ex.c:389:19:HAL_MultiProcessorEx_AddressLength_Set	2
../Drivers/STM32H5xx_HAL_Driver/Src/stm32h5xx_hal_uart_ex.c:427:19:HAL_UARTEx_StopModeWakeUpSourceConfig	4
../Drivers/STM32H5xx_HAL_Driver/Src/stm32h5xx_hal_uart_ex.c:482:19:HAL_UARTEx_EnableStopMode	3
../Drivers/STM32H5xx_HAL_Driver/Src/stm32h5xx_hal_uart_ex.c:501:19:HAL_UARTEx_DisableStopMode	3
../Drivers/STM32H5xx_HAL_Driver/Src/stm32h5xx_hal_uart_ex.c:520:19:HAL_UARTEx_EnableFifoMode	2
../Drivers/STM32H5xx_HAL_Driver/Src/stm32h5xx_hal_uart_ex.c:561:19:HAL_UARTEx_DisableFifoMode	2
../Drivers/STM32H5xx_HAL_Driver/Src/stm32h5xx_hal_uart_ex.c:607:19:HAL_UARTEx_SetTxFifoThreshold	2
../Drivers/STM32H5xx_HAL_Driver/Src/stm32h5xx_hal_uart_ex.c:656:19:HAL_UARTEx_SetRxFifoThreshold	2
../Drivers/STM32H5xx_HAL_Driver/Src/stm32h5xx_hal_uart_ex.c:713:19:HAL_UARTEx_ReceiveToIdle	21
../Drivers/STM32H5xx_HAL_Driver/Src/stm32h5xx_hal_uart_ex.c:844:19:HAL_UARTEx_ReceiveToIdle_IT	7
../Drivers/STM32H5xx_HAL_Driver/Src/stm32h5xx_hal_uart_ex.c:910:19:HAL_UARTEx_ReceiveToIdle_DMA	7
../Drivers/STM32H5xx_HAL_Driver/Src/stm32h5xx_hal_uart_ex.c:979:29:HAL_UARTEx_GetRxEventType	1
../Drivers/STM32H5xx_HAL_Driver/Src/stm32h5xx_hal_uart_ex.c:1003:13:UARTEx_Wakeup_AddressConfig	1
../Drivers/STM32H5xx_HAL_Driver/Src/stm32h5xx_hal_uart_ex.c:1021:13:UARTEx_SetNbDataToProcess	2
