"Reference","Value","Datasheet","Footprint","Qty","DNP"
"C1,C2,C3,C4,C9,C15,C16,C17,C18,C19","100n","~","Capacitor_SMD:C_1206_3216Metric","10",""
"C5","4700p 100V","~","Capacitor_THT:C_Disc_D4.3mm_W1.9mm_P5.00mm","1",""
"C6,C8","47p 100v-0805","~","Capacitor_SMD:C_0805_2012Metric","2",""
"C7","10u","~","Capacitor_SMD:C_1206_3216Metric","1",""
"C10","2.2u","~","Capacitor_SMD:CP_Elec_4x4.5","1",""
"C11,C12","47p","~","Capacitor_SMD:C_0805_2012Metric","2",""
"C13,C14","C_Small","~","Capacitor_SMD:C_1206_3216Metric","2",""
"C20","10n","~","Capacitor_SMD:C_1206_3216Metric","1",""
"C21","220u","~","Capacitor_SMD:CP_Elec_8x5.4","1",""
"D1,D2","MMBZxx","http://www.onsemi.com/pub/Collateral/MMBZ5V6ALT1-D.PDF","Package_TO_SOT_SMD:SOT-23","2",""
"D3","1n457","~","Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal","1",""
"D4","B340","http://www.jameco.com/Jameco/Products/ProdDS/1538777.pdf","Diode_SMD:D_SMC","1",""
"D12,D13","ABS2","https://diotec.com/tl_files/diotec/files/pdf/datasheets/abs2.pdf","Diode_SMD:Diode_Bridge_Diotec_ABS","2",""
"J1,J4","Conn_01x02_Pin","~","-- różne wartości --","2",""
"J2,J3","Screw_Terminal_01x04","~","TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-4-5.08_1x04_P5.08mm_Horizontal","2",""
"J5,J6","Conn_01x03_Pin","~","Connector_JST:JST_PH_B3B-PH-K_1x03_P2.00mm_Vertical","2",""
"J7","Conn_ARM_JTAG_SWD_10","http://infocenter.arm.com/help/topic/com.arm.doc.ddi0314h/DDI0314H_coresight_components_trm.pdf","Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical","1",""
"J8,J9","testpoint","~","Connector_Wire:SolderWirePad_1x01_SMD_1x2mm","2",""
"L1","10uH","~","Inductor_SMD:L_2512_6332Metric","1",""
"L2","15uH","~","Inductor_SMD:L_2512_6332Metric","1",""
"Q1,Q3","BTA16-600B","https://www.st.com/resource/en/datasheet/bta16.pdf","Package_TO_SOT_THT:TO-247-3_Horizontal_TabUp","2",""
"Q2,Q4","BC818","https://www.onsemi.com/pub/Collateral/BC818-D.pdf","Package_TO_SOT_SMD:SOT-23","2",""
"R1,R2","60.4R 1%","~","Resistor_SMD:R_1206_3216Metric","2",""
"R3,R6","180","~","Resistor_SMD:R_2010_5025Metric","2",""
"R4,R5,R7,R8,R13,R14","4k7","~","Resistor_SMD:R_1206_3216Metric","6",""
"R9,R10,R11,R12,Ra1,Rf1","100k","~","-- różne wartości --","6",""
"R15","6k2","~","Resistor_SMD:R_1206_3216Metric","1",""
"R16","2k","~","Resistor_SMD:R_1206_3216Metric","1",""
"Ra2","3k57","~","Resistor_SMD:R_1206_3216Metric","1",""
"Rb1","80k6","~","Resistor_SMD:R_1206_3216Metric","1",""
"Rf2","102k","~","Resistor_SMD:R_1206_3216Metric","1",""
"Rg1","3k48","~","Resistor_SMD:R_1206_3216Metric","1",""
"Rs1","1330 1%","~","Resistor_SMD:R_1206_3216Metric","1",""
"Rset1","133 1%","~","Resistor_SMD:R_1206_3216Metric","1",""
"U1","MCP2562-E-SN","http://ww1.microchip.com/downloads/en/DeviceDoc/25167A.pdf","Package_SO:SOIC-8_3.9x4.9mm_P1.27mm","1",""
"U2","LF33_TO252","http://www.st.com/content/ccc/resource/technical/document/datasheet/c4/0e/7e/2a/be/bc/4c/bd/CD00000546.pdf/files/CD00000546.pdf/jcr:content/translations/en.CD00000546.pdf","Package_TO_SOT_SMD:TO-252-2","1",""
"U3","TPS5430DDA","http://www.ti.com/lit/ds/symlink/tps5430.pdf","Package_SO:TI_SO-PowerPAD-8_ThermalVias","1",""
"U5,U6","ACS730xLCTR-20AB","http://www.allegromicro.com/~/media/Files/Datasheets/ACS730-Datasheet.ashx?la=en","Package_SO:SOIC-8_3.9x4.9mm_P1.27mm","2",""
"U7","STM32H503CBTx","https://www.st.com/resource/en/datasheet/stm32h503cb.pdf","Package_QFP:LQFP-48_7x7mm_P0.5mm","1",""
"U8,U13","FODM3052","https://www.onsemi.com/pub/Collateral/FODM3053_NF098-D.PDF","Package_DIP:SMDIP-4_W7.62mm","2",""
"U9,U10","TS5A23159DGS","http://www.ti.com/lit/ds/symlink/ts5a23159.pdf","Package_SO:VSSOP-10_3x3mm_P0.5mm","2",""
"U11","TS912","www.st.com/resource/en/datasheet/ts912.pdf","Package_SO:SOIC-8_3.9x4.9mm_P1.27mm","1",""
"U12","LM334M","http://www.ti.com/lit/ds/symlink/lm134.pdf","Package_SO:SOIC-8_3.9x4.9mm_P1.27mm","1",""
"U15,U16","SFH617A-1X007T","http://www.vishay.com/docs/83740/sfh617a.pdf","Package_DIP:SMDIP-4_W9.53mm_Clearance8mm","2",""
