(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal "Górna sygnałowa")
		(31 "B.Cu" signal "Dolna sygnałowa")
		(32 "B.Adhes" user "Dolna kleju")
		(33 "F.Adhes" user "Górna kleju")
		(34 "B.Paste" user "Dolna pasty")
		(35 "F.Paste" user "Górna pasty")
		(36 "B.SilkS" user "Dolna opisowa")
		(37 "F.SilkS" user "Górna opisowa")
		(38 "B.Mask" user "Dolna sodermaski")
		(39 "F.Mask" user "Górna soldermaski")
		(40 "Dwgs.User" user "Rysunkowa użytkownika")
		(41 "Cmts.User" user "Komentarzy użytkownika")
		(42 "Eco1.User" user "Inżynieryjna 1")
		(43 "Eco2.User" user "Inżynieryjna 2")
		(44 "Edge.Cuts" user "Krawędziowa")
		(45 "Margin" user "Marginesu")
		(46 "B.CrtYd" user "Dolne pola zajętości")
		(47 "F.CrtYd" user "Górne pola zajętości")
		(48 "B.Fab" user "Dolna produkcyjna")
		(49 "F.Fab" user "Górna produkcyjna")
		(50 "User.1" user "Użytkownika 1")
		(51 "User.2" user "Użytkownika 2")
		(52 "User.3" user "Użytkownika 3")
		(53 "User.4" user "Użytkownika 4")
		(54 "User.5" user "Użytkownika 5")
		(55 "User.6" user "Użytkownika 6")
		(56 "User.7" user "Użytkownika 7")
		(57 "User.8" user "Użytkownika 8")
		(58 "User.9" user "Użytkownika 9")
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "/Triac Circuit/High_Voltage_Out")
	(net 2 "/Triac Circuit1/High_Voltage_Out")
	(net 3 "/Triac Circuit2/High_Voltage_Out")
	(net 4 "/Triac Circuit3/High_Voltage_Out")
	(net 5 "/Triac Circuit4/High_Voltage_Out")
	(net 6 "/Triac Circuit5/High_Voltage_Out")
	(net 7 "/Triac Circuit6/High_Voltage_Out")
	(net 8 "/Triac Circuit7/High_Voltage_Out")
	(net 9 "/Triac Circuit8/High_Voltage_Out")
	(net 10 "/Triac Circuit9/High_Voltage_Out")
	(net 11 "/Triac Circuit10/High_Voltage_Out")
	(net 12 "/Triac Circuit11/High_Voltage_Out")
	(net 13 "/Triac Circuit12/High_Voltage_Out")
	(net 14 "/Triac Circuit13/High_Voltage_Out")
	(net 15 "/Triac Circuit14/High_Voltage_Out")
	(net 16 "/Triac Circuit15/High_Voltage_Out")
	(net 17 "/Triac Circuit/High_Voltage_L")
	(net 18 "/Triac Circuit1/High_Voltage_L")
	(net 19 "/Triac Circuit2/High_Voltage_L")
	(net 20 "/Triac Circuit3/High_Voltage_L")
	(net 21 "/Triac Circuit/Enable")
	(net 22 "/Triac Circuit1/Enable")
	(net 23 "Net-(Q1-G)")
	(net 24 "/Triac Circuit2/Enable")
	(net 25 "/Triac Circuit3/Enable")
	(net 26 "Net-(Q7-G)")
	(net 27 "/Triac Circuit4/Enable")
	(net 28 "Net-(Q3-G)")
	(net 29 "/Triac Circuit5/Enable")
	(net 30 "Net-(Q13-G)")
	(net 31 "/Triac Circuit6/Enable")
	(net 32 "/Triac Circuit7/Enable")
	(net 33 "Net-(Q5-G)")
	(net 34 "Net-(Q9-G)")
	(net 35 "Net-(Q11-G)")
	(net 36 "Net-(Q15-G)")
	(net 37 "+3V3")
	(net 38 "Net-(R13-Pad1)")
	(net 39 "Net-(R16-Pad1)")
	(net 40 "Net-(Q2-B)")
	(net 41 "GND")
	(net 42 "Net-(R37-Pad1)")
	(net 43 "Net-(R40-Pad1)")
	(net 44 "Net-(Q2-C)")
	(net 45 "unconnected-(U4-NC-Pad3)")
	(net 46 "Net-(Q4-B)")
	(net 47 "unconnected-(U6-NC-Pad3)")
	(net 48 "Net-(R1-Pad1)")
	(net 49 "unconnected-(U8-NC-Pad3)")
	(net 50 "Net-(Q4-C)")
	(net 51 "Net-(R4-Pad1)")
	(net 52 "unconnected-(U10-NC-Pad3)")
	(net 53 "Net-(Q6-B)")
	(net 54 "Net-(R7-Pad1)")
	(net 55 "unconnected-(U12-NC-Pad3)")
	(net 56 "Net-(Q6-C)")
	(net 57 "Net-(R10-Pad1)")
	(net 58 "unconnected-(U14-NC-Pad3)")
	(net 59 "Net-(Q8-B)")
	(net 60 "Net-(Q8-C)")
	(net 61 "unconnected-(U16-NC-Pad3)")
	(net 62 "Net-(Q10-B)")
	(net 63 "Net-(R19-Pad1)")
	(net 64 "Net-(R22-Pad1)")
	(net 65 "Net-(R25-Pad1)")
	(net 66 "Net-(Q10-C)")
	(net 67 "Net-(R28-Pad1)")
	(net 68 "Net-(Q12-B)")
	(net 69 "Net-(R31-Pad1)")
	(net 70 "Net-(Q12-C)")
	(net 71 "Net-(R34-Pad1)")
	(net 72 "Net-(Q14-B)")
	(net 73 "Net-(Q14-C)")
	(net 74 "Net-(Q16-B)")
	(net 75 "Net-(R43-Pad1)")
	(net 76 "/Triac Circuit4/High_Voltage_L")
	(net 77 "/Triac Circuit5/High_Voltage_L")
	(net 78 "/Triac Circuit6/High_Voltage_L")
	(net 79 "/Triac Circuit7/High_Voltage_L")
	(net 80 "/Triac Circuit8/High_Voltage_L")
	(net 81 "/Triac Circuit9/High_Voltage_L")
	(net 82 "/Triac Circuit10/High_Voltage_L")
	(net 83 "/Triac Circuit11/High_Voltage_L")
	(net 84 "/Triac Circuit12/High_Voltage_L")
	(net 85 "/Triac Circuit13/High_Voltage_L")
	(net 86 "/Triac Circuit14/High_Voltage_L")
	(net 87 "/Triac Circuit15/High_Voltage_L")
	(net 88 "Net-(R46-Pad1)")
	(net 89 "unconnected-(U4-NC-Pad5)")
	(net 90 "unconnected-(U5-NC-Pad3)")
	(net 91 "unconnected-(U5-NC-Pad5)")
	(net 92 "unconnected-(U6-NC-Pad5)")
	(net 93 "unconnected-(U7-NC-Pad3)")
	(net 94 "unconnected-(U7-NC-Pad5)")
	(net 95 "unconnected-(U8-NC-Pad5)")
	(net 96 "unconnected-(U9-NC-Pad3)")
	(net 97 "unconnected-(U9-NC-Pad5)")
	(net 98 "unconnected-(U10-NC-Pad5)")
	(net 99 "unconnected-(U11-NC-Pad3)")
	(net 100 "unconnected-(U11-NC-Pad5)")
	(net 101 "unconnected-(U12-NC-Pad5)")
	(net 102 "unconnected-(U13-NC-Pad3)")
	(net 103 "unconnected-(U13-NC-Pad5)")
	(net 104 "unconnected-(U14-NC-Pad5)")
	(net 105 "unconnected-(U15-NC-Pad3)")
	(net 106 "unconnected-(U15-NC-Pad5)")
	(net 107 "unconnected-(U16-NC-Pad5)")
	(net 108 "Net-(SW1-Pad10)")
	(net 109 "Net-(R2-Pad1)")
	(net 110 "Net-(R5-Pad1)")
	(net 111 "Net-(R8-Pad1)")
	(net 112 "Net-(R11-Pad1)")
	(net 113 "Net-(R14-Pad1)")
	(net 114 "Net-(R17-Pad1)")
	(net 115 "Net-(R20-Pad1)")
	(net 116 "Net-(R23-Pad1)")
	(net 117 "Net-(R26-Pad1)")
	(net 118 "Net-(R29-Pad1)")
	(net 119 "Net-(R32-Pad1)")
	(net 120 "Net-(R35-Pad1)")
	(net 121 "Net-(R38-Pad1)")
	(net 122 "Net-(R41-Pad1)")
	(net 123 "unconnected-(U17-NC-Pad3)")
	(net 124 "unconnected-(U17-NC-Pad5)")
	(net 125 "Net-(R44-Pad1)")
	(net 126 "Net-(Q16-C)")
	(net 127 "Net-(Q17-G)")
	(net 128 "Net-(R47-Pad1)")
	(net 129 "Net-(Q18-B)")
	(net 130 "Net-(Q18-C)")
	(net 131 "/Triac Circuit8/Enable")
	(net 132 "/Triac Circuit9/Enable")
	(net 133 "/Triac Circuit10/Enable")
	(net 134 "/Triac Circuit11/Enable")
	(net 135 "/Triac Circuit12/Enable")
	(net 136 "/Triac Circuit13/Enable")
	(net 137 "/Triac Circuit14/Enable")
	(net 138 "/Triac Circuit15/Enable")
	(net 139 "Net-(Q19-G)")
	(net 140 "Net-(Q20-B)")
	(net 141 "Net-(Q20-C)")
	(net 142 "Net-(Q21-G)")
	(net 143 "Net-(Q22-B)")
	(net 144 "Net-(Q22-C)")
	(net 145 "Net-(Q23-G)")
	(net 146 "Net-(Q24-B)")
	(net 147 "Net-(Q24-C)")
	(net 148 "Net-(Q25-G)")
	(net 149 "Net-(Q26-B)")
	(net 150 "Net-(Q26-C)")
	(net 151 "Net-(Q27-G)")
	(net 152 "Net-(Q28-B)")
	(net 153 "Net-(Q28-C)")
	(net 154 "Net-(Q29-G)")
	(net 155 "Net-(Q30-B)")
	(net 156 "Net-(Q30-C)")
	(net 157 "Net-(Q31-G)")
	(net 158 "Net-(Q32-B)")
	(net 159 "Net-(Q32-C)")
	(net 160 "unconnected-(U2-NC-Pad3)")
	(net 161 "unconnected-(U2-NC-Pad5)")
	(net 162 "unconnected-(U3-NC-Pad3)")
	(net 163 "unconnected-(U3-NC-Pad5)")
	(net 164 "Net-(C1-Pad1)")
	(net 165 "Net-(U19-OSC2)")
	(net 166 "Net-(U19-OSC1)")
	(net 167 "+3.3V")
	(net 168 "/ZeroCrossDetection/OUT")
	(net 169 "/ZeroCrossDetection1/OUT")
	(net 170 "/ZeroCrossDetection2/OUT")
	(net 171 "unconnected-(SW1-Pad4)")
	(net 172 "unconnected-(SW1-Pad6)")
	(net 173 "unconnected-(SW1-Pad3)")
	(net 174 "unconnected-(SW1-Pad5)")
	(net 175 "unconnected-(SW1-Pad2)")
	(net 176 "unconnected-(SW1-Pad1)")
	(net 177 "unconnected-(U1-Vio-Pad5)")
	(net 178 "unconnected-(D1-A-Pad3)")
	(net 179 "Net-(U1-RXD)")
	(net 180 "unconnected-(U1-STBY-Pad8)")
	(net 181 "Net-(U1-CANL)")
	(net 182 "Net-(U1-CANH)")
	(net 183 "unconnected-(D2-A-Pad3)")
	(net 184 "Net-(U1-TXD)")
	(net 185 "unconnected-(U18-PA1-Pad8)")
	(net 186 "unconnected-(U18-PB8-Pad32)")
	(net 187 "unconnected-(U18-PB7-Pad31)")
	(net 188 "unconnected-(U18-PA2-Pad9)")
	(net 189 "unconnected-(U18-PA3-Pad10)")
	(net 190 "unconnected-(U18-PB6-Pad30)")
	(net 191 "unconnected-(U18-PB5-Pad29)")
	(net 192 "unconnected-(U18-PB9-Pad1)")
	(net 193 "NRST")
	(net 194 "unconnected-(U18-PA9{slash}NC-Pad19)")
	(net 195 "unconnected-(U18-PA15-Pad26)")
	(net 196 "unconnected-(U18-PB3-Pad27)")
	(net 197 "SPI1_MISO")
	(net 198 "unconnected-(U18-PA4-Pad11)")
	(net 199 "SPI1_SCK")
	(net 200 "unconnected-(U18-PC6-Pad20)")
	(net 201 "unconnected-(U18-PC14-Pad2)")
	(net 202 "SWDIO")
	(net 203 "unconnected-(U18-PB4-Pad28)")
	(net 204 "unconnected-(U18-PA12{slash}PA10-Pad23)")
	(net 205 "unconnected-(U18-PB0-Pad15)")
	(net 206 "unconnected-(U18-PA10{slash}NC-Pad21)")
	(net 207 "unconnected-(U18-PA0-Pad7)")
	(net 208 "unconnected-(U18-PA8-Pad18)")
	(net 209 "unconnected-(U18-PA11{slash}PA9-Pad22)")
	(net 210 "unconnected-(U18-PB2-Pad17)")
	(net 211 "unconnected-(U18-PC15-Pad3)")
	(net 212 "SPI1_MOSI")
	(net 213 "SWDCLK")
	(net 214 "unconnected-(U18-PB1-Pad16)")
	(net 215 "unconnected-(U19-~{INT}-Pad4)")
	(net 216 "unconnected-(U19-~{INT1}{slash}GPIO1-Pad8)")
	(net 217 "unconnected-(U19-~{INT0}{slash}GPIO0{slash}XSTBY-Pad9)")
	(net 218 "unconnected-(U19-CLKO{slash}SOF-Pad3)")
	(net 219 "SPI1_NSS")
	(net 220 "unconnected-(U20-Pad6)")
	(net 221 "unconnected-(U20-NC-Pad3)")
	(net 222 "unconnected-(U21-NC-Pad3)")
	(net 223 "unconnected-(U21-Pad6)")
	(net 224 "unconnected-(U22-Pad6)")
	(net 225 "unconnected-(U22-NC-Pad3)")
	(net 226 "Net-(J17-Pin_2)")
	(net 227 "Net-(J17-Pin_1)")
	(net 228 "Net-(J18-Pin_1)")
	(net 229 "Net-(J18-Pin_2)")
	(net 230 "Net-(J19-Pin_2)")
	(net 231 "Net-(J19-Pin_1)")
	(net 232 "Net-(R49-Pad2)")
	(net 233 "Net-(R50-Pad2)")
	(net 234 "Net-(R54-Pad2)")
	(net 235 "Net-(R55-Pad2)")
	(net 236 "Net-(R59-Pad2)")
	(net 237 "Net-(R60-Pad2)")
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(uuid "004ddc1b-89bc-4bb9-81f0-fc90a1d5faef")
		(at 32.797858 35.7 -90)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "Q3"
			(at 6.04 -2.445 90)
			(layer "F.SilkS")
			(uuid "fcaa9ef3-85fc-44c3-a42b-bbe5afac6944")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BTA16-600B"
			(at 2.54 2.5 90)
			(layer "F.Fab")
			(uuid "ad93b486-ab42-4bb7-8392-49b7d732a667")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "8d3534fd-ba34-40be-8865-72a0119a7777")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "60413463-58cf-451e-b3a7-2bf4819f4f09")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "79c01e4e-fed5-4b37-8e9d-d207d0523ce5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO?220*")
		(path "/98cc9bb7-a6bb-4cad-bced-cd34a966891d/d1257be0-2394-4f08-8984-f580162b15f9")
		(sheetname "Triac Circuit1")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.58 1.371)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e13942bb-5c1b-411d-b076-2c92e3cae3f5")
		)
		(fp_line
			(start -2.58 -1.76)
			(end 7.66 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9c1fecb3-0f65-4d45-b1f3-694ea3efaf8c")
		)
		(fp_line
			(start -2.58 -3.27)
			(end -2.58 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8e100a4e-5cde-4567-85c5-b8b39a3475a3")
		)
		(fp_line
			(start -2.58 -3.27)
			(end 7.66 -3.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e9301021-cbf6-444b-a336-407c47f4a33e")
		)
		(fp_line
			(start 0.69 -3.27)
			(end 0.69 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ed2d3d05-6626-48bf-b332-a6ccab238a9a")
		)
		(fp_line
			(start 4.391 -3.27)
			(end 4.391 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9bf237e1-c45d-4be0-bf53-55dcb89de974")
		)
		(fp_line
			(start 7.66 -3.27)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8bb6bd03-d196-42f8-a265-8adc95305975")
		)
		(fp_line
			(start -2.71 1.51)
			(end 7.79 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1c143e3a-2fe3-486f-86b4-f0b53b4ee96c")
		)
		(fp_line
			(start 7.79 1.51)
			(end 7.79 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8ec2087d-8835-4d48-aa84-9f6bbd31543d")
		)
		(fp_line
			(start -2.71 -3.4)
			(end -2.71 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a7ff52e8-1b92-4931-9ec6-dbe01eb48bfd")
		)
		(fp_line
			(start 7.79 -3.4)
			(end -2.71 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "aad068cb-e300-4660-933b-9db4e02d06b8")
		)
		(fp_line
			(start -2.46 1.25)
			(end 7.54 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "73b2670b-df8e-4540-af73-d0ebf86b6870")
		)
		(fp_line
			(start 7.54 1.25)
			(end 7.54 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "27138f2e-9933-4cab-9ee3-cb257902ff66")
		)
		(fp_line
			(start -2.46 -1.88)
			(end 7.54 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f57dd093-7eea-4d5d-91d1-7d0b99545e00")
		)
		(fp_line
			(start -2.46 -3.15)
			(end -2.46 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c2bd8393-ce7b-41e7-b88c-4057f248860d")
		)
		(fp_line
			(start 0.69 -3.15)
			(end 0.69 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "74ca8e09-3ef6-4a19-83dc-72d00987546f")
		)
		(fp_line
			(start 4.39 -3.15)
			(end 4.39 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a4a19929-0c91-45a3-8989-740af17a4383")
		)
		(fp_line
			(start 7.54 -3.15)
			(end -2.46 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "95a19413-9316-408a-b3a1-faebc2415cf6")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 -4.27 90)
			(layer "F.Fab")
			(uuid "a2335cd0-2d04-4edd-92dd-7dbe093a09c6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/Triac Circuit1/High_Voltage_L")
			(pinfunction "A1")
			(pintype "passive")
			(uuid "bf58fe51-5775-4fd8-875e-e837b734fd61")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/Triac Circuit1/High_Voltage_Out")
			(pinfunction "A2")
			(pintype "passive")
			(uuid "c045f2cc-6e26-4d1a-9119-f3d13a0c2e78")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(Q3-G)")
			(pinfunction "G")
			(pintype "input")
			(uuid "b80f766d-b3f7-41df-aba9-1ebf0899d035")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-6_W7.62mm"
		(layer "F.Cu")
		(uuid "01b906b9-511a-4125-b6c5-24f8395592da")
		(at 57.142855 41.715)
		(descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U11"
			(at 3.599999 -2.33 180)
			(layer "F.SilkS")
			(uuid "a57cafe8-d4c8-4ee1-a614-a901c3443aae")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MOC3021M"
			(at 3.81 7.409999 180)
			(layer "F.Fab")
			(uuid "3166b403-2628-426c-83e5-6017e497ea82")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c6d5504f-90b5-4197-9688-d1e6ed44f8ff")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3023M-D.PDF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "aa59ee54-385c-4b3b-9613-9b5d65cd8531")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "5570d961-3606-4ddb-941f-fc91012a49f0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*")
		(path "/f251f0b5-0f8b-4418-bbfe-69d55a4bdeb8/0262e914-5435-478f-be04-ece49b8102cf")
		(sheetname "Triac Circuit9")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cdf8c7a5-d5c6-4c58-b54f-696802cc1671")
		)
		(fp_line
			(start 1.16 6.41)
			(end 6.46 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "24cd903c-f907-4b24-9c3f-62543c2c7399")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0539d865-7a62-4297-bb7c-c9ec9480d79c")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6fafa79e-0b0f-46a5-abf0-757a80c6aa88")
		)
		(fp_line
			(start 6.46 6.41)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "24ac497e-77ee-434e-a5e9-d17e91f5e6f1")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dba44113-8cba-475f-947f-f3c4497fac3c")
		)
		(fp_line
			(start -1.1 -1.55)
			(end -1.1 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "222957e3-6cb9-469a-ab67-38c42939107e")
		)
		(fp_line
			(start -1.1 6.6)
			(end 8.7 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "89163bdf-a680-4886-b30a-c792c54fd082")
		)
		(fp_line
			(start 8.7 -1.55)
			(end -1.1 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "932b9d8a-6599-45cd-afda-7ddcfa841430")
		)
		(fp_line
			(start 8.7 6.6)
			(end 8.7 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e5406d36-614c-4e77-8a4f-e46322d5cca7")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3b518d49-bffd-449d-86db-40e46f43b174")
		)
		(fp_line
			(start 0.635 6.35)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fb413c8a-4330-4718-a79b-9fdaaf243f0f")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ea1c5d88-9105-45bf-b815-880eb0ffea21")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7420350b-3a0f-4262-be6f-d4f12663c0f0")
		)
		(fp_line
			(start 6.985 6.35)
			(end 0.635 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1b184caa-94ba-49de-a8ac-edc50a2e5512")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.539999 180)
			(layer "F.Fab")
			(uuid "82fce5e2-ce3f-4485-9c62-9bf957609b0c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 118 "Net-(R29-Pad1)")
			(pintype "passive")
			(uuid "4e0c401c-463b-4961-8df2-58984c33e158")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 141 "Net-(Q20-C)")
			(pintype "passive")
			(uuid "0a381af8-2d68-4a59-a44f-151208174622")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 99 "unconnected-(U11-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "c786531b-48b4-4516-bef1-2d992310bb8d")
		)
		(pad "4" thru_hole oval
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 139 "Net-(Q19-G)")
			(pintype "passive")
			(uuid "8d2b97bd-0606-46aa-b396-aa9383580b30")
		)
		(pad "5" thru_hole oval
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 100 "unconnected-(U11-NC-Pad5)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "682849d1-23e8-4491-a286-ae9a351a5597")
		)
		(pad "6" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "Net-(R28-Pad1)")
			(pintype "passive")
			(uuid "98ead4c2-4772-4f80-bad1-1a9df7f791ac")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-6_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "02a5a956-f42e-40b8-85fe-ef13516583c2")
		(at 45.8 148.8)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R58"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "0bb4f8c0-4f46-4031-8c27-fa67ee06c3e0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1k"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "6ccb4a31-e626-4ca8-9c8a-527b9c19e0cc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "49db39f7-5b8d-4c6f-84ff-0e737c4cccaa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d8a01b0e-77af-485a-abbf-cc8ef262913c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "26210080-e772-4824-b76a-a0c02767c313")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/e9267efd-e7bf-4ed4-9938-23d638b0f804/547580b6-9698-46ab-b758-90ae2111cb33")
		(sheetname "ZeroCrossDetection1")
		(sheetfile "ZeroCrossDetection.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "92c23180-bc5c-4d5d-b9b1-cb16133dfaeb")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1f8b8a85-1165-4e58-a4f1-92579ef867a7")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e089887d-af95-4eb5-941f-c8740ace07f6")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "edad3f99-ffbc-4fab-b3b0-0bc8b176d5b8")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b9291b74-deb1-4025-9fe6-3a49a8ec3395")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a419320e-4943-4509-ba06-ffa75dc33145")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e8615bd9-2669-423b-beb5-2393b995666a")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1da45158-d1a6-4bcb-bb9c-743014778dc8")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6dc19aba-a86a-4c02-b009-738e8b5c64d6")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c05daf2e-1d36-495b-ae89-05ceda3309f0")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "09603359-a8b1-495d-a757-9788def23f7c")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 169 "/ZeroCrossDetection1/OUT")
			(pintype "passive")
			(uuid "578af6e8-5643-481e-8a2d-0590ddfa6c32")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 167 "+3.3V")
			(pintype "passive")
			(uuid "6615afff-36d5-45d4-bfda-fe2a08c34897")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-6_W7.62mm"
		(layer "F.Cu")
		(uuid "02cb891c-5608-4a7f-b3ad-6433fe774e70")
		(at 44.971429 115.765 180)
		(descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U8"
			(at 3.6 -2.33 0)
			(layer "F.SilkS")
			(uuid "71f6fece-8a79-4b5e-99d8-3dd2ae935184")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MOC3021M"
			(at 3.81 7.41 0)
			(layer "F.Fab")
			(uuid "6b5462f2-f451-489d-b5ac-3da31f914d44")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "4e8063a7-2efc-4a1a-bdd2-82d6a39af915")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3023M-D.PDF"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "38747b9d-a5d3-4b55-8282-163f94200d87")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "09f4561b-8549-475c-8c1a-4b45c5bb13d0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*")
		(path "/4a841339-199f-4bc7-a6bd-fe2a9936827c/0262e914-5435-478f-be04-ece49b8102cf")
		(sheetname "Triac Circuit6")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 6.46 6.41)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5210406d-3714-4ec6-93d3-9f6bc89b351a")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1d471fe9-4a65-4a3b-b376-fa691817e25e")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "abc2dd27-1f37-4aa3-99f2-43376961d495")
		)
		(fp_line
			(start 1.16 6.41)
			(end 6.46 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ca2997f4-52d9-4b54-b395-377770b11131")
		)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e9e26bcb-98cc-4126-a911-746c72da91fe")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b9948b7d-93a3-43fd-b3b6-88582938df6d")
		)
		(fp_line
			(start 8.7 6.6)
			(end 8.7 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bde7dbe4-922b-4694-ab9b-a1c79c60b565")
		)
		(fp_line
			(start 8.7 -1.55)
			(end -1.1 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "87ff22d3-3924-4760-bff6-64045757cf46")
		)
		(fp_line
			(start -1.1 6.6)
			(end 8.7 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2f748d91-88a0-41e5-b49e-b0bcadfca9a5")
		)
		(fp_line
			(start -1.1 -1.55)
			(end -1.1 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ada0ef2b-a887-4dfa-a93b-a5d0de599661")
		)
		(fp_line
			(start 6.985 6.35)
			(end 0.635 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "58bb2f54-0629-4a31-9c2b-e11a639c2f98")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "95fb00bb-67c5-42ea-9876-ac4f52e6de9e")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c06d4271-17ec-40ef-9a50-b2681a277f3c")
		)
		(fp_line
			(start 0.635 6.35)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5d30abbf-0e8e-49e5-bf92-fbe4454ce382")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "30c109b7-a15f-43a3-8e71-688c199afa41")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.54 0)
			(layer "F.Fab")
			(uuid "d684bfea-6283-433e-952e-3fe4733e54d0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 115 "Net-(R20-Pad1)")
			(pintype "passive")
			(uuid "8bf7e53a-97a5-4681-ab8c-ae053c098e44")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "Net-(Q14-C)")
			(pintype "passive")
			(uuid "09abc0d5-59f8-40c6-907e-5ec6b825f1d9")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "unconnected-(U8-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "759fa8ff-0ff6-40da-8a9d-fe65cf8bcc21")
		)
		(pad "4" thru_hole oval
			(at 7.62 5.08 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(Q13-G)")
			(pintype "passive")
			(uuid "551ee2f8-e20a-40a6-afb6-eb5f6b4f635d")
		)
		(pad "5" thru_hole oval
			(at 7.62 2.54 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 95 "unconnected-(U8-NC-Pad5)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "8833f29d-ad75-4dde-972d-deb3a78e6231")
		)
		(pad "6" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "Net-(R19-Pad1)")
			(pintype "passive")
			(uuid "44160577-2cfb-4e15-8e9b-ace55a8b9c50")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-6_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "06b3ddc6-f223-4c67-be11-cd55ca91c6ca")
		(at 53.542855 58.88 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R33"
			(at 0 -1.82 180)
			(layer "F.SilkS")
			(uuid "1555c017-8be0-443b-9ac1-6a964789a0cf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at -3.64 0 180)
			(layer "F.Fab")
			(uuid "737724c0-2c60-4036-86dd-d53fbfe67f53")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "6cb8f912-4e69-4336-bd46-459e65c8389c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "a973222f-61f0-4b1a-afc9-ca054bb066c7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "195dbb07-c7da-48cc-a9a2-fb50e83243bf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/d20c900a-3d9a-4460-9d5d-3ed4d11c2b93/ca31a324-056f-45d6-b948-82e97db62734")
		(sheetname "Triac Circuit10")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4924a752-cd9f-47c4-9844-b55324c55159")
		)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "37ba5092-40c8-4846-9918-61689070af38")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f39cbdaa-7526-4d9a-801e-c86dc235a475")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1c2060be-3fa9-499b-b71b-36291f0bcaa4")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8b11bd4c-2f2d-49bf-80dd-eebab4f3d582")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5c0dc6f1-5f68-4cef-b58d-9e7c22be5cc8")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "735dfbd3-0248-4520-b5fe-a7484b708750")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0b49d50f-e4d5-4b54-8303-c1d4daeee6d3")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "057d85bf-9520-4a74-9705-8cf6b08be000")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "46bd029c-54ef-473a-8005-e65fc0b43d3d")
		)
		(fp_text user "${REFERENCE}"
			(at 3.04 0.01 180)
			(layer "F.Fab")
			(uuid "c3a56073-2271-41b3-979b-770739878d07")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 143 "Net-(Q22-B)")
			(pintype "passive")
			(uuid "504320bd-cfa7-4952-b386-fafd8ac8a19a")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 133 "/Triac Circuit10/Enable")
			(pintype "passive")
			(uuid "f488e431-44e6-4c3b-b784-b22fbf6c9f9e")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(uuid "07eb7760-4e2b-422c-a547-d89df1f9385b")
		(at 69.287855 60.82 90)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "Q21"
			(at 6.04 -2.444999 -90)
			(layer "F.SilkS")
			(uuid "2917c3be-0524-4f4a-b05f-d35e7ac973ac")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BTA16-600B"
			(at 2.539999 2.5 -90)
			(layer "F.Fab")
			(uuid "8675526c-40e1-4bff-a0de-b09972e7c314")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "32096bd5-6f1c-401d-8c8e-7655192ca153")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "f4844bef-994f-4474-9e65-070a43e3d084")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "5f4c3d30-ec71-4663-9d16-7cd125a50eba")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO?220*")
		(path "/d20c900a-3d9a-4460-9d5d-3ed4d11c2b93/d1257be0-2394-4f08-8984-f580162b15f9")
		(sheetname "Triac Circuit10")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 7.66 -3.27)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "db1af375-2bd0-47d2-bd66-438c68f46d86")
		)
		(fp_line
			(start 4.391 -3.27)
			(end 4.391 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0a4ef12a-7386-4ff6-98db-b2002e034176")
		)
		(fp_line
			(start 0.69 -3.27)
			(end 0.69 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "19a5ff19-4ac8-421c-86dc-38f198f51bb2")
		)
		(fp_line
			(start -2.58 -3.27)
			(end 7.66 -3.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7d9a8487-c5c4-4879-bb5c-0aad59dad4a3")
		)
		(fp_line
			(start -2.58 -3.27)
			(end -2.58 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "829f0269-f04c-4113-ba18-7e912390ad9e")
		)
		(fp_line
			(start -2.58 -1.76)
			(end 7.66 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e6962f97-7f3c-4864-831c-d7338979e979")
		)
		(fp_line
			(start -2.58 1.371)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "127fd313-6d22-438f-8b94-8ebac76f34f7")
		)
		(fp_line
			(start 7.79 -3.4)
			(end -2.71 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c3bc34ec-1b6b-44de-a175-162955d1b070")
		)
		(fp_line
			(start -2.71 -3.4)
			(end -2.71 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cc96b1bb-8156-45a5-95a1-1ddfdb1924ee")
		)
		(fp_line
			(start 7.79 1.51)
			(end 7.79 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "73dd3e97-ed2a-4984-b31b-287ef5f09a55")
		)
		(fp_line
			(start -2.71 1.51)
			(end 7.79 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c6587d5b-a5f1-4c31-a788-eba96c90c7ef")
		)
		(fp_line
			(start 7.54 -3.15)
			(end -2.46 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8cfb3d2b-0037-48ff-8bc4-f3bc59991d34")
		)
		(fp_line
			(start 4.39 -3.15)
			(end 4.39 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "94c49bb9-b1cf-4303-b6b0-16af1017b322")
		)
		(fp_line
			(start 0.69 -3.15)
			(end 0.69 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e8a9e466-b944-434a-be88-ebaf9a778ad4")
		)
		(fp_line
			(start -2.46 -3.15)
			(end -2.46 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9c84c225-3973-41b0-bee7-30f913924701")
		)
		(fp_line
			(start -2.46 -1.88)
			(end 7.54 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c7a178dc-16e2-45a3-8a99-c33b7ebe0340")
		)
		(fp_line
			(start 7.54 1.25)
			(end 7.54 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "953615cb-2150-45dc-944b-2fb2eae824cc")
		)
		(fp_line
			(start -2.46 1.25)
			(end 7.54 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e79ff8e5-4571-4132-810b-5ec392cde10e")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 -4.27 -90)
			(layer "F.Fab")
			(uuid "ee15bac6-08a5-46ee-b688-0b9a66da6bb3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "/Triac Circuit10/High_Voltage_L")
			(pinfunction "A1")
			(pintype "passive")
			(uuid "7dfda45b-f918-4afd-adaa-0d304a9f80c8")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/Triac Circuit10/High_Voltage_Out")
			(pinfunction "A2")
			(pintype "passive")
			(uuid "d296fda7-ab7c-404a-92b1-c6878e11b066")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 142 "Net-(Q21-G)")
			(pinfunction "G")
			(pintype "input")
			(uuid "ce460fb1-8b0a-47b0-a23e-c1f563fff33f")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(uuid "0e9a8c95-7c8f-44e6-be82-e8dd1a225550")
		(at 35.171429 116.78 90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R19"
			(at 3.81 -1.92 90)
			(layer "F.SilkS")
			(uuid "9daf5289-4d32-430f-88dc-967cc815a2bf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "180"
			(at 3.81 1.92 90)
			(layer "F.Fab")
			(uuid "209abe36-b497-45f7-9349-83dbe6d8c748")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8d04978b-b36b-44f0-95f7-b78daa89580e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "05c17192-1491-4344-a8b3-f3f0ca6cfe9f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c62798af-84de-42bb-951c-4b91f17f62b0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/4a841339-199f-4bc7-a6bd-fe2a9936827c/4ab64e29-964f-40b2-bf58-c546b31cd3eb")
		(sheetname "Triac Circuit6")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 5.73 -0.92)
			(end 1.89 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "420845a7-7b06-49c3-a357-1fd40c3fe75f")
		)
		(fp_line
			(start 1.89 -0.92)
			(end 1.89 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cd445cda-ac49-436f-87be-c99fe02e0cb6")
		)
		(fp_line
			(start 6.68 0)
			(end 5.73 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f4d9d5b4-3754-4255-aa14-f30519ed1a6b")
		)
		(fp_line
			(start 0.94 0)
			(end 1.89 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1241c3d7-9866-492f-a0bc-046677c7bd14")
		)
		(fp_line
			(start 5.73 0.92)
			(end 5.73 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "29717bd0-d850-4ffe-a3e9-4c5068b2661b")
		)
		(fp_line
			(start 1.89 0.92)
			(end 5.73 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0a4e1827-6d5a-475e-a826-3653a5d78b8c")
		)
		(fp_line
			(start 8.57 -1.05)
			(end -0.95 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e9be9d16-f61b-4c44-abc4-c438091217fe")
		)
		(fp_line
			(start -0.95 -1.05)
			(end -0.95 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "abbc8b44-849b-4389-baa4-af4b09963dcb")
		)
		(fp_line
			(start 8.57 1.05)
			(end 8.57 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "13dfe6ff-f38e-4872-a527-10c4b73e82f5")
		)
		(fp_line
			(start -0.95 1.05)
			(end 8.57 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "43ea0087-0872-42e9-b303-2f2de51cc557")
		)
		(fp_line
			(start 5.61 -0.8)
			(end 2.01 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1aaa32f9-737e-4928-8344-59eb61b936f5")
		)
		(fp_line
			(start 2.01 -0.8)
			(end 2.01 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "abeeffee-04c2-4d74-8cd2-d2248f8fd445")
		)
		(fp_line
			(start 7.62 0)
			(end 5.61 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "69c8de04-9919-452c-a5d5-a6b065b7ce7b")
		)
		(fp_line
			(start 0 0)
			(end 2.01 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bc5c22af-0161-45ca-a5a4-a6d0da829514")
		)
		(fp_line
			(start 5.61 0.8)
			(end 5.61 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "90a13e26-46b8-4035-87d3-c4d88f16b6f1")
		)
		(fp_line
			(start 2.01 0.8)
			(end 5.61 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f4239534-9a56-4bc9-824d-7dc9c7b6209f")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
			(uuid "cee07009-3ff3-4721-915a-96764900c0bb")
			(effects
				(font
					(size 0.72 0.72)
					(thickness 0.108)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "Net-(R19-Pad1)")
			(pintype "passive")
			(uuid "0027c69a-a50b-4481-bd4a-f774d589e3db")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "/Triac Circuit6/High_Voltage_L")
			(pintype "passive")
			(uuid "092f6961-b09a-4613-8b91-a19080c2cc2d")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(uuid "0f309ea5-93f3-4fc5-85b5-7fea54989f82")
		(at 33.4 179.12 90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R50"
			(at 2.54 -1.92 90)
			(layer "F.SilkS")
			(uuid "e6f98da1-867c-4782-9320-09cbc6b5f5b5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "220k"
			(at 2.54 1.92 90)
			(layer "F.Fab")
			(uuid "a09d08c8-f795-4594-82f5-503b5e49482a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "321d3733-fc66-4ddd-8681-50e8c0b476c8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "84dd78a8-682b-4f97-8ec2-a15692f39edb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0d679bc5-71e3-4754-a73b-364f43c70bc7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/eb409310-6102-43e5-b48c-2438ac1942c0/a8ed06bc-ef8c-4560-b835-f2ef8ce81949")
		(sheetname "ZeroCrossDetection")
		(sheetfile "ZeroCrossDetection.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 0.62 -0.92)
			(end 4.46 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "73637dac-b168-47d4-a55b-a7a77e3e0130")
		)
		(fp_line
			(start 0.62 0.92)
			(end 4.46 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a03f4c79-bd21-4867-b51d-c4618e804385")
		)
		(fp_line
			(start 6.03 -1.05)
			(end -0.95 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6b2b3d32-de0a-487b-ad06-e3767d610a36")
		)
		(fp_line
			(start -0.95 -1.05)
			(end -0.95 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6b85be9c-c782-4a12-969d-82e88c1587ce")
		)
		(fp_line
			(start 6.03 1.05)
			(end 6.03 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "595d1d5d-ef95-4ede-8d5f-ccc00a8ce1b6")
		)
		(fp_line
			(start -0.95 1.05)
			(end 6.03 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c76537ad-6f3c-4fca-9ea0-489abf53f9d8")
		)
		(fp_line
			(start 4.34 -0.8)
			(end 0.74 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "12fbda3d-dabf-4c4f-acc7-40071c543831")
		)
		(fp_line
			(start 0.74 -0.8)
			(end 0.74 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0b98f292-eeab-4590-9ce4-59b1dda14ebf")
		)
		(fp_line
			(start 5.08 0)
			(end 4.34 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3509d012-a8b5-44c3-933b-6f1123d45254")
		)
		(fp_line
			(start 0 0)
			(end 0.74 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "856157dd-b2bd-4a84-af12-a9eb0be06c18")
		)
		(fp_line
			(start 4.34 0.8)
			(end 4.34 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "77a7cb92-bc59-4712-9d88-b19fa314d41d")
		)
		(fp_line
			(start 0.74 0.8)
			(end 4.34 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d5976db4-9b0a-48eb-83d9-490ae9574662")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 90)
			(layer "F.Fab")
			(uuid "473928a1-c1ff-4a72-af07-05e271f6e0b9")
			(effects
				(font
					(size 0.72 0.72)
					(thickness 0.108)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 226 "Net-(J17-Pin_2)")
			(pintype "passive")
			(uuid "53a394cf-e003-4686-982f-9cc3512b9ba3")
		)
		(pad "2" thru_hole oval
			(at 5.08 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 233 "Net-(R50-Pad2)")
			(pintype "passive")
			(uuid "5cf9718f-3f5e-4878-8ca1-e67b7a3c3e80")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
		(layer "F.Cu")
		(uuid "0f3eadea-c838-4298-a441-1b94a5768093")
		(at 77 91.36 90)
		(descr "Terminal Block Phoenix MKDS-3-2-5.08, 2 pins, pitch 5.08mm, size 10.2x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-3-2-5.08 pitch 5.08mm size 10.2x11.2mm^2 drill 1.3mm pad 2.6mm")
		(property "Reference" "J13"
			(at 3.1 -2.999999 -90)
			(layer "F.SilkS")
			(uuid "972d3694-737b-44ce-a9f3-15814ef4579e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 2.539999 6.36 90)
			(layer "F.Fab")
			(uuid "f96191e7-7c27-4438-8b85-30a5f48edd9b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "e58393fd-351b-4157-bcc4-4045bc441276")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "0034e671-e7fe-429e-a256-b2e0298395e7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "6f966f43-d58c-437e-8e09-eabce43f971f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/fb144577-8e6f-488b-ba1b-870763a27401/60e4d8a3-c16e-48cd-a1fd-61f2968ecc7b")
		(sheetname "Triac Circuit12")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 7.68 -5.96)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4076b7c6-0aeb-49fa-b05f-f11ea8153c14")
		)
		(fp_line
			(start -2.6 -5.96)
			(end 7.68 -5.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2a89436f-ae67-4592-9791-dfd58ccbe020")
		)
		(fp_line
			(start -2.6 -5.96)
			(end -2.6 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2e4cc866-62fd-49ee-a25a-16acd40bc310")
		)
		(fp_line
			(start -2.6 -3.9)
			(end 7.68 -3.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "97e703df-8785-4a23-ac8b-0be084718652")
		)
		(fp_line
			(start 6.468 -1.654)
			(end 6.088 -1.274)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a1dd66cb-1134-42b0-a602-dab6144d5e26")
		)
		(fp_line
			(start 1.388 -1.654)
			(end 1.281 -1.547)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f76a1a81-8688-42f2-881c-3fab23e660a6")
		)
		(fp_line
			(start 6.734 -1.388)
			(end 6.339 -0.992)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "55606d93-78fd-4e12-946c-4fff2283e9fc")
		)
		(fp_line
			(start 1.654 -1.388)
			(end 1.547 -1.281)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1b62e3cc-99f6-4c7f-80ec-3060bb72a178")
		)
		(fp_line
			(start 3.822 0.992)
			(end 3.427 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dbbf87d3-f211-4afd-b334-cddb987214ec")
		)
		(fp_line
			(start 4.073 1.274)
			(end 3.693 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "98e7b495-c106-462f-8d15-a917d2407bbe")
		)
		(fp_line
			(start -1.548 1.281)
			(end -1.654 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1ee0aaba-273b-4de4-938b-e040febeedd0")
		)
		(fp_line
			(start -1.282 1.547)
			(end -1.388 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "994fa917-dd48-4c87-b0dc-1345613a11ca")
		)
		(fp_line
			(start -2.6 2.3)
			(end 7.68 2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a04b7c91-ab9a-433f-ae0c-6a99ef502c9b")
		)
		(fp_line
			(start -2.6 4.8)
			(end 7.68 4.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f5d536a7-3067-4b4a-926b-5497acdd7634")
		)
		(fp_line
			(start -2.84 4.86)
			(end -2.84 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6fdd0ff6-a220-4b98-b409-d5812360e0c2")
		)
		(fp_line
			(start -2.6 5.36)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cc2a3e46-379d-45b2-8458-03687e0d167c")
		)
		(fp_line
			(start -2.84 5.6)
			(end -2.34 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4bc2525d-2fdc-4ee9-959f-f32b5a8b32f1")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.26 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "391120ad-7677-42f7-8dc9-b8205e5b4430")
		)
		(fp_circle
			(center 0 0)
			(end 2.18 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "c97c36b7-9bad-42f0-98b9-81911cf4a450")
		)
		(fp_line
			(start 8.13 -6.4)
			(end -3.04 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cc9b906b-c03f-489a-96a0-e3e1606313f3")
		)
		(fp_line
			(start -3.04 -6.4)
			(end -3.04 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a182e442-be4f-4b46-b964-4d80b4517726")
		)
		(fp_line
			(start 8.13 5.8)
			(end 8.13 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6f95a0fe-0269-4cdd-a6e8-7c7ba809d14b")
		)
		(fp_line
			(start -3.04 5.8)
			(end 8.13 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7e17e58a-a8af-452d-b6f8-2109d88c9c08")
		)
		(fp_line
			(start 7.62 -5.9)
			(end 7.62 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0bacb385-f119-4bad-942b-f9064a15adce")
		)
		(fp_line
			(start -2.54 -5.9)
			(end 7.62 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fd08ba79-c215-4360-af6b-120c9ee670de")
		)
		(fp_line
			(start -2.54 -3.9)
			(end 7.62 -3.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cca76bb3-0459-49ba-b6ae-7aeee2b60216")
		)
		(fp_line
			(start 6.353 -1.517)
			(end 3.564 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8d928786-f085-401d-8851-bdb4355cc334")
		)
		(fp_line
			(start 1.273 -1.517)
			(end -1.517 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b3e51edf-c20c-4f51-8000-b86a6b366968")
		)
		(fp_line
			(start 6.597 -1.273)
			(end 3.808 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "346e9d1e-2e0b-44f2-adab-f555bf15770d")
		)
		(fp_line
			(start 1.517 -1.273)
			(end -1.273 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9d1a5e4b-1e3e-4139-a9ac-e113f668c6fa")
		)
		(fp_line
			(start -2.54 2.3)
			(end 7.62 2.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "57730f4c-e582-4039-8b81-356df59cb9f7")
		)
		(fp_line
			(start -2.54 4.8)
			(end -2.54 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cf62cc38-2f5d-4f73-9696-d5f75a6771d4")
		)
		(fp_line
			(start -2.54 4.8)
			(end 7.62 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6ed4bef0-9934-4be9-b297-51ffad5900ef")
		)
		(fp_line
			(start 7.62 5.3)
			(end -2.04 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "346845a2-ce94-4b7c-aa6d-0e8a52cd17ae")
		)
		(fp_line
			(start -2.04 5.3)
			(end -2.54 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "09f4ab6d-090a-4f11-afad-b94c0157185a")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.08 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "bf4b5ff5-4283-4f68-9d16-bbd05ebadbc7")
		)
		(fp_circle
			(center 0 0)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "637fd0b2-1eae-4600-b0b6-936ddd54791a")
		)
		(fp_text user "${REFERENCE}"
			(at 2.539999 3.1 90)
			(layer "F.Fab")
			(uuid "dbce4d30-5a3a-411c-bb3c-c6f55213ae7a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 84 "/Triac Circuit12/High_Voltage_L")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "aaffa9f0-bbf9-4d51-a2ef-43957d2933cb")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/Triac Circuit12/High_Voltage_Out")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "4aa5c69b-56a5-4586-80f6-50ccc0167707")
		)
		(model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
		(layer "F.Cu")
		(uuid "138f1880-267a-4cf0-89d9-93f27ab943b1")
		(at 25.028571 66.12 -90)
		(descr "Terminal Block Phoenix MKDS-3-2-5.08, 2 pins, pitch 5.08mm, size 10.2x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-3-2-5.08 pitch 5.08mm size 10.2x11.2mm^2 drill 1.3mm pad 2.6mm")
		(property "Reference" "J4"
			(at 3.1 -3 90)
			(layer "F.SilkS")
			(uuid "2149e187-88fa-4124-a98e-3ee02f4ded2e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 2.54 6.36 -90)
			(layer "F.Fab")
			(uuid "f7aa17c2-b41e-496c-ad79-8906e5d725ca")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "2dd9887a-016f-4e7f-b862-71839f5a312a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "f3d52e53-fa07-428b-bd86-5bb78523f50f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "16905085-ec0f-4ffc-bc22-f193e171fa33")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/1abc9394-30bb-4ef5-a1be-aa230dbd1566/60e4d8a3-c16e-48cd-a1fd-61f2968ecc7b")
		(sheetname "Triac Circuit3")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.84 5.6)
			(end -2.34 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6bbd6733-74d8-45a3-bade-d011784f8871")
		)
		(fp_line
			(start -2.6 5.36)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "32bb4a52-7150-43e3-b629-835d21f61bdf")
		)
		(fp_line
			(start -2.84 4.86)
			(end -2.84 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d5902b70-5af0-4a1a-9eeb-846de7e99d4a")
		)
		(fp_line
			(start -2.6 4.8)
			(end 7.68 4.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7d134439-34dd-4b58-84fd-064cd0a2c84e")
		)
		(fp_line
			(start -2.6 2.3)
			(end 7.68 2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "be9341db-0b0b-4d1d-a8a3-76852ecefc75")
		)
		(fp_line
			(start -1.282 1.547)
			(end -1.388 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7f646817-38e6-4fed-8917-06004add263d")
		)
		(fp_line
			(start -1.548 1.281)
			(end -1.654 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f7411e80-8395-4b2a-bb0d-984022002ac1")
		)
		(fp_line
			(start 4.073 1.274)
			(end 3.693 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fc0c2786-df8b-4f31-a9eb-3b194c990c5f")
		)
		(fp_line
			(start 3.822 0.992)
			(end 3.427 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "97d4182d-c7ba-4db0-a1c5-95c3299739c5")
		)
		(fp_line
			(start 1.654 -1.388)
			(end 1.547 -1.281)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4cf76b0d-e012-4081-9bf6-c106267bc987")
		)
		(fp_line
			(start 6.734 -1.388)
			(end 6.339 -0.992)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d305fa08-c07c-428c-a951-11629a9ea58b")
		)
		(fp_line
			(start 1.388 -1.654)
			(end 1.281 -1.547)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e22d60eb-607d-4161-8499-a16037335d4b")
		)
		(fp_line
			(start 6.468 -1.654)
			(end 6.088 -1.274)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3342a330-1cd1-4e40-bb06-861627f7a610")
		)
		(fp_line
			(start -2.6 -3.9)
			(end 7.68 -3.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "411b8908-7759-4a53-8b32-51d66eeeda62")
		)
		(fp_line
			(start -2.6 -5.96)
			(end -2.6 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2c214101-1095-4e74-8168-61605c77e9e4")
		)
		(fp_line
			(start -2.6 -5.96)
			(end 7.68 -5.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d0a86de3-f9be-4554-8cbf-a50b1f0f1ab7")
		)
		(fp_line
			(start 7.68 -5.96)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4aabb1d1-5995-4d4a-a018-02130fda1e20")
		)
		(fp_circle
			(center 0 0)
			(end 2.18 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "1e6571c7-c87b-4057-bb41-e1868f51068d")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.26 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "eba9e3c7-527b-4332-b018-271e6737e93c")
		)
		(fp_line
			(start -3.04 5.8)
			(end 8.13 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "58c5906e-a586-4117-92e4-d96ee2fbdbfd")
		)
		(fp_line
			(start 8.13 5.8)
			(end 8.13 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "800a3692-c5ec-4bac-972d-a71d44ec7cf0")
		)
		(fp_line
			(start -3.04 -6.4)
			(end -3.04 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cd4b5ea4-ac08-41f4-abb6-aaf0dbdb09f9")
		)
		(fp_line
			(start 8.13 -6.4)
			(end -3.04 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ca324766-b39f-4906-b719-77e31ca1d083")
		)
		(fp_line
			(start -2.04 5.3)
			(end -2.54 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ae8ac788-b677-47b8-a7e4-a1bab475892c")
		)
		(fp_line
			(start 7.62 5.3)
			(end -2.04 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4d40cdb5-405e-4276-a6c1-e8b866730956")
		)
		(fp_line
			(start -2.54 4.8)
			(end 7.62 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "98676f92-dbc2-4df1-9f52-c4041afec961")
		)
		(fp_line
			(start -2.54 4.8)
			(end -2.54 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d11b50ac-1e2c-43d9-abc9-e1b7b4677379")
		)
		(fp_line
			(start -2.54 2.3)
			(end 7.62 2.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "16060895-d5b4-4b60-8f33-ea41349a87e6")
		)
		(fp_line
			(start 1.517 -1.273)
			(end -1.273 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "acebc254-33b8-48ab-a397-4c40d15391e7")
		)
		(fp_line
			(start 6.597 -1.273)
			(end 3.808 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b4a55ae6-779e-4422-959e-9561c585f5a4")
		)
		(fp_line
			(start 1.273 -1.517)
			(end -1.517 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "89e31a14-56d5-4a35-9362-f039eefbb97b")
		)
		(fp_line
			(start 6.353 -1.517)
			(end 3.564 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "46c99218-e100-4b03-8e45-e5516aa258bf")
		)
		(fp_line
			(start -2.54 -3.9)
			(end 7.62 -3.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8fee8af0-eaed-400a-b471-0d84196a5dfa")
		)
		(fp_line
			(start -2.54 -5.9)
			(end 7.62 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "380aef87-695e-45d8-9a8a-184adc6366b6")
		)
		(fp_line
			(start 7.62 -5.9)
			(end 7.62 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "575b1c46-8e43-4164-af12-7aee80680995")
		)
		(fp_circle
			(center 0 0)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "ca19b33b-ea01-405b-aeec-4286cc35c0ac")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.08 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "6fb8cd97-bfab-41ec-b4ef-657acb0700cb")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 3.1 -90)
			(layer "F.Fab")
			(uuid "7b45505b-49bc-4cc8-a5e6-88b7a92b2708")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/Triac Circuit3/High_Voltage_L")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "aaff2720-c41f-4aea-beec-d3bd0ae96372")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/Triac Circuit3/High_Voltage_Out")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "2c0b8a55-1569-4fa5-9b1c-e91d6aa39487")
		)
		(model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(uuid "1473479f-ebcd-4a3f-b8b2-30b4a326738c")
		(at 69.287855 106.54 90)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "Q27"
			(at 6.04 -2.444999 -90)
			(layer "F.SilkS")
			(uuid "e22e04ed-af70-4afc-a043-0769680240ac")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BTA16-600B"
			(at 2.539999 2.5 -90)
			(layer "F.Fab")
			(uuid "39feaa83-a623-42bb-a148-46bdd7959403")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "4f82e616-0d45-4f3e-bafa-bd1a3d67bbe7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "8f0cadbb-d454-4794-b6e8-c7b3446602ab")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "7d315abe-6b96-40ce-ae48-7aaac3c0508d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO?220*")
		(path "/4a948621-4b4c-41c9-b07f-b928eecc9e1e/d1257be0-2394-4f08-8984-f580162b15f9")
		(sheetname "Triac Circuit13")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 7.66 -3.27)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "14e6b3e0-c581-4dab-b28c-66ff42f607bc")
		)
		(fp_line
			(start 4.391 -3.27)
			(end 4.391 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "95f5a953-79e1-4657-b8a4-bfdca8f20058")
		)
		(fp_line
			(start 0.69 -3.27)
			(end 0.69 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "19ee6ef7-7456-4ac8-aad5-7967e640f601")
		)
		(fp_line
			(start -2.58 -3.27)
			(end 7.66 -3.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "69364b74-6474-4988-90ab-0a4940cff3f8")
		)
		(fp_line
			(start -2.58 -3.27)
			(end -2.58 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3ddb1c3d-0f0c-43bb-af95-b29fbfee528c")
		)
		(fp_line
			(start -2.58 -1.76)
			(end 7.66 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8cfd86a1-c9ca-41b1-8ad3-584dbcfafec3")
		)
		(fp_line
			(start -2.58 1.371)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dc481078-7a00-49eb-8924-c81fb470e32d")
		)
		(fp_line
			(start 7.79 -3.4)
			(end -2.71 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e6fc0f48-c803-4d29-a221-3e338e28857a")
		)
		(fp_line
			(start -2.71 -3.4)
			(end -2.71 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "271eb62b-858f-46dd-9897-5f92b0a1bcb7")
		)
		(fp_line
			(start 7.79 1.51)
			(end 7.79 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b9c693ac-a53a-4116-a436-2add5a7ac7f7")
		)
		(fp_line
			(start -2.71 1.51)
			(end 7.79 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "316e9786-4f8d-46b4-83a3-2f9d2157a395")
		)
		(fp_line
			(start 7.54 -3.15)
			(end -2.46 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ce9b936c-9e7c-47a8-8f74-e4794ec5539b")
		)
		(fp_line
			(start 4.39 -3.15)
			(end 4.39 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "392a0ed2-67c6-4ab1-a1f4-99298d77a9ca")
		)
		(fp_line
			(start 0.69 -3.15)
			(end 0.69 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ba825cbf-30a1-419d-bf37-1f3e67af3e20")
		)
		(fp_line
			(start -2.46 -3.15)
			(end -2.46 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "446a1347-4930-4472-8a2b-4f38c648f71a")
		)
		(fp_line
			(start -2.46 -1.88)
			(end 7.54 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a039f7b3-04e0-4a70-adc2-cbb88b34a052")
		)
		(fp_line
			(start 7.54 1.25)
			(end 7.54 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6c59932c-8385-4416-a19b-377f1a5ecaf1")
		)
		(fp_line
			(start -2.46 1.25)
			(end 7.54 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c717f140-9638-4bd0-9d6c-d06de7fa3e01")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 -4.27 -90)
			(layer "F.Fab")
			(uuid "2b2bde46-9437-4e91-aa11-64f297589f50")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 85 "/Triac Circuit13/High_Voltage_L")
			(pinfunction "A1")
			(pintype "passive")
			(uuid "b13b932e-1625-48ca-8b48-f819f5f8e45f")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/Triac Circuit13/High_Voltage_Out")
			(pinfunction "A2")
			(pintype "passive")
			(uuid "96c8bff4-23c1-451e-b8bb-0d9d634d6d72")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 151 "Net-(Q27-G)")
			(pinfunction "G")
			(pintype "input")
			(uuid "0badaeff-d278-4938-8391-8ebbaa26b6d2")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "165ad4ba-e93b-492d-a147-f73735b92329")
		(at 53.605355 117.64 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R44"
			(at 0 -1.82 180)
			(layer "F.SilkS")
			(uuid "fef5a284-ae9c-4a07-b9ea-54534703cd90")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at 0 1.82 180)
			(layer "F.Fab")
			(uuid "f5a95f7c-6c80-45c7-96da-1345cd696ae3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "8b1fd281-a504-4dd1-8e26-f70914eb42c2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "0d3b2658-e739-4c3d-9fc7-23ba7469ac17")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "cd1b4809-d436-4d28-87f4-cad54f854d97")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/683a6cfc-1cb6-4c63-ae1f-c9d1fdc220d0/de24ad75-a874-4d54-a682-b1d6f2079d30")
		(sheetname "Triac Circuit14")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "15170b49-ae5e-4ba0-ae29-2fc15eb9758e")
		)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2f3dff95-8799-4df1-a86f-794c7a032612")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "98fbcc71-a251-49b6-9c71-67552f954b3c")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a3f210c4-f74f-407a-8ec8-0c7e7f424c65")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d64fb211-7005-494c-a6fd-4d65e5d763d3")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "96d5dc6b-b9ee-4495-a4b7-49cb555a621b")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d5b8c1b7-6978-479b-819e-6e808e3d8498")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1f9ea1b0-bbac-455d-a419-4ae482e4ea5d")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ae0641df-b7af-4708-9975-512825c5d600")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d26b3aa5-9205-4f9d-88b1-3873455446a4")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
			(uuid "edf76a78-14a4-470c-930b-f86041fac0cc")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 125 "Net-(R44-Pad1)")
			(pintype "passive")
			(uuid "d1d320c9-d442-44a5-89b9-039acabf719f")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 37 "+3V3")
			(pintype "passive")
			(uuid "412af308-1f05-44dd-93a4-099105a0f1d3")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(uuid "1a705261-5a9b-4a60-868b-7868d7faeaea")
		(at 35.8 149.46 -90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R54"
			(at 2.54 -1.92 90)
			(layer "F.SilkS")
			(uuid "5bae2df9-06d9-4daa-80d2-b4fa35134516")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "220k"
			(at 2.54 1.92 90)
			(layer "F.Fab")
			(uuid "00fd13fd-6f51-4149-9ff1-4c8b6ad39c18")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "020e6a70-7953-40ca-8a6e-1e1583a9c647")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "79c7bfd4-ffc8-4254-8452-e489a4e493f2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c5f285b0-850b-4310-a568-a6ca6bb5a192")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/e9267efd-e7bf-4ed4-9938-23d638b0f804/651d23d0-fccd-4821-a525-06dced80ce07")
		(sheetname "ZeroCrossDetection1")
		(sheetfile "ZeroCrossDetection.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 0.62 0.92)
			(end 4.46 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b97f5eea-1745-48b0-a37b-03403f2959da")
		)
		(fp_line
			(start 0.62 -0.92)
			(end 4.46 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "89ca28c1-6593-48a0-a19d-bff35d5c86fe")
		)
		(fp_line
			(start -0.95 1.05)
			(end 6.03 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e54fd120-d6e7-4c00-8fcf-caa80415707a")
		)
		(fp_line
			(start 6.03 1.05)
			(end 6.03 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "19c7d363-b0ca-44cf-b2c2-87440e43c7c5")
		)
		(fp_line
			(start -0.95 -1.05)
			(end -0.95 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f90d9791-654a-4f5f-ac5e-43ae6b609998")
		)
		(fp_line
			(start 6.03 -1.05)
			(end -0.95 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4392b1e7-4484-46cf-a678-234d8ed7d742")
		)
		(fp_line
			(start 0.74 0.8)
			(end 4.34 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7746ef30-436f-4d2d-b0d8-ae8c8ea15e18")
		)
		(fp_line
			(start 4.34 0.8)
			(end 4.34 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5181df0d-aa8c-494c-951e-525d5477954e")
		)
		(fp_line
			(start 0 0)
			(end 0.74 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c974f065-e7f6-4556-84af-7550981ae873")
		)
		(fp_line
			(start 5.08 0)
			(end 4.34 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "47d55f70-74da-45f4-a794-250c78815eec")
		)
		(fp_line
			(start 0.74 -0.8)
			(end 0.74 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "39b554c8-ddae-45e9-903c-3d974559f0b0")
		)
		(fp_line
			(start 4.34 -0.8)
			(end 0.74 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "77b2b409-68c5-4673-b08c-4c7ab8023612")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 90)
			(layer "F.Fab")
			(uuid "eae51bed-9b59-43e1-ba3d-df55bbe7e39d")
			(effects
				(font
					(size 0.72 0.72)
					(thickness 0.108)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 228 "Net-(J18-Pin_1)")
			(pintype "passive")
			(uuid "3224fa82-c46c-4f67-bd9a-1d3ba1f574d5")
		)
		(pad "2" thru_hole oval
			(at 5.08 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 234 "Net-(R54-Pad2)")
			(pintype "passive")
			(uuid "376d43de-5263-443b-a789-cfc94a2a76ce")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(uuid "1b2c368c-d161-41ec-b3b7-794f72204174")
		(at 35.228571 86.3 90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R13"
			(at 3.81 -1.92 90)
			(layer "F.SilkS")
			(uuid "a744dd74-a72b-43d3-ae92-90ddb1af1feb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "180"
			(at 3.81 1.92 90)
			(layer "F.Fab")
			(uuid "b0f8f5c8-818d-4ace-b013-6de96fa46201")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a484db20-e826-4df8-981c-e1b6e3b181a0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d68bc639-7269-4f70-bb29-8b329742cf37")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "af0ef7f9-c3cf-4b73-b6b0-e638d30d2bc8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/e56f6699-6dcd-4f6f-a67f-2156f450d5f1/4ab64e29-964f-40b2-bf58-c546b31cd3eb")
		(sheetname "Triac Circuit4")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 5.73 -0.92)
			(end 1.89 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "af592e60-fd9c-43bd-b513-8ab1b2e5974c")
		)
		(fp_line
			(start 1.89 -0.92)
			(end 1.89 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d3d33841-fb05-4b9e-ba0b-a6a906d35f43")
		)
		(fp_line
			(start 6.68 0)
			(end 5.73 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2774814c-3d63-4c31-a316-40d914e11765")
		)
		(fp_line
			(start 0.94 0)
			(end 1.89 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5f8bf667-4fa7-4b75-88b9-b4c43cee03c9")
		)
		(fp_line
			(start 5.73 0.92)
			(end 5.73 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "417cb0fa-b00c-4e4d-9325-48b3ba2ebba0")
		)
		(fp_line
			(start 1.89 0.92)
			(end 5.73 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "68a2bc10-8a5c-44af-b05e-5109e77049ee")
		)
		(fp_line
			(start 8.57 -1.05)
			(end -0.95 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e73f070d-6484-4ce2-88a7-b3070af85a74")
		)
		(fp_line
			(start -0.95 -1.05)
			(end -0.95 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7fae0e3a-485f-4bbc-9ade-9699c65506a5")
		)
		(fp_line
			(start 8.57 1.05)
			(end 8.57 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3947c0f0-61eb-42de-9965-dfb4c516c3ff")
		)
		(fp_line
			(start -0.95 1.05)
			(end 8.57 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5f6a28d8-c409-4037-ae94-25ee4cc64ba4")
		)
		(fp_line
			(start 5.61 -0.8)
			(end 2.01 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6fb1f516-d7fb-4cf4-bffd-403ddf070f0d")
		)
		(fp_line
			(start 2.01 -0.8)
			(end 2.01 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8cc704e1-073a-46fe-b8c9-4d4ba76acd9a")
		)
		(fp_line
			(start 7.62 0)
			(end 5.61 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c69c7513-3e80-4ad2-9897-7e82447c1f8b")
		)
		(fp_line
			(start 0 0)
			(end 2.01 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b50d7159-8e88-4af8-9667-e0873c9fdd1e")
		)
		(fp_line
			(start 5.61 0.8)
			(end 5.61 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fcbc28f7-b989-46e4-b4c2-645ee626b195")
		)
		(fp_line
			(start 2.01 0.8)
			(end 5.61 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1ea18dfe-b172-474f-bfa3-4e55f5c65c67")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
			(uuid "0b9dfe2c-d28f-4609-ad2a-44f7ee6914b7")
			(effects
				(font
					(size 0.72 0.72)
					(thickness 0.108)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(R13-Pad1)")
			(pintype "passive")
			(uuid "5f4a7e2b-3bff-4e4d-85e6-2712c89313c3")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "/Triac Circuit4/High_Voltage_L")
			(pintype "passive")
			(uuid "52017f37-8e17-4b02-bb6b-d8702fa4da81")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "1cf323f0-5b59-4946-b795-f6c4f76e4b49")
		(at 53.542855 74.12 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R36"
			(at 0 -1.82 180)
			(layer "F.SilkS")
			(uuid "db81af04-664f-4d36-ae70-f689df31a12f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at -3.64 0 180)
			(layer "F.Fab")
			(uuid "0edab9e6-9113-4995-baa2-27d37e309e9b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "29876b51-a1d1-4afc-8438-2afad79bbcf2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "74ba8a5c-7d89-4d84-958b-6dc8bf205c9a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "d80e32c4-50bf-4f8b-a9d9-2a490448e339")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/15d8fe7c-2a9b-438f-a777-3e4687188af1/ca31a324-056f-45d6-b948-82e97db62734")
		(sheetname "Triac Circuit11")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7d77e332-2ad6-42b1-af55-92a5cb5996c6")
		)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d502d112-ecd7-49ca-b07e-5be59e8d7452")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "744173b2-d2c4-4287-b03e-833300701043")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3632fdce-08c8-42e5-b9d6-4604f78cc098")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8e3d9bd8-08c5-4406-bc8e-0429c28a2fdb")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b71e57a1-0d6f-4aaa-b359-d9045f57a188")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "585daf34-da4b-48a1-a171-6d12182cd44e")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7d99c491-33ce-40dc-acc4-86f4b22e23c1")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "69d46ab6-9da6-43a3-9024-335f528a4cd4")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cdf4e69f-14bf-424d-8e1d-1110bc7998e1")
		)
		(fp_text user "${REFERENCE}"
			(at 3.04 0.01 180)
			(layer "F.Fab")
			(uuid "b614f4d7-8f4b-4c05-82d5-6ed5d80fab28")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 146 "Net-(Q24-B)")
			(pintype "passive")
			(uuid "0e42f58b-1c1a-4c05-bc18-71cc8774d718")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 134 "/Triac Circuit11/Enable")
			(pintype "passive")
			(uuid "d5f28390-96bd-4624-888b-eee669ee58ce")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(uuid "1f1e1f50-1ddd-40fb-9a0a-a43d3501dfbb")
		(at 66.942855 55.94 -90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R31"
			(at 3.809999 -1.92 -90)
			(layer "F.SilkS")
			(uuid "13e28eb4-4468-4418-b03b-8b3ef40fd6e1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "180"
			(at 3.81 1.919999 -90)
			(layer "F.Fab")
			(uuid "f36b843f-009b-497a-803f-9a4c9643feb0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1cd1dc73-2a84-4d80-93ea-3784e0ffdc9a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4fcf0497-2a0c-4697-98f4-e057da220557")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7d1084b9-006a-4811-927f-398d09b0c4f4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/d20c900a-3d9a-4460-9d5d-3ed4d11c2b93/4ab64e29-964f-40b2-bf58-c546b31cd3eb")
		(sheetname "Triac Circuit10")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.89 0.92)
			(end 5.73 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "10b117c8-ea58-4573-b12a-8ff49280cb81")
		)
		(fp_line
			(start 5.73 0.92)
			(end 5.73 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a56933ed-e043-4f42-bf1a-a7a7902bc0a5")
		)
		(fp_line
			(start 0.94 0)
			(end 1.89 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6b4fb7b6-340d-4d44-b425-7ea80ad3ea18")
		)
		(fp_line
			(start 6.68 0)
			(end 5.73 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "32d0dc9f-9be6-42d1-a9dd-88a94e42dd75")
		)
		(fp_line
			(start 1.89 -0.92)
			(end 1.89 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "33596ea1-3c5a-4b23-8af2-a6d546d2a8d3")
		)
		(fp_line
			(start 5.73 -0.92)
			(end 1.89 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dd360dd4-3b42-489b-b57d-df6a2872357b")
		)
		(fp_line
			(start -0.95 1.05)
			(end 8.57 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1c8aa5d5-5846-438a-86d6-73938b184f42")
		)
		(fp_line
			(start 8.57 1.05)
			(end 8.57 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eada779d-3e29-4819-8f6b-b21a04bc2640")
		)
		(fp_line
			(start -0.95 -1.05)
			(end -0.95 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "aa6afda5-8720-4064-a730-02402aed7eae")
		)
		(fp_line
			(start 8.57 -1.05)
			(end -0.95 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "58b95392-7be8-4cae-a786-ac0ab4df0848")
		)
		(fp_line
			(start 2.01 0.8)
			(end 5.61 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4bc9003a-9010-4bf7-a9ed-d7bace40cf3c")
		)
		(fp_line
			(start 5.61 0.8)
			(end 5.61 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3eecc939-39e5-4579-bd33-55ffc819321c")
		)
		(fp_line
			(start 0 0)
			(end 2.01 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "39269331-ae37-4ba0-b296-fa6dda510daf")
		)
		(fp_line
			(start 7.62 0)
			(end 5.61 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "46b063a5-8b2c-45e4-adda-adf573be10ce")
		)
		(fp_line
			(start 2.01 -0.8)
			(end 2.01 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "996612f7-d48a-4b62-80e3-b0fb777e8f2d")
		)
		(fp_line
			(start 5.61 -0.8)
			(end 2.01 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "af711c2b-9c2d-449f-bc05-3a85a26d6d46")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 -90)
			(layer "F.Fab")
			(uuid "00d5fd1b-0bc9-47a4-95d8-d80846cf8a86")
			(effects
				(font
					(size 0.72 0.72)
					(thickness 0.108)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "Net-(R31-Pad1)")
			(pintype "passive")
			(uuid "c5c2cd70-d8dd-41b1-b417-da7e468f6b8b")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "/Triac Circuit10/High_Voltage_L")
			(pintype "passive")
			(uuid "8f085ad7-51f2-410b-979f-50cca46a4f85")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
		(layer "F.Cu")
		(uuid "211e79a6-6972-48cd-90bb-032dc3533346")
		(at 77 137.08 90)
		(descr "Terminal Block Phoenix MKDS-3-2-5.08, 2 pins, pitch 5.08mm, size 10.2x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-3-2-5.08 pitch 5.08mm size 10.2x11.2mm^2 drill 1.3mm pad 2.6mm")
		(property "Reference" "J16"
			(at 3.1 -2.999999 -90)
			(layer "F.SilkS")
			(uuid "2baf0bc1-4535-43b7-a2a8-270946777197")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 2.539999 6.36 90)
			(layer "F.Fab")
			(uuid "f6319052-2b27-44a3-9936-ebda86144f38")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "5da187fe-50cc-4020-a620-f31f727498da")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "9542328c-045a-447f-ab33-8976f8f7e1b0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "bc5ab276-b34d-4881-9605-333c90a700f9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/4b0c0d83-8522-4ffe-8435-2c6bf5567543/60e4d8a3-c16e-48cd-a1fd-61f2968ecc7b")
		(sheetname "Triac Circuit15")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 7.68 -5.96)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8038a968-59fd-4435-8e6e-1d255c3451f0")
		)
		(fp_line
			(start -2.6 -5.96)
			(end 7.68 -5.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e025d8f3-0ddb-44ed-9f9e-54a7488f88b2")
		)
		(fp_line
			(start -2.6 -5.96)
			(end -2.6 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "056fde3e-0fc8-4956-965a-fb1c5eca947d")
		)
		(fp_line
			(start -2.6 -3.9)
			(end 7.68 -3.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c0b55901-6773-4c48-9822-e117560a380b")
		)
		(fp_line
			(start 6.468 -1.654)
			(end 6.088 -1.274)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a9e48138-11af-48d7-a76a-ca864e5aff49")
		)
		(fp_line
			(start 1.388 -1.654)
			(end 1.281 -1.547)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e09a8b14-f934-40d2-ba6b-02476d068dee")
		)
		(fp_line
			(start 6.734 -1.388)
			(end 6.339 -0.992)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ffc49aa3-3f43-49aa-b24e-fe7bed63b2d2")
		)
		(fp_line
			(start 1.654 -1.388)
			(end 1.547 -1.281)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e8bd8bc7-0871-4137-84fe-5ade52dd6373")
		)
		(fp_line
			(start 3.822 0.992)
			(end 3.427 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ee4790c2-9b04-4257-906e-3ac18c651232")
		)
		(fp_line
			(start 4.073 1.274)
			(end 3.693 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f78615bf-71e3-4c92-b11c-f6d1688e203e")
		)
		(fp_line
			(start -1.548 1.281)
			(end -1.654 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e70819d5-e14d-42e1-b374-7eb9a7b21156")
		)
		(fp_line
			(start -1.282 1.547)
			(end -1.388 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3a6cd7af-669a-41cb-b572-3192cdf2fcbd")
		)
		(fp_line
			(start -2.6 2.3)
			(end 7.68 2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6df4b6d3-b8dc-428d-a15e-e173790681c7")
		)
		(fp_line
			(start -2.6 4.8)
			(end 7.68 4.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "40cf7ca0-135a-44bb-9052-6df5786002ab")
		)
		(fp_line
			(start -2.84 4.86)
			(end -2.84 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "37037983-30e9-4d1f-b366-b8428148b48f")
		)
		(fp_line
			(start -2.6 5.36)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "416a4461-f008-413b-8e7a-72c6aee76f51")
		)
		(fp_line
			(start -2.84 5.6)
			(end -2.34 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b8c005f1-6cdb-4117-ade7-fe93f8bdd008")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.26 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "ebfe8079-519f-451a-9787-3ede1402e86c")
		)
		(fp_circle
			(center 0 0)
			(end 2.18 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "074cc7b8-dde4-44d8-9b33-29b9d2b9e969")
		)
		(fp_line
			(start 8.13 -6.4)
			(end -3.04 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c6408cd1-8a96-420b-a200-5d57ae0fbc3f")
		)
		(fp_line
			(start -3.04 -6.4)
			(end -3.04 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5f669554-30a5-4621-81de-5823e4e82789")
		)
		(fp_line
			(start 8.13 5.8)
			(end 8.13 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3521e171-6ea6-4265-9bcf-3fe6a5d77061")
		)
		(fp_line
			(start -3.04 5.8)
			(end 8.13 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "37888dbc-1497-4a2b-b168-8fcfc7b956bb")
		)
		(fp_line
			(start 7.62 -5.9)
			(end 7.62 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b4e1884a-a104-450f-baf8-2e64dc9bc6ea")
		)
		(fp_line
			(start -2.54 -5.9)
			(end 7.62 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e79afb04-7c4b-41b2-835e-c7a8d3269556")
		)
		(fp_line
			(start -2.54 -3.9)
			(end 7.62 -3.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5baa19aa-b022-4d64-b313-81f128b7dac8")
		)
		(fp_line
			(start 6.353 -1.517)
			(end 3.564 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "76db026c-61aa-410e-82da-cdc4a5336ab1")
		)
		(fp_line
			(start 1.273 -1.517)
			(end -1.517 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "06952afc-49d0-44c6-8d91-da3793821bba")
		)
		(fp_line
			(start 6.597 -1.273)
			(end 3.808 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2a287366-c446-48d5-85cc-f3df89f5702d")
		)
		(fp_line
			(start 1.517 -1.273)
			(end -1.273 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1ca5a476-2a58-450b-af3a-d19965522fb3")
		)
		(fp_line
			(start -2.54 2.3)
			(end 7.62 2.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f04ad7d8-dd10-44b7-b28a-44e17c1eafc9")
		)
		(fp_line
			(start -2.54 4.8)
			(end -2.54 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b73d80e5-43e1-4530-a017-77eb751880d8")
		)
		(fp_line
			(start -2.54 4.8)
			(end 7.62 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ab462253-1df5-4626-9c80-ed6253669f44")
		)
		(fp_line
			(start 7.62 5.3)
			(end -2.04 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7c088f52-7ad7-4335-807e-11336564596a")
		)
		(fp_line
			(start -2.04 5.3)
			(end -2.54 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fdaf8663-cc31-4bc7-9136-57619a1abaeb")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.08 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "609219a1-2cba-4c41-afd7-9ccdbd340e35")
		)
		(fp_circle
			(center 0 0)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "55783d11-a27c-4330-af26-e4e1e12aaaf6")
		)
		(fp_text user "${REFERENCE}"
			(at 2.539999 3.1 90)
			(layer "F.Fab")
			(uuid "ae5d8ee0-9385-4cf9-b0ac-9c23607c06c1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 87 "/Triac Circuit15/High_Voltage_L")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "22137b1e-854f-4291-aeee-dbec05183eac")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/Triac Circuit15/High_Voltage_Out")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "7d11f2e9-dd6a-41bc-97f0-dfc1c9e0bec9")
		)
		(model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "21f3052d-f9e0-4c98-b814-888835e0de18")
		(at 45.8 159.4)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R63"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "c1cf582f-86af-459e-8a67-839b36de58ac")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1k"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "079d21bd-5e82-4adc-9d2f-d8b44ecd4e45")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a6019846-9aea-4848-9d5c-c1ea7442064c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "49ac9df6-1b9a-49e5-9a97-e3ee31764bdb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "38eed2f7-a38e-4ec1-ae97-8fa351b1ee20")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/b0506013-ce11-444b-bc5e-374e3b418856/547580b6-9698-46ab-b758-90ae2111cb33")
		(sheetname "ZeroCrossDetection2")
		(sheetfile "ZeroCrossDetection.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a26a4082-f6f4-410d-8d45-a3ac826ce595")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1d3a6e41-9838-4126-b110-e1e10d9556d6")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d794a282-0898-4e67-bea6-17fc53298f17")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d22f918c-872b-4fc6-905e-2e47895d9fa5")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "606cacb4-cbec-4cea-a484-60b03a6a641e")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eb3e6c02-95c3-4970-baa2-d51e6dc82341")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d6a03487-b6f2-49eb-a801-f5e36e8e379b")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1c7e15bf-37c7-4e2b-ab64-3c25cfdf7790")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "688429a9-6343-4a70-a22e-05643524444b")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ea63602b-677d-465e-80e6-91b925c79d62")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "e67bd5a0-5a86-47bc-b999-b02b466f54be")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 170 "/ZeroCrossDetection2/OUT")
			(pintype "passive")
			(uuid "5643e0a8-c5d2-4c5f-bc0c-d35c70616c29")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 167 "+3.3V")
			(pintype "passive")
			(uuid "91d01548-8dd5-475f-92e9-abff29f5af24")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(uuid "232d0c9a-0752-47ab-a532-e1a9d47faefb")
		(at 32.826429 111.9 -90)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "Q13"
			(at 6.04 -2.445 90)
			(layer "F.SilkS")
			(uuid "6528649b-facb-4ab1-998e-bcfba7272622")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BTA16-600B"
			(at 2.54 2.5 90)
			(layer "F.Fab")
			(uuid "2eeb8285-af6a-4bc2-b66d-1f7cf100771b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "30ad8e91-7706-40a3-b4e0-523fb9ae2acc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "b4c2d05a-6687-45d2-9075-85809ab33f45")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "a2e82a59-c69c-43e2-8191-3c476ef7d683")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO?220*")
		(path "/4a841339-199f-4bc7-a6bd-fe2a9936827c/d1257be0-2394-4f08-8984-f580162b15f9")
		(sheetname "Triac Circuit6")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.58 1.371)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d8ad3d0b-a514-4926-8210-0358568c1c93")
		)
		(fp_line
			(start -2.58 -1.76)
			(end 7.66 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3236f7f9-7c77-4c57-ba1c-1645c61b49e4")
		)
		(fp_line
			(start -2.58 -3.27)
			(end -2.58 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "56addcf9-685e-4ec6-a3ed-7643cc2c1571")
		)
		(fp_line
			(start -2.58 -3.27)
			(end 7.66 -3.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aab734f9-6505-48cf-9346-603a86136a4d")
		)
		(fp_line
			(start 0.69 -3.27)
			(end 0.69 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1f4d7ff7-340c-47af-aae5-4c148165ea2e")
		)
		(fp_line
			(start 4.391 -3.27)
			(end 4.391 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "51e099d3-dbc5-4a5e-accf-8abd595bd9f3")
		)
		(fp_line
			(start 7.66 -3.27)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "84327f58-77a0-461e-8950-4f01dab31a3e")
		)
		(fp_line
			(start -2.71 1.51)
			(end 7.79 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c9aa018e-c652-44d0-bce5-7bb43fa024a9")
		)
		(fp_line
			(start 7.79 1.51)
			(end 7.79 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "41478cc8-fec5-43fc-91b6-6f1f7c2eb022")
		)
		(fp_line
			(start -2.71 -3.4)
			(end -2.71 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6c7cb3d7-2168-4ea8-b26c-e1ac3a513f9c")
		)
		(fp_line
			(start 7.79 -3.4)
			(end -2.71 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "72375175-3bc4-4fe0-9eee-5806c8409c1d")
		)
		(fp_line
			(start -2.46 1.25)
			(end 7.54 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a96df703-f0fc-43ea-98a6-1329de55e7c4")
		)
		(fp_line
			(start 7.54 1.25)
			(end 7.54 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "db8ce114-7301-469b-a06c-35bb06fb6aca")
		)
		(fp_line
			(start -2.46 -1.88)
			(end 7.54 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d6f51978-f5d0-43bd-8fa0-97cf5b887a1a")
		)
		(fp_line
			(start -2.46 -3.15)
			(end -2.46 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3b98f5a4-7131-4673-a305-070657f6982b")
		)
		(fp_line
			(start 0.69 -3.15)
			(end 0.69 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3eae916a-d3e2-4609-80a9-83cae4fadbf4")
		)
		(fp_line
			(start 4.39 -3.15)
			(end 4.39 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d6aa6ba1-63d1-487c-b859-e6515f9c9aaf")
		)
		(fp_line
			(start 7.54 -3.15)
			(end -2.46 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d03314db-93cf-4167-8f04-0cc677ce2da4")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 -4.27 90)
			(layer "F.Fab")
			(uuid "eebf7b0c-392f-44cf-b566-794059e3493d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "/Triac Circuit6/High_Voltage_L")
			(pinfunction "A1")
			(pintype "passive")
			(uuid "56baf5e0-b133-437d-b9ea-77e690f4d3f8")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/Triac Circuit6/High_Voltage_Out")
			(pinfunction "A2")
			(pintype "passive")
			(uuid "a636bb76-fb2e-4d0d-8907-762fea245b4e")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(Q13-G)")
			(pinfunction "G")
			(pintype "input")
			(uuid "21ef2cf9-f52f-448d-b601-db16640cc397")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-6_W7.62mm"
		(layer "F.Cu")
		(uuid "2c4711b1-b01d-4b3e-acba-00e7c9f6e5c2")
		(at 44.914287 131.005 180)
		(descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U9"
			(at 3.6 -2.33 0)
			(layer "F.SilkS")
			(uuid "619fbe0e-da59-441c-8846-4b8cc7289fce")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MOC3021M"
			(at 3.81 7.41 0)
			(layer "F.Fab")
			(uuid "5c7d8dea-7bfe-483e-b20e-1b451774b648")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "c0d258ce-b30f-41d1-bdbc-f667709cfd59")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3023M-D.PDF"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "435a8f9c-a5be-4fce-9442-8a1252345b68")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "1078a7ec-31f6-4a25-bc84-6a035a5afb0c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*")
		(path "/6df26bae-1f6b-42ab-99b6-42742cd98df0/0262e914-5435-478f-be04-ece49b8102cf")
		(sheetname "Triac Circuit7")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 6.46 6.41)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "62aa72bd-13be-4851-94f7-731e36203593")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "343a4bc8-c44e-44b1-9802-29c319154bd7")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "66e31c69-e278-45b1-9f25-2c60deb68fa7")
		)
		(fp_line
			(start 1.16 6.41)
			(end 6.46 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9d871034-460c-4db2-b5ed-5c2ec82a9d8a")
		)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2bf0484f-c486-4f88-97b0-961e5a0b799b")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ac36b01a-7024-434b-8ecb-653584b4ac33")
		)
		(fp_line
			(start 8.7 6.6)
			(end 8.7 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f7a835be-9701-47ff-811c-249fdd5fad29")
		)
		(fp_line
			(start 8.7 -1.55)
			(end -1.1 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fc58515c-d5e7-486c-8dee-03d7b01a108a")
		)
		(fp_line
			(start -1.1 6.6)
			(end 8.7 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dfb09b90-e08e-46af-971b-37d42418ceff")
		)
		(fp_line
			(start -1.1 -1.55)
			(end -1.1 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f423f647-5001-480c-813d-c30642f86da1")
		)
		(fp_line
			(start 6.985 6.35)
			(end 0.635 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "12a3ee02-343e-477c-a4d6-569d24194857")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3be369c7-676f-48bc-8f4a-8680df7ff773")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3f1be906-d8d3-48ba-b4c6-9f5186999888")
		)
		(fp_line
			(start 0.635 6.35)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "860caf32-bb4f-41c1-8d38-61129cdd7a91")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f8a183d5-ebd5-45f6-be4f-337530ec8726")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.54 0)
			(layer "F.Fab")
			(uuid "21f86ca0-27c7-469e-99f1-1029717cf571")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 116 "Net-(R23-Pad1)")
			(pintype "passive")
			(uuid "4b0755dc-f779-4c92-99c3-578b4a43b679")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 126 "Net-(Q16-C)")
			(pintype "passive")
			(uuid "6b3e20d1-22ed-40c4-99a8-39ff210efdc0")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 96 "unconnected-(U9-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "b3c84cb2-47ce-4198-bdbc-3a83b8775f94")
		)
		(pad "4" thru_hole oval
			(at 7.62 5.08 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(Q15-G)")
			(pintype "passive")
			(uuid "50a0f601-ddd8-4861-b4a1-99084c63042a")
		)
		(pad "5" thru_hole oval
			(at 7.62 2.54 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 97 "unconnected-(U9-NC-Pad5)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "fa75259a-15fd-4d1c-bfbb-ede09c9e6a51")
		)
		(pad "6" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "Net-(R22-Pad1)")
			(pintype "passive")
			(uuid "2a9204c0-20d7-402d-8258-b00776644e2b")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-6_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-6_W7.62mm"
		(layer "F.Cu")
		(uuid "2d6325f6-a6e1-4b62-bd31-731f04a9e35a")
		(at 57.142855 72.195)
		(descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U13"
			(at 3.599999 -2.33 180)
			(layer "F.SilkS")
			(uuid "b34df951-24a9-4ae2-8a84-1f46a4321755")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MOC3021M"
			(at 3.81 7.409999 180)
			(layer "F.Fab")
			(uuid "2fa682d4-0cf2-4007-932c-66baefcfe5c5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "85948595-d6fd-4ef9-aa07-5cd410f00246")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3023M-D.PDF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6cf267ac-9cc9-4237-b3e2-8e36d3826543")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3d8d5eba-3494-42ad-bdd8-1b224997efdf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*")
		(path "/15d8fe7c-2a9b-438f-a777-3e4687188af1/0262e914-5435-478f-be04-ece49b8102cf")
		(sheetname "Triac Circuit11")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f07e8dfb-a066-45c0-8426-63d408959b7a")
		)
		(fp_line
			(start 1.16 6.41)
			(end 6.46 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b9d641fc-1bae-41fe-8a9a-d82cc270461f")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bfa53637-aa86-44e5-aca1-f97105ec4d49")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ec1214d4-999f-4c7b-9a81-b070d07001f6")
		)
		(fp_line
			(start 6.46 6.41)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5e73573b-5780-4da4-b3ba-a98c0acfe0c5")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f477f2c2-42d7-40da-a0a7-ddf125d8d465")
		)
		(fp_line
			(start -1.1 -1.55)
			(end -1.1 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8df197c7-b298-421b-8578-838e43e15b59")
		)
		(fp_line
			(start -1.1 6.6)
			(end 8.7 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f06281ca-d97b-4f71-a2fd-7f216e00a268")
		)
		(fp_line
			(start 8.7 -1.55)
			(end -1.1 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "673b2892-b0df-48da-841a-09545eaa8618")
		)
		(fp_line
			(start 8.7 6.6)
			(end 8.7 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "db7b5e9f-508f-474f-917e-eac5406328dd")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "741a0431-c30b-411a-b5ad-9e0e3d2a94c0")
		)
		(fp_line
			(start 0.635 6.35)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c9d73ee1-1d40-4c16-b818-9525f75618a6")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "84c9ce46-6795-48e3-a9b0-e40bb9972ffc")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a0dfe1f7-b745-419f-a0ba-5847583c4b12")
		)
		(fp_line
			(start 6.985 6.35)
			(end 0.635 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1f41836c-e3fc-4699-accf-6e42b980ff47")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.539999 180)
			(layer "F.Fab")
			(uuid "24a2c916-a653-4f63-bfb0-f42a93a9eae1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 120 "Net-(R35-Pad1)")
			(pintype "passive")
			(uuid "e45a3235-ee96-4242-8c64-4127a2907fcb")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 147 "Net-(Q24-C)")
			(pintype "passive")
			(uuid "b6653c3f-8046-4937-b1c6-9ff489272655")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 102 "unconnected-(U13-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "ffcb2df6-6c4b-4d92-a9fc-77c333cd5ec1")
		)
		(pad "4" thru_hole oval
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 145 "Net-(Q23-G)")
			(pintype "passive")
			(uuid "9b944e7f-89fe-4b18-9c1e-b2f0fe6c3226")
		)
		(pad "5" thru_hole oval
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 103 "unconnected-(U13-NC-Pad5)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "20f10770-91c2-4973-bc06-fe7b56781072")
		)
		(pad "6" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "Net-(R34-Pad1)")
			(pintype "passive")
			(uuid "cd2c9ab8-815f-4e66-8d24-361bfafbcf94")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-6_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
		(layer "F.Cu")
		(uuid "2d87fda9-b766-4b9a-9472-7abc69d9d09d")
		(at 25.057142 127.08 -90)
		(descr "Terminal Block Phoenix MKDS-3-2-5.08, 2 pins, pitch 5.08mm, size 10.2x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-3-2-5.08 pitch 5.08mm size 10.2x11.2mm^2 drill 1.3mm pad 2.6mm")
		(property "Reference" "J8"
			(at 3.1 -3 90)
			(layer "F.SilkS")
			(uuid "6f4d53d1-ce00-407f-a3c5-23ad26fced4b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 2.54 6.36 -90)
			(layer "F.Fab")
			(uuid "d53a57c8-f1d1-4955-a765-8bbfac8ec9c7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "f4fb716d-60bc-4b73-b353-b1ad7913c80d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "ad2bd332-590f-4646-b2b4-e0e7d856c5f2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "afcd6493-af4a-49a7-ad6e-420bf4d8e5fa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/6df26bae-1f6b-42ab-99b6-42742cd98df0/60e4d8a3-c16e-48cd-a1fd-61f2968ecc7b")
		(sheetname "Triac Circuit7")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.84 5.6)
			(end -2.34 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "df56689f-abbd-4721-9ffd-e2f8e511c104")
		)
		(fp_line
			(start -2.6 5.36)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1848c213-d1ea-4015-95db-7f0c81a8bf4a")
		)
		(fp_line
			(start -2.84 4.86)
			(end -2.84 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "91f03fa3-6b6c-412c-bd6b-95a611456824")
		)
		(fp_line
			(start -2.6 4.8)
			(end 7.68 4.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1bd01fb9-60e7-4079-b3af-8fc8923d1513")
		)
		(fp_line
			(start -2.6 2.3)
			(end 7.68 2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d940bb2e-c871-4aec-8d5a-2f8d3e3084e0")
		)
		(fp_line
			(start -1.282 1.547)
			(end -1.388 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "95a607b1-6686-48a7-abfe-34a9e9aeb4f3")
		)
		(fp_line
			(start -1.548 1.281)
			(end -1.654 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ff8e2a46-24fc-4b3e-a8e1-4fb0aa08d452")
		)
		(fp_line
			(start 4.073 1.274)
			(end 3.693 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a454b781-bb51-437d-a2d1-d117dd9401f6")
		)
		(fp_line
			(start 3.822 0.992)
			(end 3.427 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5c027e02-3daa-4084-8cfd-42e93fb68965")
		)
		(fp_line
			(start 1.654 -1.388)
			(end 1.547 -1.281)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8eb70ece-b1ac-470c-a4a7-ec52490beb6e")
		)
		(fp_line
			(start 6.734 -1.388)
			(end 6.339 -0.992)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e7b40a81-58f3-4dfb-95eb-f6501e584eff")
		)
		(fp_line
			(start 1.388 -1.654)
			(end 1.281 -1.547)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "09e2c009-d0b6-4537-ba7e-aedb8858cb05")
		)
		(fp_line
			(start 6.468 -1.654)
			(end 6.088 -1.274)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "75c6ba82-3d40-4b95-8bf9-80fd9150e1fc")
		)
		(fp_line
			(start -2.6 -3.9)
			(end 7.68 -3.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "912b9007-5976-4cf6-bbf6-389ab4cf5fba")
		)
		(fp_line
			(start -2.6 -5.96)
			(end -2.6 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b691e64c-9b90-4077-bd72-b9752e7044b1")
		)
		(fp_line
			(start -2.6 -5.96)
			(end 7.68 -5.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "90a1d80c-16b7-4325-b4ab-60576f462640")
		)
		(fp_line
			(start 7.68 -5.96)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "65c18ea6-214f-45c2-ba50-8ab56576be5e")
		)
		(fp_circle
			(center 0 0)
			(end 2.18 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "9286a053-c682-4d4e-822e-b707a4e115e0")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.26 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "eee03100-939b-4257-bc67-cf44dbbeb850")
		)
		(fp_line
			(start -3.04 5.8)
			(end 8.13 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "18268b93-eb88-41c9-ab0d-914e7e9dc460")
		)
		(fp_line
			(start 8.13 5.8)
			(end 8.13 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "afd0d540-a361-430b-b87d-21543a9bf152")
		)
		(fp_line
			(start -3.04 -6.4)
			(end -3.04 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "61c66698-9258-4823-aba7-a5e1aedf86a8")
		)
		(fp_line
			(start 8.13 -6.4)
			(end -3.04 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "36b517de-ca95-4903-abbe-1b10e98cd5fe")
		)
		(fp_line
			(start -2.04 5.3)
			(end -2.54 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1988b4d9-b58d-4025-8c91-6c3ea906f2ec")
		)
		(fp_line
			(start 7.62 5.3)
			(end -2.04 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "76d54a2c-2cd9-4139-97e9-6338c77b4f06")
		)
		(fp_line
			(start -2.54 4.8)
			(end 7.62 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d1ef1f6d-609f-4add-8f84-1089ef5c4615")
		)
		(fp_line
			(start -2.54 4.8)
			(end -2.54 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "86081d8f-b4ac-4e68-8699-bfe30a9dacb7")
		)
		(fp_line
			(start -2.54 2.3)
			(end 7.62 2.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cdf157f1-e9ba-40d0-a600-32d770e01703")
		)
		(fp_line
			(start 1.517 -1.273)
			(end -1.273 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d61499d1-30c6-494a-b66f-e46d313ff64a")
		)
		(fp_line
			(start 6.597 -1.273)
			(end 3.808 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "844b5681-e969-4e06-b1d3-9303109d4e03")
		)
		(fp_line
			(start 1.273 -1.517)
			(end -1.517 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "58ff00de-ba3e-4952-a9e7-e987cad7f9a9")
		)
		(fp_line
			(start 6.353 -1.517)
			(end 3.564 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d60adb2f-8f5d-4c7c-afba-2cb5e198f53f")
		)
		(fp_line
			(start -2.54 -3.9)
			(end 7.62 -3.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f2b7d1a2-e95d-4069-8c96-34120945f2a4")
		)
		(fp_line
			(start -2.54 -5.9)
			(end 7.62 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2fe6b80a-de68-4e34-9701-fdf4aa0b3d6d")
		)
		(fp_line
			(start 7.62 -5.9)
			(end 7.62 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3905d80d-e8ea-4484-9684-da6f3ec9d50b")
		)
		(fp_circle
			(center 0 0)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "f0509201-5fcb-4a44-b925-b917f7277198")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.08 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "e8261a5c-d7ba-4614-b13c-578820552159")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 3.1 -90)
			(layer "F.Fab")
			(uuid "d71b9a77-2c51-4719-914b-eac1d15a7c1c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "/Triac Circuit7/High_Voltage_L")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "1e6f6e2b-c8f5-4a77-ad24-0ca80a262e61")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/Triac Circuit7/High_Voltage_Out")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "3f4bac8a-7955-40ab-adf2-1fa2ac99b14b")
		)
		(model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "2dbfb5e6-a2c5-4cfb-9fc7-62e763eff9ca")
		(at 54.005355 122.639999)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q30"
			(at 0 -2.4 180)
			(layer "F.SilkS")
			(uuid "7ea5afc0-cede-4c7b-8f12-f1d33de87277")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BC818"
			(at 0 2.4 180)
			(layer "F.Fab")
			(uuid "d6a712b7-72a7-47d2-906d-16ce08c67a44")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8afa87cc-bf96-4f60-99d6-5e3dd71244a8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC818-D.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "97832ec4-08d6-43de-ac1d-e2ac0468bebc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "68c98947-a10d-4852-b024-983d439e9c9a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/683a6cfc-1cb6-4c63-ae1f-c9d1fdc220d0/00e550ea-8431-483d-ac3c-b4a719825546")
		(sheetname "Triac Circuit14")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -1.56)
			(end -1.675 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cbeabadf-7e61-47e6-b87d-c843f9067638")
		)
		(fp_line
			(start 0 -1.56)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ea915a4a-1ad1-489b-b7e9-32e33ebb495f")
		)
		(fp_line
			(start 0 1.56)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "511d045b-b589-4046-a1c8-2f3f0c2dc554")
		)
		(fp_line
			(start 0 1.56)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5336224d-f7bf-4fcc-9fbb-7a5513602253")
		)
		(fp_line
			(start -1.92 -1.7)
			(end -1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2d27f03f-02c4-4e73-b1c0-d7ac6aab988e")
		)
		(fp_line
			(start -1.92 1.7)
			(end 1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fc7d9c16-7938-4fc4-bc77-b2916b0c4a16")
		)
		(fp_line
			(start 1.92 -1.7)
			(end -1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "acd5739a-d6bf-47ba-b8b2-bc71a616403e")
		)
		(fp_line
			(start 1.92 1.7)
			(end 1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dd5d2617-642f-473e-8cf8-f20d3f72b008")
		)
		(fp_line
			(start -0.65 -1.125)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "65f3d369-dde6-4749-9b2b-12ec79c9c999")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e27872c8-1af1-4ff2-8fc1-86d5abe81a45")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7b79f335-d0a8-42f7-8649-7c3fecda3cdf")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "527eefcb-e208-444f-8d86-0cb53d2e6709")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "80ca3bcc-b793-4754-9876-602457857835")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
			(uuid "cb6b2a51-336b-44fb-9100-a896b0a897ea")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 155 "Net-(Q30-B)")
			(pinfunction "B")
			(pintype "input")
			(uuid "5bb5b707-cab8-47a8-a61e-ece4ae3a84d3")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "GND")
			(pinfunction "E")
			(pintype "passive")
			(uuid "886c8a2c-81cd-451e-89dc-92c2a6b2bbb6")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 156 "Net-(Q30-C)")
			(pinfunction "C")
			(pintype "passive")
			(uuid "d5eb726a-6d9f-4361-84df-b71a562d5cd8")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "2ecf78c3-befb-47ee-8375-56fa5a6da766")
		(at 48.657142 98.6)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R18"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "76dd8502-ef22-4ccd-b6b2-35d3f171bae0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at -3.64 0 0)
			(layer "F.Fab")
			(uuid "5a98db2f-362c-4e20-986a-5314a9883a0e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6c82fa28-67ae-4f58-b545-e96019151b73")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e4520f77-3f3e-4eaf-b8c7-3bf372ad9d1b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "01264338-86fa-488b-b786-694bdc389655")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/6eb41966-4a54-4fd9-a1be-49d2f272d785/ca31a324-056f-45d6-b948-82e97db62734")
		(sheetname "Triac Circuit5")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "68c7dd1a-728b-45d6-957c-248465da0cdf")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eacfccdb-496f-4d23-be5f-1e7301d4a980")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "917451ea-2fa1-47fc-882f-6cad1b0a6492")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "adb484dc-73c8-4e47-871f-1a5ed34a3c70")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2b1b7797-1c8d-42ec-8656-7380925088e6")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c2bdd96b-ae16-41e0-9c01-22c8cd929bb9")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b1a27d37-29da-48c6-9c75-9f29b4634731")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2ab89796-8240-4d63-a7b6-1e0fef2d8bf8")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "46efe7bc-4d64-441a-81e3-3765f3f7798b")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "63e59f98-801c-4ba0-a31f-3c2327708cfc")
		)
		(fp_text user "${REFERENCE}"
			(at 3.04 0.01 0)
			(layer "F.Fab")
			(uuid "436d9412-51d7-4b13-b8c9-785bdde990d1")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 68 "Net-(Q12-B)")
			(pintype "passive")
			(uuid "7d340828-82fa-42cc-85d7-c3e7ee35fbba")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 29 "/Triac Circuit5/Enable")
			(pintype "passive")
			(uuid "2677c85a-106c-4d35-90d9-fab063185a05")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "2edd5c47-ce09-406d-b51d-c025e5e4fa1e")
		(at 54.005355 107.399999)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q28"
			(at 0 -2.4 180)
			(layer "F.SilkS")
			(uuid "b7744d37-5d8c-41e7-b39d-8754ed9b4124")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BC818"
			(at 0 2.4 180)
			(layer "F.Fab")
			(uuid "34d1c845-5e95-4036-beed-5da38a1d261b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e25429de-c982-4006-9c8c-ccde659d7aab")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC818-D.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0188cec2-383b-4b13-be34-abf7661c6c55")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ee639897-87fc-4d48-b0a4-9eba0b008b07")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/4a948621-4b4c-41c9-b07f-b928eecc9e1e/00e550ea-8431-483d-ac3c-b4a719825546")
		(sheetname "Triac Circuit13")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -1.56)
			(end -1.675 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e2c738e4-f8cd-4be1-b460-ee3f7f72660e")
		)
		(fp_line
			(start 0 -1.56)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4b069a71-e44c-4e46-81a0-d9c87881b522")
		)
		(fp_line
			(start 0 1.56)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "15575b18-88fd-4e3c-a528-7e7400222d76")
		)
		(fp_line
			(start 0 1.56)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "16ee6000-92fe-481e-b865-7ed07a6d16c9")
		)
		(fp_line
			(start -1.92 -1.7)
			(end -1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "898fcf99-0c58-4ea2-beae-383ead131354")
		)
		(fp_line
			(start -1.92 1.7)
			(end 1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f6926328-d2e7-45b3-a70d-650c2c91d367")
		)
		(fp_line
			(start 1.92 -1.7)
			(end -1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "228847e5-9546-4d2c-9a47-1fcc1e902e5b")
		)
		(fp_line
			(start 1.92 1.7)
			(end 1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bb7b9501-4a8d-4511-a8fa-e1a25507ab43")
		)
		(fp_line
			(start -0.65 -1.125)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "794f8626-8de2-4b9c-8f3c-9cff732aba33")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1798de21-1ebb-416b-a7ed-47be44672227")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1a09510e-efa1-4ad3-9246-ad00337098ab")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c6f6a8be-a3ce-4fe5-bab0-6b3555e9fddd")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b60286d0-d6d5-4f62-982f-138a2c27640a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
			(uuid "4ea2201f-c0de-40a9-9151-d10d19841c73")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 152 "Net-(Q28-B)")
			(pinfunction "B")
			(pintype "input")
			(uuid "3f33f18b-2c9c-4779-b402-8581e20a05c2")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "GND")
			(pinfunction "E")
			(pintype "passive")
			(uuid "beddaa1f-e985-42f5-b658-db8d45ed9fee")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 153 "Net-(Q28-C)")
			(pinfunction "C")
			(pintype "passive")
			(uuid "19011454-9e86-4875-ba34-baa0f57d18ef")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
		(layer "F.Cu")
		(uuid "3034e429-f9f9-44a2-8240-03a24b63e1fb")
		(at 25.085713 35.64 -90)
		(descr "Terminal Block Phoenix MKDS-3-2-5.08, 2 pins, pitch 5.08mm, size 10.2x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-3-2-5.08 pitch 5.08mm size 10.2x11.2mm^2 drill 1.3mm pad 2.6mm")
		(property "Reference" "J2"
			(at 3.1 -3 90)
			(layer "F.SilkS")
			(uuid "876f7c78-b034-4358-9514-45728adcae2c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 2.54 6.36 -90)
			(layer "F.Fab")
			(uuid "f3e94841-be13-4257-be0a-7b781baba749")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "1f418071-3847-485b-b89a-0e3e7fc6b242")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "e3fea66e-0601-4883-8fed-16cb3484527e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "2406920b-7598-4f38-ba13-17a4e59e4ad0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/98cc9bb7-a6bb-4cad-bced-cd34a966891d/60e4d8a3-c16e-48cd-a1fd-61f2968ecc7b")
		(sheetname "Triac Circuit1")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.84 5.6)
			(end -2.34 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aeb04927-768c-4d72-bb9c-cd91d0868e45")
		)
		(fp_line
			(start -2.6 5.36)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f1952131-bb00-4437-84ef-4e615369e701")
		)
		(fp_line
			(start -2.84 4.86)
			(end -2.84 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "828af886-3013-4916-a5ab-6ac0588882d7")
		)
		(fp_line
			(start -2.6 4.8)
			(end 7.68 4.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "889c27dd-2e0c-452d-a230-f3591fc86fa9")
		)
		(fp_line
			(start -2.6 2.3)
			(end 7.68 2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "19252480-2932-4054-9f44-e0b80646b1bf")
		)
		(fp_line
			(start -1.282 1.547)
			(end -1.388 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "22d04405-a0ec-4288-a725-5799133ec625")
		)
		(fp_line
			(start -1.548 1.281)
			(end -1.654 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ccc13e8f-7738-4e69-a250-d4472e0e0e0b")
		)
		(fp_line
			(start 4.073 1.274)
			(end 3.693 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7d5965d4-e48e-4b9b-bfaf-140d446aaebd")
		)
		(fp_line
			(start 3.822 0.992)
			(end 3.427 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6bf5b4c5-de0b-4f6a-9587-69ff75c8c002")
		)
		(fp_line
			(start 1.654 -1.388)
			(end 1.547 -1.281)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2a30739d-13d8-4d5f-bc91-f17c5b8eef83")
		)
		(fp_line
			(start 6.734 -1.388)
			(end 6.339 -0.992)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d1ad73e1-3068-4798-840d-676f7806cb98")
		)
		(fp_line
			(start 1.388 -1.654)
			(end 1.281 -1.547)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "80016e25-1226-4bd9-865f-889cfebcd50a")
		)
		(fp_line
			(start 6.468 -1.654)
			(end 6.088 -1.274)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9ada878c-bcb5-4f11-abce-f812ed5aea15")
		)
		(fp_line
			(start -2.6 -3.9)
			(end 7.68 -3.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "db336dce-d62a-4189-bf82-01df5c470adb")
		)
		(fp_line
			(start -2.6 -5.96)
			(end -2.6 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "65acea52-ecee-4679-bdcb-7e67eecef404")
		)
		(fp_line
			(start -2.6 -5.96)
			(end 7.68 -5.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6e16ad79-6f1b-4727-96c8-c2d9d414b675")
		)
		(fp_line
			(start 7.68 -5.96)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5cdce361-689e-4a7e-b36f-863d1cb2723e")
		)
		(fp_circle
			(center 0 0)
			(end 2.18 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "d1693ad8-da68-42ce-86b5-7a51442185b0")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.26 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "c7892545-5434-4f39-99ac-713ebe784bc8")
		)
		(fp_line
			(start -3.04 5.8)
			(end 8.13 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b705c0d9-299c-49ab-b90e-7bab23ddba31")
		)
		(fp_line
			(start 8.13 5.8)
			(end 8.13 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9289631c-3fe9-4930-9723-392543a138ca")
		)
		(fp_line
			(start -3.04 -6.4)
			(end -3.04 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3829e970-1ad3-41ad-93d6-57fe355ce287")
		)
		(fp_line
			(start 8.13 -6.4)
			(end -3.04 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "95d1cfcd-3ea0-45ff-8992-ed89fd57646c")
		)
		(fp_line
			(start -2.04 5.3)
			(end -2.54 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4f850e4d-2f41-42ea-85e1-3c844bc1a760")
		)
		(fp_line
			(start 7.62 5.3)
			(end -2.04 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "32e86d5b-aa8c-49c3-8b94-85b6faf6c5e2")
		)
		(fp_line
			(start -2.54 4.8)
			(end 7.62 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0476c35b-7177-4f18-8623-984529b71a0a")
		)
		(fp_line
			(start -2.54 4.8)
			(end -2.54 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dbb6fd24-29dc-4e01-a66d-cae01a7840d2")
		)
		(fp_line
			(start -2.54 2.3)
			(end 7.62 2.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4467f603-d548-4020-9894-4b0baa27e22b")
		)
		(fp_line
			(start 1.517 -1.273)
			(end -1.273 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f9c679a8-cd48-48ed-a861-82c439ca0e3a")
		)
		(fp_line
			(start 6.597 -1.273)
			(end 3.808 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fb11b81f-f4f2-4707-8a1b-32febd4c495b")
		)
		(fp_line
			(start 1.273 -1.517)
			(end -1.517 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c267cd66-a6d4-4ae5-96f5-4b9a7b45acd7")
		)
		(fp_line
			(start 6.353 -1.517)
			(end 3.564 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5699a3a6-a2a6-4df8-bc09-e5a18dedeea7")
		)
		(fp_line
			(start -2.54 -3.9)
			(end 7.62 -3.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b2fa4b38-b2c3-4254-b883-48b04dcaf831")
		)
		(fp_line
			(start -2.54 -5.9)
			(end 7.62 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "106904f1-24f8-493b-afc7-e0c7c8e733a7")
		)
		(fp_line
			(start 7.62 -5.9)
			(end 7.62 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "669cda5c-8da3-4acb-8d42-202e289847ab")
		)
		(fp_circle
			(center 0 0)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "102fe86c-1f58-43e9-9d61-ebb8f35b0a1c")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.08 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "dce701a0-48a6-438b-9546-d6ede8acf8a3")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 3.1 -90)
			(layer "F.Fab")
			(uuid "251c449c-3dc8-4adf-8587-a6967a5e082c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/Triac Circuit1/High_Voltage_L")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "58e28e6d-4886-4473-8a51-d110a69cbd22")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/Triac Circuit1/High_Voltage_Out")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "a03c2657-87b5-4d8b-b2ec-2eaf2977229f")
		)
		(model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_THT:SW_DIP_SPSTx06_Slide_6.7x16.8mm_W7.62mm_P2.54mm_LowProfile"
		(layer "F.Cu")
		(uuid "31cb0499-bf2b-46eb-b933-da2fe4cf6dbe")
		(at 105 144)
		(descr "6x-dip-switch SPST , Slide, row spacing 7.62 mm (300 mils), body size 6.7x16.8mm (see e.g. https://www.ctscorp.com/wp-content/uploads/209-210.pdf), LowProfile")
		(tags "DIP Switch SPST Slide 7.62mm 300mil LowProfile")
		(property "Reference" "SW1"
			(at 3.81 -3.11 0)
			(layer "F.SilkS")
			(uuid "5e00067a-c794-483c-9baf-0181ad72eeb9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "SW_DIP_x06"
			(at 3.81 15.81 0)
			(layer "F.Fab")
			(uuid "678bba8e-d94a-426d-aaa3-69891bdb8b5f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Button_Switch_THT:SW_DIP_SPSTx06_Slide_6.7x16.8mm_W7.62mm_P2.54mm_LowProfile"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f9b0fdcc-ff76-4e75-ab75-58b7c872a021")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e279a04f-0b36-4930-be5b-afe3d91bd04a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c2b4cdec-7aae-44f3-8372-ebbf816b4e03")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SW?DIP?x6*")
		(path "/975c7644-dedb-4c45-8c1b-57248314d6fc")
		(sheetname "Główny")
		(sheetfile "16_ChannelPowerControlBoard.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 0.16 -2.35)
			(end 0.16 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "405f9209-c75e-4456-9332-a92382897c47")
		)
		(fp_line
			(start 0.16 -2.35)
			(end 1.543 -2.35)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "01225526-1a38-4ec7-a0d6-625b8ed5ea63")
		)
		(fp_line
			(start 0.4 -2.11)
			(end 0.4 -1.04)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "03f19fef-08fe-41d1-b004-73d068cfc154")
		)
		(fp_line
			(start 0.4 -2.11)
			(end 7.221 -2.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f8312355-7cf0-4159-a83a-2aeb15084884")
		)
		(fp_line
			(start 0.4 1.04)
			(end 0.4 1.551)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9a144e47-2d60-4344-800c-cd74dbed4565")
		)
		(fp_line
			(start 0.4 3.53)
			(end 0.4 4.091)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5e34696e-b484-4123-9a0c-63f6dded9b4b")
		)
		(fp_line
			(start 0.4 6.07)
			(end 0.4 6.631)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a0eae9c0-779a-483f-a03d-0980facdae03")
		)
		(fp_line
			(start 0.4 8.61)
			(end 0.4 9.17)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d9543259-5710-4b03-bc97-c3c9b767a05c")
		)
		(fp_line
			(start 0.4 11.15)
			(end 0.4 11.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "25127157-6667-4c8b-9c32-5fcdd0427bf6")
		)
		(fp_line
			(start 0.4 13.69)
			(end 0.4 14.811)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fb3d66dc-9f0c-4fe4-970d-c7b29eeabf45")
		)
		(fp_line
			(start 0.4 14.811)
			(end 7.221 14.811)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6b0784aa-e8d0-4dea-b532-d569d981a721")
		)
		(fp_line
			(start 2 -0.635)
			(end 2 0.635)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0e5b7ecf-af9d-4d8c-baf2-7f9d0ece31c5")
		)
		(fp_line
			(start 2 -0.515)
			(end 3.206667 -0.515)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5fa7620a-6db1-47b8-a827-cace78d26359")
		)
		(fp_line
			(start 2 -0.395)
			(end 3.206667 -0.395)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "309f2ad8-e00b-4f6f-84b8-f0645a767e23")
		)
		(fp_line
			(start 2 -0.275)
			(end 3.206667 -0.275)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4be055a1-00ef-426e-a487-9e0885cb60a2")
		)
		(fp_line
			(start 2 -0.155)
			(end 3.206667 -0.155)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e17ce317-7f19-4c26-af53-bb1522e74ac2")
		)
		(fp_line
			(start 2 -0.035)
			(end 3.206667 -0.035)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0ff812dd-ebbf-47dd-897c-07f7cd8b0414")
		)
		(fp_line
			(start 2 0.085)
			(end 3.206667 0.085)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "419a495e-5bc1-492a-9e08-f20ef5adf145")
		)
		(fp_line
			(start 2 0.205)
			(end 3.206667 0.205)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dfc789e4-7c27-4155-891a-67d148756e04")
		)
		(fp_line
			(start 2 0.325)
			(end 3.206667 0.325)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "df763508-aeee-4eae-b60f-b661bbd3b337")
		)
		(fp_line
			(start 2 0.445)
			(end 3.206667 0.445)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "63e0e604-52e1-4caa-ab0c-272bbebf1079")
		)
		(fp_line
			(start 2 0.565)
			(end 3.206667 0.565)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "881b79ee-3177-4181-aec5-6cd04b58abc2")
		)
		(fp_line
			(start 2 0.635)
			(end 5.62 0.635)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fe3f4f18-20ae-463b-baba-1463c69e2b0e")
		)
		(fp_line
			(start 2 1.905)
			(end 2 3.175)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f85efe6a-24a0-4411-969f-0761a1db9cba")
		)
		(fp_line
			(start 2 2.025)
			(end 3.206667 2.025)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6a3d4db6-0c8a-46d0-a85e-7d17e0b4e0db")
		)
		(fp_line
			(start 2 2.145)
			(end 3.206667 2.145)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6b6727b8-4a7c-4715-8f15-0fad6f597f59")
		)
		(fp_line
			(start 2 2.265)
			(end 3.206667 2.265)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f73c1c28-ba28-4087-b0bb-38cb345e9610")
		)
		(fp_line
			(start 2 2.385)
			(end 3.206667 2.385)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dddf01af-bcb4-455d-88cd-1312e7e56977")
		)
		(fp_line
			(start 2 2.505)
			(end 3.206667 2.505)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0519cb2c-a256-4e9b-bff6-acb5213b55af")
		)
		(fp_line
			(start 2 2.625)
			(end 3.206667 2.625)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "680990aa-a5a1-46ac-8c92-3c7d06168c97")
		)
		(fp_line
			(start 2 2.745)
			(end 3.206667 2.745)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bb5de587-0bd6-4420-b2d6-3cafa9b4b04e")
		)
		(fp_line
			(start 2 2.865)
			(end 3.206667 2.865)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fe304bcf-24c1-415e-8691-3225c1c4772b")
		)
		(fp_line
			(start 2 2.985)
			(end 3.206667 2.985)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2d4d5131-1aa1-4a53-8d7c-c9fc48f96111")
		)
		(fp_line
			(start 2 3.105)
			(end 3.206667 3.105)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3c2dd5d1-7a2a-4eb3-bc6f-e5be1828dcad")
		)
		(fp_line
			(start 2 3.175)
			(end 5.62 3.175)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4806d519-6a82-478f-b6e1-ec558b52ef04")
		)
		(fp_line
			(start 2 4.445)
			(end 2 5.715)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1494cb64-0c47-46e1-bbd7-2648983f1489")
		)
		(fp_line
			(start 2 4.565)
			(end 3.206667 4.565)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "53309028-cbb5-4202-ac5e-e8712c3dda38")
		)
		(fp_line
			(start 2 4.685)
			(end 3.206667 4.685)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cb95236a-4389-4b44-a731-2e57edd9e2ad")
		)
		(fp_line
			(start 2 4.805)
			(end 3.206667 4.805)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a09498a0-a0c3-4a41-84cc-656a43e1cd1e")
		)
		(fp_line
			(start 2 4.925)
			(end 3.206667 4.925)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "96c97c1b-1d85-49ec-ab9d-bada8f0192b3")
		)
		(fp_line
			(start 2 5.045)
			(end 3.206667 5.045)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9c4ff54a-0a72-4b31-b803-2e9f520f7757")
		)
		(fp_line
			(start 2 5.165)
			(end 3.206667 5.165)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "611d4537-f120-4e73-bf7d-e347db2bb8a3")
		)
		(fp_line
			(start 2 5.285)
			(end 3.206667 5.285)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bcab3f86-ba1f-46ed-833d-e08605cf6f72")
		)
		(fp_line
			(start 2 5.405)
			(end 3.206667 5.405)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b94f2dee-2c19-49d0-b6e6-d605071707b1")
		)
		(fp_line
			(start 2 5.525)
			(end 3.206667 5.525)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9791a266-0d5f-4f49-921c-1e7443f89b4f")
		)
		(fp_line
			(start 2 5.645)
			(end 3.206667 5.645)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4dd2114f-583f-425c-9822-6cb97b465e78")
		)
		(fp_line
			(start 2 5.715)
			(end 5.62 5.715)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0a44e825-f295-4234-a21f-8ac24bc88cb5")
		)
		(fp_line
			(start 2 6.985)
			(end 2 8.255)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "13700c4f-7cd0-4c70-a4c9-35da2cfcab5b")
		)
		(fp_line
			(start 2 7.105)
			(end 3.206667 7.105)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ca95c078-f00c-4113-8cbf-5354970bffcf")
		)
		(fp_line
			(start 2 7.225)
			(end 3.206667 7.225)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ed64ea3a-8649-485c-ad51-ad1ec78d8b27")
		)
		(fp_line
			(start 2 7.345)
			(end 3.206667 7.345)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c39b43ee-c4c7-40bd-8d57-b7eb5b6273a1")
		)
		(fp_line
			(start 2 7.465)
			(end 3.206667 7.465)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4b838822-8d18-4a22-8e4e-50edf587ead3")
		)
		(fp_line
			(start 2 7.585)
			(end 3.206667 7.585)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c628c4f6-c7a5-4fbd-9e29-850c61c93566")
		)
		(fp_line
			(start 2 7.705)
			(end 3.206667 7.705)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "097aaebe-e125-4b61-a23d-4ef9a53dae52")
		)
		(fp_line
			(start 2 7.825)
			(end 3.206667 7.825)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e2aa5537-c534-4075-9110-9a2896b86192")
		)
		(fp_line
			(start 2 7.945)
			(end 3.206667 7.945)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0dcdf9d4-82ca-47a5-8d5e-91e9d6f451ff")
		)
		(fp_line
			(start 2 8.065)
			(end 3.206667 8.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8715bba0-edfd-480b-9493-a4e2e29648ee")
		)
		(fp_line
			(start 2 8.185)
			(end 3.206667 8.185)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1a45047d-55ea-44e2-a437-ddb8c0d932c5")
		)
		(fp_line
			(start 2 8.255)
			(end 5.62 8.255)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cbbcb4e2-f7b7-4892-b7fd-43164847d27d")
		)
		(fp_line
			(start 2 9.525)
			(end 2 10.795)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a0328f17-a338-495f-8e3b-4291bf179341")
		)
		(fp_line
			(start 2 9.645)
			(end 3.206667 9.645)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7dc1577b-9ddd-466c-8364-1c7bf2414169")
		)
		(fp_line
			(start 2 9.765)
			(end 3.206667 9.765)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d199af75-5779-423c-8223-a76eb82cb5e0")
		)
		(fp_line
			(start 2 9.885)
			(end 3.206667 9.885)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b2d93fc9-71a7-4294-92a0-ef3622e939c6")
		)
		(fp_line
			(start 2 10.005)
			(end 3.206667 10.005)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d8f536da-ac4f-4390-9561-e96038195080")
		)
		(fp_line
			(start 2 10.125)
			(end 3.206667 10.125)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f420faef-da9f-47d9-8a75-12889d5f6b80")
		)
		(fp_line
			(start 2 10.245)
			(end 3.206667 10.245)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aee8a0d4-f15f-47da-92b0-a37fab573b77")
		)
		(fp_line
			(start 2 10.365)
			(end 3.206667 10.365)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f30a1f96-bdaf-492b-9e0c-0280601d8879")
		)
		(fp_line
			(start 2 10.485)
			(end 3.206667 10.485)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "14f4d4ad-effa-4b72-854c-229edf25699c")
		)
		(fp_line
			(start 2 10.605)
			(end 3.206667 10.605)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fa7409b1-4e89-45d3-9a99-ab3c29e465ac")
		)
		(fp_line
			(start 2 10.725)
			(end 3.206667 10.725)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "09fd977a-f123-4955-a2b3-9a8179e197d6")
		)
		(fp_line
			(start 2 10.795)
			(end 5.62 10.795)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aeb02b50-1791-476b-8127-a72c12c81160")
		)
		(fp_line
			(start 2 12.065)
			(end 2 13.335)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "300849dc-d0a4-41da-9d22-6c9e8160b373")
		)
		(fp_line
			(start 2 12.185)
			(end 3.206667 12.185)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7ef5b4d3-ce79-451e-9fcf-dce76756a566")
		)
		(fp_line
			(start 2 12.305)
			(end 3.206667 12.305)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5f0592db-d79c-44af-8826-a5d7dac60ecd")
		)
		(fp_line
			(start 2 12.425)
			(end 3.206667 12.425)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "063c0698-bb52-46b5-ac0d-c389090db9d9")
		)
		(fp_line
			(start 2 12.545)
			(end 3.206667 12.545)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3f24a862-705d-4add-bc15-7d432cd73927")
		)
		(fp_line
			(start 2 12.665)
			(end 3.206667 12.665)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7fe054a1-8e7f-45eb-bc66-1befe18d12b6")
		)
		(fp_line
			(start 2 12.785)
			(end 3.206667 12.785)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2a8ae8a0-f8f0-4151-bc54-1397d6f3a541")
		)
		(fp_line
			(start 2 12.905)
			(end 3.206667 12.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d3758883-7038-4049-abb3-7de4691d244d")
		)
		(fp_line
			(start 2 13.025)
			(end 3.206667 13.025)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3373642f-16d5-45a9-ab79-b6267e252d4d")
		)
		(fp_line
			(start 2 13.145)
			(end 3.206667 13.145)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2d8d6e69-1c9f-4473-8eb7-4a1200c3fae8")
		)
		(fp_line
			(start 2 13.265)
			(end 3.206667 13.265)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1d6df56f-e6ea-4c38-8574-a11cf7795a43")
		)
		(fp_line
			(start 2 13.335)
			(end 5.62 13.335)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "50543b9e-4ea3-48f0-a897-db9a1385f306")
		)
		(fp_line
			(start 3.206667 -0.635)
			(end 3.206667 0.635)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "95feb61c-83ba-4d0b-b165-cb683c8b6e8f")
		)
		(fp_line
			(start 3.206667 1.905)
			(end 3.206667 3.175)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9290b344-72c8-43fb-8052-9a266358eee7")
		)
		(fp_line
			(start 3.206667 4.445)
			(end 3.206667 5.715)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "231e9089-ac3d-4940-af3c-da740ed4fcd5")
		)
		(fp_line
			(start 3.206667 6.985)
			(end 3.206667 8.255)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8b66fdde-7ad2-437d-bcfa-314b3e2f9418")
		)
		(fp_line
			(start 3.206667 9.525)
			(end 3.206667 10.795)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1202afb4-ed3c-4657-88d2-e2718249975f")
		)
		(fp_line
			(start 3.206667 12.065)
			(end 3.206667 13.335)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4e12a2c2-b7e4-45cc-81e9-2ec72a5370ce")
		)
		(fp_line
			(start 5.62 -0.635)
			(end 2 -0.635)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e1bff4a2-79ec-4c6d-ade2-637c4615c976")
		)
		(fp_line
			(start 5.62 0.635)
			(end 5.62 -0.635)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "73f8f029-b9fa-4e63-aa25-ec430b112b79")
		)
		(fp_line
			(start 5.62 1.905)
			(end 2 1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "23796799-694b-4654-a803-8484c976b983")
		)
		(fp_line
			(start 5.62 3.175)
			(end 5.62 1.905)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "095f36b2-c9a3-4ed6-aaff-c8d69d2bfe7a")
		)
		(fp_line
			(start 5.62 4.445)
			(end 2 4.445)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "110337db-40be-4d55-8ecd-64eefe940e24")
		)
		(fp_line
			(start 5.62 5.715)
			(end 5.62 4.445)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6f9cb802-0db0-48c5-af37-61bbd50e2128")
		)
		(fp_line
			(start 5.62 6.985)
			(end 2 6.985)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "996de047-9227-476f-a172-acb3de07bc52")
		)
		(fp_line
			(start 5.62 8.255)
			(end 5.62 6.985)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ed548e98-3930-4299-b653-ae95802cd2e3")
		)
		(fp_line
			(start 5.62 9.525)
			(end 2 9.525)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ba5be949-ec81-4c63-8a38-026cea7c8cc7")
		)
		(fp_line
			(start 5.62 10.795)
			(end 5.62 9.525)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "99805cb1-4058-4c2f-a67d-b7ebae6cf47b")
		)
		(fp_line
			(start 5.62 12.065)
			(end 2 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "78ff10eb-d20b-4394-aa07-95b79f2d97d7")
		)
		(fp_line
			(start 5.62 13.335)
			(end 5.62 12.065)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a159eb64-3cc7-42e8-8a63-fd02e2cb1053")
		)
		(fp_line
			(start 7.221 -2.11)
			(end 7.221 -0.99)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "11d6e48f-95ea-440d-844f-0a292ff6f05d")
		)
		(fp_line
			(start 7.221 0.99)
			(end 7.221 1.551)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "62f8055a-1514-4288-ab40-f9900c90158e")
		)
		(fp_line
			(start 7.221 3.53)
			(end 7.221 4.091)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c628618c-4ab7-4692-88c7-6bb3d9507d25")
		)
		(fp_line
			(start 7.221 6.07)
			(end 7.221 6.631)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a31760fc-7115-46c1-9b33-3a811412e3cc")
		)
		(fp_line
			(start 7.221 8.61)
			(end 7.221 9.17)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "62baca39-98ca-49d9-843d-3d034eb09efb")
		)
		(fp_line
			(start 7.221 11.15)
			(end 7.221 11.71)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fb6afa79-8933-4313-8f4c-d9dc279512c3")
		)
		(fp_line
			(start 7.221 13.69)
			(end 7.221 14.811)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e397d546-9af7-4292-aa5a-7ba8005ee149")
		)
		(fp_line
			(start -1.1 -2.4)
			(end -1.1 15.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "59eb4bfb-3937-4b35-a127-5e3557e142fb")
		)
		(fp_line
			(start -1.1 15.1)
			(end 8.7 15.1)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3b9be977-c823-4046-8801-a3b597fc7713")
		)
		(fp_line
			(start 8.7 -2.4)
			(end -1.1 -2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f20655aa-cf43-4da8-af8c-08a53e9c48d6")
		)
		(fp_line
			(start 8.7 15.1)
			(end 8.7 -2.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "38e116c2-80e3-43bc-b9f5-c8884d4584f6")
		)
		(fp_line
			(start 0.46 -1.05)
			(end 1.46 -2.05)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "533ae23e-ea3e-4b77-84cb-1fdc4b759ed0")
		)
		(fp_line
			(start 0.46 14.75)
			(end 0.46 -1.05)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9f678f9d-4994-49b1-b65e-ebc467caead5")
		)
		(fp_line
			(start 1.46 -2.05)
			(end 7.16 -2.05)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "90496b06-ce66-4fee-8b59-4b3b0f8bcc6a")
		)
		(fp_line
			(start 2 -0.635)
			(end 2 0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9033c31d-069a-4cc3-8377-2e7389798790")
		)
		(fp_line
			(start 2 -0.535)
			(end 3.206667 -0.535)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "83798a94-bdc7-4b02-8859-64efa95ddfcf")
		)
		(fp_line
			(start 2 -0.435)
			(end 3.206667 -0.435)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cd2b285d-53df-48d9-ac0f-54c7921610ec")
		)
		(fp_line
			(start 2 -0.335)
			(end 3.206667 -0.335)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4ee3cd08-6fdc-418e-ad2c-d2c13332231c")
		)
		(fp_line
			(start 2 -0.235)
			(end 3.206667 -0.235)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "37b6066e-4b84-4cf1-ac64-3910eb61a932")
		)
		(fp_line
			(start 2 -0.135)
			(end 3.206667 -0.135)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "086ad682-87aa-4e8c-b415-554c746b210c")
		)
		(fp_line
			(start 2 -0.035)
			(end 3.206667 -0.035)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "153cb9b9-55e0-4991-996b-f5474d69a525")
		)
		(fp_line
			(start 2 0.065)
			(end 3.206667 0.065)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3871ca7f-c41b-4aca-819a-39465a717df3")
		)
		(fp_line
			(start 2 0.165)
			(end 3.206667 0.165)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b3b9e4eb-96c0-46dc-85e6-f9242bddb21a")
		)
		(fp_line
			(start 2 0.265)
			(end 3.206667 0.265)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bf39836c-e3c5-4075-be1f-101253f14529")
		)
		(fp_line
			(start 2 0.365)
			(end 3.206667 0.365)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d1e75c85-d732-4858-bea1-58ecf9a36ec4")
		)
		(fp_line
			(start 2 0.465)
			(end 3.206667 0.465)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "69ef7d44-2ac8-41b9-ae90-c3939687f3d1")
		)
		(fp_line
			(start 2 0.565)
			(end 3.206667 0.565)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "06f16e6f-f2da-4a6d-8b0d-d7788799dcc0")
		)
		(fp_line
			(start 2 0.635)
			(end 5.62 0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d593cd36-f52a-4769-85d8-1d8026cd12e7")
		)
		(fp_line
			(start 2 1.905)
			(end 2 3.175)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a4f415cb-9219-4d5c-a42a-5a187ef6ea31")
		)
		(fp_line
			(start 2 2.005)
			(end 3.206667 2.005)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a2daf3a8-6efa-40d1-a712-cd50387643ad")
		)
		(fp_line
			(start 2 2.105)
			(end 3.206667 2.105)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1573f7ee-9b90-4b71-9f19-5e661806ffc4")
		)
		(fp_line
			(start 2 2.205)
			(end 3.206667 2.205)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2c6e9da2-e37c-4200-93ce-a585960833c5")
		)
		(fp_line
			(start 2 2.305)
			(end 3.206667 2.305)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0451804f-9707-40ff-b4d2-f787d68aba1b")
		)
		(fp_line
			(start 2 2.405)
			(end 3.206667 2.405)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b7d30ec1-ccc8-4133-8b15-d006aef7ba82")
		)
		(fp_line
			(start 2 2.505)
			(end 3.206667 2.505)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b1644aba-cbbc-4ae6-a42a-089fc1569876")
		)
		(fp_line
			(start 2 2.605)
			(end 3.206667 2.605)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0429e3d7-c95a-41ba-ae04-bd59b9357e93")
		)
		(fp_line
			(start 2 2.705)
			(end 3.206667 2.705)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "014ffbb2-c9fb-4063-87c9-9becdffd307d")
		)
		(fp_line
			(start 2 2.805)
			(end 3.206667 2.805)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ac71e7b1-a8d8-4232-b569-1674756f3956")
		)
		(fp_line
			(start 2 2.905)
			(end 3.206667 2.905)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "063a9c59-8b3b-4bc1-9ca9-2fa8fcf402d9")
		)
		(fp_line
			(start 2 3.005)
			(end 3.206667 3.005)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b1f89fc1-ccca-4b47-b96e-b246d2b7f5e1")
		)
		(fp_line
			(start 2 3.105)
			(end 3.206667 3.105)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e39f7c9e-cac0-4aa0-9570-4ffc9642d916")
		)
		(fp_line
			(start 2 3.175)
			(end 5.62 3.175)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "947b8b24-8f14-467b-bb86-ff2ce99ad07c")
		)
		(fp_line
			(start 2 4.445)
			(end 2 5.715)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c6abebec-5675-4beb-90b1-6caba0eaa7a4")
		)
		(fp_line
			(start 2 4.545)
			(end 3.206667 4.545)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "548f44d0-ca14-4cd2-befd-f2b9351f4639")
		)
		(fp_line
			(start 2 4.645)
			(end 3.206667 4.645)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "30c4663d-dec2-4149-b947-42f04e4dfaa3")
		)
		(fp_line
			(start 2 4.745)
			(end 3.206667 4.745)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f27c7c49-5ebd-4e16-a928-634b58011eab")
		)
		(fp_line
			(start 2 4.845)
			(end 3.206667 4.845)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b781bc05-68d1-47da-92f5-9a45a1f09af2")
		)
		(fp_line
			(start 2 4.945)
			(end 3.206667 4.945)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bfa99066-b423-4dc0-9e6c-ceaa9f783bf0")
		)
		(fp_line
			(start 2 5.045)
			(end 3.206667 5.045)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "41ea113d-c7ae-4c73-8fe3-01fdebe02d81")
		)
		(fp_line
			(start 2 5.145)
			(end 3.206667 5.145)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b97998ba-a6d6-464f-b42b-96db13086453")
		)
		(fp_line
			(start 2 5.245)
			(end 3.206667 5.245)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b32fcabe-ca15-4a31-b1b8-e3edfb2175ae")
		)
		(fp_line
			(start 2 5.345)
			(end 3.206667 5.345)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b6c5a0c0-4c83-43b1-b494-309915274c90")
		)
		(fp_line
			(start 2 5.445)
			(end 3.206667 5.445)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c4d769c4-8c02-4699-a41f-58a737d5fba6")
		)
		(fp_line
			(start 2 5.545)
			(end 3.206667 5.545)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "450cd587-8994-443f-86d5-02d39275f022")
		)
		(fp_line
			(start 2 5.645)
			(end 3.206667 5.645)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "75bd9b33-c774-425c-ac25-be2d3ffa9745")
		)
		(fp_line
			(start 2 5.715)
			(end 5.62 5.715)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "424b68c3-f067-47f5-8d45-af56ff2fcdc0")
		)
		(fp_line
			(start 2 6.985)
			(end 2 8.255)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2168be71-38fb-486c-9e5c-d76183c70642")
		)
		(fp_line
			(start 2 7.085)
			(end 3.206667 7.085)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9b36480e-d442-4a44-99c3-cf8883c6a0b9")
		)
		(fp_line
			(start 2 7.185)
			(end 3.206667 7.185)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5c6e1b08-57ba-4e25-a13a-34cf7f15bba6")
		)
		(fp_line
			(start 2 7.285)
			(end 3.206667 7.285)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "678e8f7d-40b4-4fa7-b603-d4f39b89a90c")
		)
		(fp_line
			(start 2 7.385)
			(end 3.206667 7.385)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "961f23f2-10dc-4db3-a0d7-3f1ed42c2b99")
		)
		(fp_line
			(start 2 7.485)
			(end 3.206667 7.485)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b280f1bd-06b4-4c5c-8634-ee84e2c6c6df")
		)
		(fp_line
			(start 2 7.585)
			(end 3.206667 7.585)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "df11d5ef-b854-4fd0-bee0-074bb8147816")
		)
		(fp_line
			(start 2 7.685)
			(end 3.206667 7.685)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c3b19219-1441-4cce-b504-43c4a7aa0c93")
		)
		(fp_line
			(start 2 7.785)
			(end 3.206667 7.785)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e0d75f4a-8962-41ce-8a96-42f077013d02")
		)
		(fp_line
			(start 2 7.885)
			(end 3.206667 7.885)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "da0480fc-f6a9-4599-8850-4ba77b79320a")
		)
		(fp_line
			(start 2 7.985)
			(end 3.206667 7.985)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fd55e1ed-339c-43d7-b2b2-4ddeded8928d")
		)
		(fp_line
			(start 2 8.085)
			(end 3.206667 8.085)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9b28b2ed-1e85-4bf1-a196-47124fef693d")
		)
		(fp_line
			(start 2 8.185)
			(end 3.206667 8.185)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2fe811d9-fc4e-4cdf-82fc-0ee358fdfabc")
		)
		(fp_line
			(start 2 8.255)
			(end 5.62 8.255)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b224c941-5b41-44eb-8e42-634efa9c59c2")
		)
		(fp_line
			(start 2 9.525)
			(end 2 10.795)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d9798288-362a-410f-b3b1-9b03cc2d7456")
		)
		(fp_line
			(start 2 9.625)
			(end 3.206667 9.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a83816a8-69ae-43c8-a625-f6e972d51fe9")
		)
		(fp_line
			(start 2 9.725)
			(end 3.206667 9.725)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1febc3d3-1232-4356-ae77-f63755fd1b7d")
		)
		(fp_line
			(start 2 9.825)
			(end 3.206667 9.825)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6473d371-cd1e-41e4-bdf1-51c5e3bc8f4a")
		)
		(fp_line
			(start 2 9.925)
			(end 3.206667 9.925)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d3e2340e-6b77-4004-a622-dcb6333f3423")
		)
		(fp_line
			(start 2 10.025)
			(end 3.206667 10.025)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8f892319-a371-423e-946d-380a72110d84")
		)
		(fp_line
			(start 2 10.125)
			(end 3.206667 10.125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "783b2114-57d8-4689-b837-613b8ac93d87")
		)
		(fp_line
			(start 2 10.225)
			(end 3.206667 10.225)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d30bc620-fba1-4120-9b01-44ffcef86b7d")
		)
		(fp_line
			(start 2 10.325)
			(end 3.206667 10.325)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "422c78db-6414-4a14-91e2-0297e9d1657a")
		)
		(fp_line
			(start 2 10.425)
			(end 3.206667 10.425)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "46fcf5ff-d106-4bc1-8a08-746899f8a8b1")
		)
		(fp_line
			(start 2 10.525)
			(end 3.206667 10.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0a2b63ec-f336-4ad4-8ea1-f2698fced1a9")
		)
		(fp_line
			(start 2 10.625)
			(end 3.206667 10.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9a85e0d0-b176-4250-a5be-9f052b8bf1ed")
		)
		(fp_line
			(start 2 10.725)
			(end 3.206667 10.725)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e4b80444-2fd9-4bf6-b69d-6dbe061cf50f")
		)
		(fp_line
			(start 2 10.795)
			(end 5.62 10.795)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9cf54396-0bc6-476b-aadf-e542e3b5174d")
		)
		(fp_line
			(start 2 12.065)
			(end 2 13.335)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3d0eedb0-929f-4ade-be4d-ee670897ad17")
		)
		(fp_line
			(start 2 12.165)
			(end 3.206667 12.165)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f8fdb6ba-1cac-4140-adde-99ec3b083a87")
		)
		(fp_line
			(start 2 12.265)
			(end 3.206667 12.265)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d6f07202-7f21-42e4-b7fa-111c13c76333")
		)
		(fp_line
			(start 2 12.365)
			(end 3.206667 12.365)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "31a291d7-3534-45c6-bb87-e065a396258c")
		)
		(fp_line
			(start 2 12.465)
			(end 3.206667 12.465)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "36c787af-1578-44df-8086-fe0b786d07fb")
		)
		(fp_line
			(start 2 12.565)
			(end 3.206667 12.565)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e5f05974-3cb5-42ea-8a92-a7aa33f071a8")
		)
		(fp_line
			(start 2 12.665)
			(end 3.206667 12.665)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ca88d3c9-bedd-49a5-bded-e1133ca3f90f")
		)
		(fp_line
			(start 2 12.765)
			(end 3.206667 12.765)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a5665743-ff54-43b8-935d-d02a26765497")
		)
		(fp_line
			(start 2 12.865)
			(end 3.206667 12.865)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bf67a2a6-557c-41b4-9446-4d0607b9bf8c")
		)
		(fp_line
			(start 2 12.965)
			(end 3.206667 12.965)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1eab8311-1860-4b9c-9361-d7a2fe75136f")
		)
		(fp_line
			(start 2 13.065)
			(end 3.206667 13.065)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "676a4094-db0a-4aba-9ca0-31df98a5a2d9")
		)
		(fp_line
			(start 2 13.165)
			(end 3.206667 13.165)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "56f12f97-ee39-4859-a337-31cb62e7ed81")
		)
		(fp_line
			(start 2 13.265)
			(end 3.206667 13.265)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dee1675f-4226-4457-9cef-97c6b4d704c2")
		)
		(fp_line
			(start 2 13.335)
			(end 5.62 13.335)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ab2a86b6-1e87-41e1-b941-eefbcb7845ae")
		)
		(fp_line
			(start 3.206667 -0.635)
			(end 3.206667 0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6277f115-9b51-44db-b905-ace095ceb30e")
		)
		(fp_line
			(start 3.206667 1.905)
			(end 3.206667 3.175)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "77e1d948-8bdc-426e-9bf2-76e21f6444b1")
		)
		(fp_line
			(start 3.206667 4.445)
			(end 3.206667 5.715)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b986a190-c156-4033-af46-fb95727f5048")
		)
		(fp_line
			(start 3.206667 6.985)
			(end 3.206667 8.255)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a05c538b-baed-4b67-b128-2c2f4fd1b1dd")
		)
		(fp_line
			(start 3.206667 9.525)
			(end 3.206667 10.795)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e5163a3e-32b2-4a0e-a96a-e832fa49ebaf")
		)
		(fp_line
			(start 3.206667 12.065)
			(end 3.206667 13.335)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2cf5632d-7714-499e-ac06-647f0081d24d")
		)
		(fp_line
			(start 5.62 -0.635)
			(end 2 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "30da0cef-ae3d-4110-a130-e8a5c2147df6")
		)
		(fp_line
			(start 5.62 0.635)
			(end 5.62 -0.635)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dea46de2-61b3-4107-ba43-43402da3eb14")
		)
		(fp_line
			(start 5.62 1.905)
			(end 2 1.905)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "742504f1-b896-45a8-897d-c872f8d20a7c")
		)
		(fp_line
			(start 5.62 3.175)
			(end 5.62 1.905)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cc0f74aa-9374-4cbe-97fd-a28644a0623d")
		)
		(fp_line
			(start 5.62 4.445)
			(end 2 4.445)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c09c39f0-a063-4d9a-a665-f18ec93dd58f")
		)
		(fp_line
			(start 5.62 5.715)
			(end 5.62 4.445)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9a4ee56c-49e7-4e1f-91d3-42bee0b16beb")
		)
		(fp_line
			(start 5.62 6.985)
			(end 2 6.985)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bc52f923-43e8-435c-945b-95de6bfddd51")
		)
		(fp_line
			(start 5.62 8.255)
			(end 5.62 6.985)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3c22d360-b755-471e-a3d6-a3ad2dd78482")
		)
		(fp_line
			(start 5.62 9.525)
			(end 2 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0c411139-6da0-4bed-8c20-319819e127f3")
		)
		(fp_line
			(start 5.62 10.795)
			(end 5.62 9.525)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "94dae302-264c-4e2f-b002-d35f9b45c346")
		)
		(fp_line
			(start 5.62 12.065)
			(end 2 12.065)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8f6372f2-9b36-42e9-9cbf-a583d7a56309")
		)
		(fp_line
			(start 5.62 13.335)
			(end 5.62 12.065)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8535fba2-fa0e-415a-9f87-ae79ea00fb0e")
		)
		(fp_line
			(start 7.16 -2.05)
			(end 7.16 14.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6c5e4460-b27b-4030-af01-1a6f324a426b")
		)
		(fp_line
			(start 7.16 14.75)
			(end 0.46 14.75)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b3e3ad60-40a5-42f7-ad9c-0997aa06af5e")
		)
		(fp_text user "${REFERENCE}"
			(at 6.39 6.35 90)
			(layer "F.Fab")
			(uuid "066e14eb-6204-4d56-8d7f-96f5505b2a00")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(fp_text user "on"
			(at 4.485 -1.3425 0)
			(layer "F.Fab")
			(uuid "a24afab8-6b96-47fd-8158-ea069d4e092b")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 176 "unconnected-(SW1-Pad1)")
			(pintype "passive")
			(uuid "ddce54f4-baf4-4b18-ae14-c13e0de03804")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 175 "unconnected-(SW1-Pad2)")
			(pintype "passive")
			(uuid "c7ed2ecd-fe69-4d08-8379-ffaace14ab7d")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 173 "unconnected-(SW1-Pad3)")
			(pintype "passive")
			(uuid "8bf82fa6-ae1f-46c1-8054-e0cf049aa842")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 171 "unconnected-(SW1-Pad4)")
			(pintype "passive")
			(uuid "0c2c8453-f1d8-4aaa-a3cc-f82c3178a183")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 174 "unconnected-(SW1-Pad5)")
			(pintype "passive")
			(uuid "c5bc8616-509d-4aaf-824b-285d3ca3c999")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 172 "unconnected-(SW1-Pad6)")
			(pintype "passive")
			(uuid "5af0df69-b53e-490e-ab97-a30eb883a6c7")
		)
		(pad "7" thru_hole oval
			(at 7.62 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 108 "Net-(SW1-Pad10)")
			(pintype "passive")
			(uuid "c4ae8b35-4135-415e-961a-eae96dc63738")
		)
		(pad "8" thru_hole oval
			(at 7.62 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 108 "Net-(SW1-Pad10)")
			(pintype "passive")
			(uuid "f7c25a3f-2381-4cb9-bad2-444a03930a07")
		)
		(pad "9" thru_hole oval
			(at 7.62 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 108 "Net-(SW1-Pad10)")
			(pintype "passive")
			(uuid "69dab8e5-4f1d-4310-8be3-74f01ecad7ac")
		)
		(pad "10" thru_hole oval
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 108 "Net-(SW1-Pad10)")
			(pintype "passive")
			(uuid "f35fbfa1-208e-40ac-8b9d-ad97910505d9")
		)
		(pad "11" thru_hole oval
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 108 "Net-(SW1-Pad10)")
			(pintype "passive")
			(uuid "605ccce0-ba9e-4a3f-958a-77941e1f7514")
		)
		(pad "12" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 108 "Net-(SW1-Pad10)")
			(pintype "passive")
			(uuid "907eaf8b-36fe-443b-ab03-30b42647c935")
		)
		(model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_DIP_SPSTx06_Slide_6.7x16.8mm_W7.62mm_P2.54mm_LowProfile.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "33ee1de5-d217-4ce0-b42b-be4fefb6b75e")
		(at 48.080358 34.84 180)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q4"
			(at 0 -2.4 0)
			(layer "F.SilkS")
			(uuid "c4f59246-9070-48c8-b18b-5df2977eae02")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BC818"
			(at 0 2.4 0)
			(layer "F.Fab")
			(uuid "c1c3fc72-ec7e-47d8-b08e-15c197f8442d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "34bdebbb-cc06-40f9-b823-1cb18ce9de01")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC818-D.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "a5e6bae8-6712-42f7-afad-210003e29da4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "309124cf-45f6-41d5-875b-9e24fa712a66")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/98cc9bb7-a6bb-4cad-bced-cd34a966891d/00e550ea-8431-483d-ac3c-b4a719825546")
		(sheetname "Triac Circuit1")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 1.56)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d47d7e2a-371f-431f-94c7-562229491f0f")
		)
		(fp_line
			(start 0 1.56)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "175eee13-c8ff-423e-9a7d-f672146947c4")
		)
		(fp_line
			(start 0 -1.56)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0cab2dbf-a382-4e78-934b-5ef9bbf824de")
		)
		(fp_line
			(start 0 -1.56)
			(end -1.675 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d8a6a566-b69c-4e0e-bbb0-593c003d7a78")
		)
		(fp_line
			(start 1.92 1.7)
			(end 1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "910e007b-dc16-4e5b-97a2-6f7cd74c6665")
		)
		(fp_line
			(start 1.92 -1.7)
			(end -1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "709bec8a-5032-498c-a4f5-f562193ad4a2")
		)
		(fp_line
			(start -1.92 1.7)
			(end 1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3546700a-b3ad-4c4f-87df-391e963d4fc0")
		)
		(fp_line
			(start -1.92 -1.7)
			(end -1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "90f6e70c-6bf1-482b-a482-d6ec7e1fe0e1")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b16646bb-1439-4308-953f-e1a7ed54162f")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2149afb0-93af-4466-9855-38073e9ebbfb")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4bd83d60-73f9-4984-a932-11b6c57a0ab3")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e25a253f-02cd-4122-bb8a-396dc3c34ae3")
		)
		(fp_line
			(start -0.65 -1.125)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2efef2c8-652a-49c7-80fb-19c0661cb691")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "59c64717-8e8d-4162-afbe-a7941805d8a2")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 46 "Net-(Q4-B)")
			(pinfunction "B")
			(pintype "input")
			(uuid "3eb8139e-3603-48e3-bb67-8ebc7b8161ad")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "GND")
			(pinfunction "E")
			(pintype "passive")
			(uuid "4b7377b2-758d-4b07-ad77-597afe4e338e")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 50 "Net-(Q4-C)")
			(pinfunction "C")
			(pintype "passive")
			(uuid "5392343d-4207-4940-869e-5512d49b9052")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Crystal:Crystal_HC18-U_Vertical"
		(layer "F.Cu")
		(uuid "349f366b-39b7-4e90-83b6-8426fb5232d0")
		(at 82.2 162.25 90)
		(descr "Crystal THT HC-18/U, http://5hertz.com/pdfs/04404_D.pdf")
		(tags "THT crystalHC-18/U")
		(property "Reference" "Y1"
			(at 2.45 -3.525 90)
			(layer "F.SilkS")
			(uuid "7e8eba53-a797-45b4-b2cb-285f4b4d52d3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4, 40 or 20MHz"
			(at 2.45 3.525 90)
			(layer "F.Fab")
			(uuid "afe190a4-65cb-491a-acb6-df21ef3628d4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Crystal:Crystal_HC18-U_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d7d6ad22-5858-4fd8-b440-0f441381c99f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ea8f064d-ea7e-473a-b761-1503f983406f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Two pin crystal, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ef7783ff-f8c1-4b89-81ef-15e7b1ab6dd6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Crystal*")
		(path "/e08767e2-0992-4432-86db-08688f02df69")
		(sheetname "Główny")
		(sheetfile "16_ChannelPowerControlBoard.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -0.675 -2.525)
			(end 5.575 -2.525)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "99b8adf9-7700-4e0e-8f6f-0e60678f5fd1")
		)
		(fp_line
			(start -0.675 2.525)
			(end 5.575 2.525)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "055b38c4-b2fb-4048-9bf8-745529e04610")
		)
		(fp_arc
			(start 5.575 -2.525)
			(mid 8.1 0)
			(end 5.575 2.525)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dc8a9160-504f-47b8-adda-0d947eca0f18")
		)
		(fp_arc
			(start -0.675 2.525)
			(mid -3.2 0)
			(end -0.675 -2.525)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c1df4d17-15a0-4a59-8037-c5616005cd2c")
		)
		(fp_line
			(start 8.4 -2.8)
			(end -3.5 -2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4374439c-a77b-4c1d-b94d-4bbafedd02ef")
		)
		(fp_line
			(start -3.5 -2.8)
			(end -3.5 2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "30d02281-ce3f-42a3-9e04-ef475c364c95")
		)
		(fp_line
			(start 8.4 2.8)
			(end 8.4 -2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "27a15d34-17ba-403b-9539-631eaa677751")
		)
		(fp_line
			(start -3.5 2.8)
			(end 8.4 2.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "28de0116-1fac-42ba-bc38-e993dc0ae169")
		)
		(fp_line
			(start -0.675 -2.325)
			(end 5.575 -2.325)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b07a8ec0-4c47-4a49-9389-5541f7d4076d")
		)
		(fp_line
			(start -0.55 -2)
			(end 5.45 -2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8461b06b-2922-4c72-b4bc-b6deeb3b116f")
		)
		(fp_line
			(start -0.55 2)
			(end 5.45 2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fad38d0b-053c-4a43-ba50-5e296ef40513")
		)
		(fp_line
			(start -0.675 2.325)
			(end 5.575 2.325)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5094a961-c31c-4454-8d6d-23bae449f80b")
		)
		(fp_arc
			(start 5.575 -2.325)
			(mid 7.9 0)
			(end 5.575 2.325)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bbc88274-8eeb-4921-a471-88ae85312414")
		)
		(fp_arc
			(start 5.45 -2)
			(mid 7.45 0)
			(end 5.45 2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2ad08e58-bd20-49ea-8e1b-e2c2788d0574")
		)
		(fp_arc
			(start -0.55 2)
			(mid -2.55 0)
			(end -0.55 -2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6388e219-389b-4759-88ef-63df1cbf15aa")
		)
		(fp_arc
			(start -0.675 2.325)
			(mid -3 0)
			(end -0.675 -2.325)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "43db8924-21bd-43e6-b313-67900561fad1")
		)
		(fp_text user "${REFERENCE}"
			(at 2.45 0 90)
			(layer "F.Fab")
			(uuid "b3751165-89e0-4e48-944e-8cb065f45c0b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 165 "Net-(U19-OSC2)")
			(pinfunction "1")
			(pintype "passive")
			(uuid "3a9a3439-1510-408d-ae04-0f90f5b717c5")
		)
		(pad "2" thru_hole circle
			(at 4.9 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 166 "Net-(U19-OSC1)")
			(pinfunction "2")
			(pintype "passive")
			(uuid "c454bc9c-819f-4a96-b987-8957b9c6ef7b")
		)
		(model "${KICAD8_3DMODEL_DIR}/Crystal.3dshapes/Crystal_HC18-U_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-6_W7.62mm"
		(layer "F.Cu")
		(uuid "3532e872-7dac-4174-8d3b-51b8bddc9503")
		(at 57.142855 133.155)
		(descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U17"
			(at 3.599999 -2.33 180)
			(layer "F.SilkS")
			(uuid "61c31c69-ae3e-4f35-a2e8-18ea4ac32dc7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MOC3021M"
			(at 3.81 7.409999 180)
			(layer "F.Fab")
			(uuid "6967fc95-e7dd-4b80-a43f-7284451f12cf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "98e99173-2782-4a61-9a7e-f57bc34ad9b7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3023M-D.PDF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ea042477-861a-45f5-bf50-5769cfdbf877")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b90279fc-1628-45e1-8ac1-4b99dcbc6c7f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*")
		(path "/4b0c0d83-8522-4ffe-8435-2c6bf5567543/0262e914-5435-478f-be04-ece49b8102cf")
		(sheetname "Triac Circuit15")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "562166b5-be7e-4873-8732-377351ea0960")
		)
		(fp_line
			(start 1.16 6.41)
			(end 6.46 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d68d3ccb-e3de-4fc6-a7eb-d260f891f3d9")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ee563469-bcfb-4236-95d9-1f374f8b8de1")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "97f20c1f-3789-42d5-a58c-7672436463cb")
		)
		(fp_line
			(start 6.46 6.41)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "84a4145f-0b98-4799-9c6d-64e9c323e201")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1ad368a1-26c5-4a9d-b6aa-79088a81f693")
		)
		(fp_line
			(start -1.1 -1.55)
			(end -1.1 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f0f43fe9-734e-4f50-8374-e8c436a3531f")
		)
		(fp_line
			(start -1.1 6.6)
			(end 8.7 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c1fdd69e-a74c-4fd2-9fcf-80e314dbde55")
		)
		(fp_line
			(start 8.7 -1.55)
			(end -1.1 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f60b8f17-7040-49b0-8ad2-6ad8c33fcdb6")
		)
		(fp_line
			(start 8.7 6.6)
			(end 8.7 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e6cf39c6-da3b-4c59-89dd-176c1b75724b")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2cd275ee-f3cd-4dec-bf50-962565faf0f7")
		)
		(fp_line
			(start 0.635 6.35)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "461732be-b0eb-4378-947e-095b1137a9e6")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "08f557cd-d8d9-43a0-b6e1-a6e7121a32ea")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2bbc54a7-9bb2-4ae1-9f8d-a62c96f1ff7e")
		)
		(fp_line
			(start 6.985 6.35)
			(end 0.635 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c78f1bd2-2e8f-4eae-a53d-c8264bad63de")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.539999 180)
			(layer "F.Fab")
			(uuid "7a832bd6-dd62-4587-b1b5-934849f92269")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 128 "Net-(R47-Pad1)")
			(pintype "passive")
			(uuid "5c0f8e69-0ecd-4ea0-b021-b91c50c51e64")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 159 "Net-(Q32-C)")
			(pintype "passive")
			(uuid "25b98849-4a7b-49ea-8d28-7f61ba196573")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 123 "unconnected-(U17-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "72331644-5760-416b-9b7c-d8f3f484cfe5")
		)
		(pad "4" thru_hole oval
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 157 "Net-(Q31-G)")
			(pintype "passive")
			(uuid "1bda8335-4931-4cd2-afba-c0d359e8cab1")
		)
		(pad "5" thru_hole oval
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 124 "unconnected-(U17-NC-Pad5)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "26e2a8bf-497f-4ca1-a0f7-44fbb9b467b0")
		)
		(pad "6" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 88 "Net-(R46-Pad1)")
			(pintype "passive")
			(uuid "a9a74f0d-b7cd-487f-a0ec-dfbf86d1219a")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-6_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:DFN-14-1EP_3x4.5mm_P0.65mm_EP1.65x4.25mm"
		(layer "F.Cu")
		(uuid "353d83b1-8d2d-4dfd-a940-436ad4e232a9")
		(at 75.1875 159.80625 180)
		(descr "14-lead very thin plastic quad flat, 3.0x4.5mm size, 0.65mm pitch (http://ww1.microchip.com/downloads/en/DeviceDoc/14L_VDFN_4_5x3_0mm_JHA_C041198A.pdf)")
		(tags "VDFN DFN 0.65mm")
		(property "Reference" "U19"
			(at 0 -3.45 0)
			(layer "F.SilkS")
			(uuid "fa25745b-6728-4e95-893e-b089f03e344c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MCP2518FD-xQBB"
			(at 0 3.65 0)
			(layer "F.Fab")
			(uuid "51d859c1-a269-44b0-8332-cec4320512c5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-14-1EP_3x4.5mm_P0.65mm_EP1.65x4.25mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b54b5cbd-dd8f-4977-8757-0732a7529e7b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/External-CAN-FD-Controller-with-SPI-Interface-DS20006027B.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ad4557cb-7e79-49dd-b781-08b7346412db")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "CAN FD Controller with SPI Interface, up to 8 Mbps, Vdd 2.7..5.5V,  functional safety ready, VDFN-14"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ad66cf80-57a7-4e88-bc0a-30b9961f8a1b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DFN*1EP*3x4.5mm*P0.65mm*")
		(path "/742e1537-39e1-4cc7-8b28-8e44347174fb")
		(sheetname "Główny")
		(sheetfile "16_ChannelPowerControlBoard.kicad_sch")
		(attr smd)
		(fp_line
			(start 1.5 -2.36)
			(end -1.5 -2.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fa9b196c-5c6c-4c83-bc94-4d2a7f40fd10")
		)
		(fp_line
			(start -1.5 2.36)
			(end 1.5 2.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9b6898a3-1cf6-48aa-8b62-81957fb04c64")
		)
		(fp_poly
			(pts
				(xy -2.07 -2.26) (xy -2.55 -2.26) (xy -2.07 -2.74) (xy -2.07 -2.26)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "1c16461e-6c2f-4019-9a0d-3bb3926fe438")
		)
		(fp_line
			(start 2.18 2.5)
			(end 2.18 -2.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "08772ba2-adb3-4af8-bc68-af7d5dcded7f")
		)
		(fp_line
			(start 2.18 -2.5)
			(end -2.18 -2.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8060de9e-81b0-4504-8b37-2488df1c8ccf")
		)
		(fp_line
			(start -2.18 2.5)
			(end 2.18 2.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "246d0ceb-d3ee-4156-a70c-a68b37b24f61")
		)
		(fp_line
			(start -2.18 -2.5)
			(end -2.18 2.5)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "046f3ae6-0acf-41b5-91ac-b4334f7c012b")
		)
		(fp_line
			(start 1.5 2.25)
			(end 1.5 -2.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "87dd7012-c8ee-4034-afb0-982ce4636f1f")
		)
		(fp_line
			(start 1.5 -2.25)
			(end -0.75 -2.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b20aab84-26cc-4f2d-aacc-5859088d4adc")
		)
		(fp_line
			(start -0.75 -2.25)
			(end -1.5 -1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c035b306-ee95-45db-8dc8-92db3fc745f5")
		)
		(fp_line
			(start -1.5 2.25)
			(end 1.5 2.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0f11bff4-0093-4b21-9896-70312e308d2c")
		)
		(fp_line
			(start -1.5 2.25)
			(end -1.5 -1.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8787dc2d-62f4-427f-9927-b2ec898183b9")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "c3e2d1b4-22b0-4d15-a5e2-d0b50f6a2a6b")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "" smd rect
			(at -0.4125 -1.59375 180)
			(size 0.66 0.85)
			(layers "F.Paste")
			(uuid "f3ddf199-39f3-4232-abcb-2dc2ea87a14b")
		)
		(pad "" smd rect
			(at -0.4125 -0.53125 180)
			(size 0.66 0.85)
			(layers "F.Paste")
			(uuid "e8606e04-9a77-47c0-b804-8a39bfbccf67")
		)
		(pad "" smd rect
			(at -0.4125 0.53125 180)
			(size 0.66 0.85)
			(layers "F.Paste")
			(uuid "84fe979a-76a9-4620-8fe3-9a8097466463")
		)
		(pad "" smd rect
			(at -0.4125 1.59375 180)
			(size 0.66 0.85)
			(layers "F.Paste")
			(uuid "22f08994-6b0b-464e-8236-e77c4c390d97")
		)
		(pad "" smd rect
			(at 0.4125 -1.59375 180)
			(size 0.66 0.85)
			(layers "F.Paste")
			(uuid "3eebd641-1934-4b63-82f8-f6467d6f7ea2")
		)
		(pad "" smd rect
			(at 0.4125 -0.53125 180)
			(size 0.66 0.85)
			(layers "F.Paste")
			(uuid "2509745a-ae68-43cd-a115-fc2fcac7a3bf")
		)
		(pad "" smd rect
			(at 0.4125 0.53125 180)
			(size 0.66 0.85)
			(layers "F.Paste")
			(uuid "1f09a474-b934-4262-b3ac-8596b5bfa2e9")
		)
		(pad "" smd rect
			(at 0.4125 1.59375 180)
			(size 0.66 0.85)
			(layers "F.Paste")
			(uuid "69e2a55f-f305-4d69-a23f-5e6ae6a2e558")
		)
		(pad "1" smd oval
			(at -1.5 -1.95 180)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 184 "Net-(U1-TXD)")
			(pinfunction "TXCAN")
			(pintype "output")
			(uuid "a63bb9b0-225f-4426-be32-54d16dc1505a")
		)
		(pad "2" smd oval
			(at -1.5 -1.3 180)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 179 "Net-(U1-RXD)")
			(pinfunction "RXCAN")
			(pintype "input")
			(uuid "e9b9f87c-8cae-4b81-970b-fdc4d28fbcc9")
		)
		(pad "3" smd oval
			(at -1.5 -0.65 180)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 218 "unconnected-(U19-CLKO{slash}SOF-Pad3)")
			(pinfunction "CLKO/SOF")
			(pintype "output")
			(uuid "6beff7d0-5345-49ec-8873-1278f8d90a31")
		)
		(pad "4" smd oval
			(at -1.5 0 180)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 215 "unconnected-(U19-~{INT}-Pad4)")
			(pinfunction "~{INT}")
			(pintype "output")
			(uuid "06d29f9f-7303-4138-b9b5-371be377061a")
		)
		(pad "5" smd oval
			(at -1.5 0.65 180)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 165 "Net-(U19-OSC2)")
			(pinfunction "OSC2")
			(pintype "output")
			(uuid "803b4cdf-c73e-46d5-85ab-14308c2e8bfa")
		)
		(pad "6" smd oval
			(at -1.5 1.3 180)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 166 "Net-(U19-OSC1)")
			(pinfunction "OSC1")
			(pintype "input")
			(uuid "e4d6e892-f543-4b99-8c9c-09da07ac63a4")
		)
		(pad "7" smd oval
			(at -1.5 1.95 180)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(uuid "27d873ca-1a3a-4360-8175-b280022df7e1")
		)
		(pad "8" smd oval
			(at 1.5 1.95 180)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 216 "unconnected-(U19-~{INT1}{slash}GPIO1-Pad8)")
			(pinfunction "~{INT1}/GPIO1")
			(pintype "bidirectional")
			(uuid "2b201c86-787d-4a4e-a91c-484ee88282cf")
		)
		(pad "9" smd oval
			(at 1.5 1.3 180)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 217 "unconnected-(U19-~{INT0}{slash}GPIO0{slash}XSTBY-Pad9)")
			(pinfunction "~{INT0}/GPIO0/XSTBY")
			(pintype "bidirectional")
			(uuid "5831a988-657d-4e36-a637-dcc5fe39fc71")
		)
		(pad "10" smd oval
			(at 1.5 0.65 180)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 167 "+3.3V")
			(pinfunction "SCK")
			(pintype "input")
			(uuid "779e843d-bf5c-4a49-9dcf-c73bb36fe5ab")
		)
		(pad "11" smd oval
			(at 1.5 0 180)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 212 "SPI1_MOSI")
			(pinfunction "SDI")
			(pintype "input")
			(uuid "44e17362-a872-4c12-886d-c6a1643264ed")
		)
		(pad "12" smd oval
			(at 1.5 -0.65 180)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 197 "SPI1_MISO")
			(pinfunction "SDO")
			(pintype "output")
			(uuid "e9d290bf-de8e-4f74-9895-0b1103af859d")
		)
		(pad "13" smd oval
			(at 1.5 -1.3 180)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 219 "SPI1_NSS")
			(pinfunction "~{CS}")
			(pintype "input")
			(uuid "dcaa7ca2-d604-4ffc-87eb-8659168586c5")
		)
		(pad "14" smd oval
			(at 1.5 -1.95 180)
			(size 0.85 0.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 167 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
			(uuid "c4849685-a629-4e1d-b93d-7f99b5096215")
		)
		(pad "15" smd rect
			(at 0 0 180)
			(size 1.65 4.25)
			(layers "F.Cu" "F.Mask")
			(net 41 "GND")
			(pinfunction "VSS")
			(pintype "passive")
			(uuid "fa3220e7-e331-4d5f-bc73-c648efce6e76")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/DFN-14-1EP_3x4.5mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
		(layer "F.Cu")
		(uuid "41c89c8e-0f97-4797-9a39-8582a63268a5")
		(at 25.114284 111.84 -90)
		(descr "Terminal Block Phoenix MKDS-3-2-5.08, 2 pins, pitch 5.08mm, size 10.2x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-3-2-5.08 pitch 5.08mm size 10.2x11.2mm^2 drill 1.3mm pad 2.6mm")
		(property "Reference" "J7"
			(at 3.1 -3 90)
			(layer "F.SilkS")
			(uuid "17219a8f-0b7d-46f0-9166-0850dd66ff0f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 2.54 6.36 -90)
			(layer "F.Fab")
			(uuid "09265c9d-66b9-49b2-a719-6948651d9615")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "9897539c-7747-49e6-bd7a-eadd7da6d441")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "4dd1cb18-2c9b-4e86-b8ad-4dfb6de294f7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "ec4f85e3-8f3d-4066-a4c9-2b5ab0e61ecc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/4a841339-199f-4bc7-a6bd-fe2a9936827c/60e4d8a3-c16e-48cd-a1fd-61f2968ecc7b")
		(sheetname "Triac Circuit6")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.84 5.6)
			(end -2.34 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "49d205fe-96cf-4a97-bbc1-ab80d05701d0")
		)
		(fp_line
			(start -2.6 5.36)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "45ca2bde-808b-4e3e-a52c-1178d6d8f54e")
		)
		(fp_line
			(start -2.84 4.86)
			(end -2.84 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "26a01ce1-0110-433c-b5b8-426f0d036b46")
		)
		(fp_line
			(start -2.6 4.8)
			(end 7.68 4.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "48d77b3a-b2ec-420b-91e1-d2cd31b5a6da")
		)
		(fp_line
			(start -2.6 2.3)
			(end 7.68 2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "92bc5796-63e6-48c3-aa82-884d36ce2c70")
		)
		(fp_line
			(start -1.282 1.547)
			(end -1.388 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7a0a6a2e-d755-4ea9-888e-f8bc9331b4f6")
		)
		(fp_line
			(start -1.548 1.281)
			(end -1.654 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f4652b13-be25-4843-81d9-1423fa6efa5e")
		)
		(fp_line
			(start 4.073 1.274)
			(end 3.693 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7e9ff34b-49b1-45f3-9fb3-c38d5c9c246d")
		)
		(fp_line
			(start 3.822 0.992)
			(end 3.427 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "73b654eb-7452-4aa3-83f8-dc441b9364e4")
		)
		(fp_line
			(start 1.654 -1.388)
			(end 1.547 -1.281)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9f3af075-389a-40bf-adf5-239c92c8b825")
		)
		(fp_line
			(start 6.734 -1.388)
			(end 6.339 -0.992)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "59fbae61-b60a-4bae-a1c6-f3674b0f12ee")
		)
		(fp_line
			(start 1.388 -1.654)
			(end 1.281 -1.547)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "497c40d1-2890-49ec-ab61-a841f36d2dc3")
		)
		(fp_line
			(start 6.468 -1.654)
			(end 6.088 -1.274)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9519bb00-d71d-498d-b124-f9d770ccfe41")
		)
		(fp_line
			(start -2.6 -3.9)
			(end 7.68 -3.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ea754683-06e5-4325-8b31-6b742bf578ab")
		)
		(fp_line
			(start -2.6 -5.96)
			(end -2.6 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1c26a231-31c3-423b-9502-181a4ff0d517")
		)
		(fp_line
			(start -2.6 -5.96)
			(end 7.68 -5.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3e80fffd-5851-4c2c-b4d3-14a97c6ac721")
		)
		(fp_line
			(start 7.68 -5.96)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a0f629ed-6d74-4e63-b237-9d0d3f9e9955")
		)
		(fp_circle
			(center 0 0)
			(end 2.18 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "d690d2ed-8406-4c20-b1f5-e211ec077bbf")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.26 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "d84a0915-5d9d-4dd5-8751-45620d45e14b")
		)
		(fp_line
			(start -3.04 5.8)
			(end 8.13 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bb8c3bc0-7293-4721-9028-2f876a7e2b8b")
		)
		(fp_line
			(start 8.13 5.8)
			(end 8.13 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9fc4c5e7-ed23-4c44-9c71-ebba514cc4d9")
		)
		(fp_line
			(start -3.04 -6.4)
			(end -3.04 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "14410b13-9745-46b2-8dcc-bf2d8950a0f4")
		)
		(fp_line
			(start 8.13 -6.4)
			(end -3.04 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "12900a9a-3c38-4462-bdb3-38780c5c3e59")
		)
		(fp_line
			(start -2.04 5.3)
			(end -2.54 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "08be8fde-4bed-4aa9-99a6-dde7b48c9b49")
		)
		(fp_line
			(start 7.62 5.3)
			(end -2.04 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8753d497-fc66-4032-a422-e273126aae43")
		)
		(fp_line
			(start -2.54 4.8)
			(end 7.62 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6c898972-7666-4fb1-ad7e-e82b6270dea2")
		)
		(fp_line
			(start -2.54 4.8)
			(end -2.54 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c034ba36-49f9-4472-8eac-4dfd0703a3c0")
		)
		(fp_line
			(start -2.54 2.3)
			(end 7.62 2.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1fe506d4-acc3-4900-b37b-a9f88b2f18d3")
		)
		(fp_line
			(start 1.517 -1.273)
			(end -1.273 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fc957808-69a7-49b8-9378-6a009b2cef80")
		)
		(fp_line
			(start 6.597 -1.273)
			(end 3.808 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d4097c7e-a073-454e-aa6e-d86731295070")
		)
		(fp_line
			(start 1.273 -1.517)
			(end -1.517 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2995043a-8e2f-4d5e-966e-9c3a73d6e66f")
		)
		(fp_line
			(start 6.353 -1.517)
			(end 3.564 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3db764f6-41ef-41aa-a4b2-30803f5ef5a7")
		)
		(fp_line
			(start -2.54 -3.9)
			(end 7.62 -3.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4d23fc3e-fff2-4af2-ad35-8e49f0ef25a7")
		)
		(fp_line
			(start -2.54 -5.9)
			(end 7.62 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "45db4704-eb3e-4837-835c-e149c8269c47")
		)
		(fp_line
			(start 7.62 -5.9)
			(end 7.62 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "480fb691-cf35-4512-bf4e-4cb384301ea5")
		)
		(fp_circle
			(center 0 0)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "1fa83f96-5c6f-4891-8275-8716627263f8")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.08 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "641afe9f-87d0-4c4b-8370-b686b29d1a5b")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 3.1 -90)
			(layer "F.Fab")
			(uuid "71a57323-0e81-4dba-be7b-caec6b75d587")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "/Triac Circuit6/High_Voltage_L")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "0d2f0676-90fe-43e7-8ff0-547fd36e0d19")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/Triac Circuit6/High_Voltage_Out")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "62234fb0-e3e2-422b-973d-4d867e678ad5")
		)
		(model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "44b6c4c8-74e0-4c38-98a8-2bbe67f98cb2")
		(at 48.628571 83.36)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "2ac584dd-28b4-4494-b984-d3aa70c5b261")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at -3.64 0 0)
			(layer "F.Fab")
			(uuid "0c2dee59-509f-4056-84fc-63392b185abe")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3d570a7b-16b9-411c-aa3e-923aae011382")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "076dad7a-e018-4d5c-b4b6-fa999538b437")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4438fee3-647a-4c80-8d0f-9fa0aad815f6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/e56f6699-6dcd-4f6f-a67f-2156f450d5f1/ca31a324-056f-45d6-b948-82e97db62734")
		(sheetname "Triac Circuit4")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c1de7c16-0fb5-4855-9c92-9e6b4b6586a6")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a3178939-5806-4853-8ab0-3b5b0e2adea2")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f67f9630-d6be-4af4-8b80-dc4411bff76a")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1a604fa8-8809-498a-9c51-7ce0a36303b8")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d7d4e51b-b558-41b3-88d2-51f380116bc4")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9badf30d-e9b0-4bf0-8024-97ff6edd9f1c")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b0d7ce7c-6ce6-4d83-9d84-7ae8e28d870d")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6a8087e9-033b-453f-8e3b-66078de3dc3e")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c2980f75-7d2e-48ee-a9a6-ca6ce38f0a86")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "90dd16e7-d068-412a-b518-16a1e9fa0d08")
		)
		(fp_text user "${REFERENCE}"
			(at 3.04 0.01 0)
			(layer "F.Fab")
			(uuid "abc3558b-cd90-40eb-bf81-c96c6c3a35f5")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 62 "Net-(Q10-B)")
			(pintype "passive")
			(uuid "c55a18be-17a4-4d46-b0cd-1b1664d60cad")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 27 "/Triac Circuit4/Enable")
			(pintype "passive")
			(uuid "dcafe74d-0bf3-494e-91f4-367502f8f654")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "4519c7c1-b4c7-46a0-abb2-eec72756e8a2")
		(at 53.605355 56.68 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R32"
			(at 0 -1.82 180)
			(layer "F.SilkS")
			(uuid "1ab403f1-1a0a-4e27-afd6-89a937755d8b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at 0 1.82 180)
			(layer "F.Fab")
			(uuid "ebf6fef0-c941-4bb6-b3fb-aaf23bb99832")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "20d96d09-0073-42e6-b4b2-f32ae6373a3a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "9f40e992-2f10-4e13-a3b0-8fe05675fc5a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "db990c9b-46b8-433e-a378-8c7bfc8932b7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/d20c900a-3d9a-4460-9d5d-3ed4d11c2b93/de24ad75-a874-4d54-a682-b1d6f2079d30")
		(sheetname "Triac Circuit10")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bb7b09da-d921-4b4d-ad7c-6c45ba51e771")
		)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dc98e0a4-9d61-4fcc-a7dd-b8872fef99d3")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9efabd05-6f6d-4d2f-b63e-76e48a5dddc2")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0e20a350-91cd-4768-aad7-902cc22cf9e0")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dac3768a-b4e9-4e92-9358-bb29a5c0ecae")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "daa984c9-19e1-4a8d-a152-ca2e09099d70")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0b1a7eb4-b68f-4d0a-b693-9479e4313d23")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9bb78bf9-eeaa-4eb0-b102-4e8753cf43d2")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c19ec80c-5c4d-439c-bb18-14a76d7b7dff")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "70c6bef1-20ad-4de7-8ad4-e710d8a2acda")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
			(uuid "9a6c6533-d5a1-4627-8343-b49ef17a8678")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 119 "Net-(R32-Pad1)")
			(pintype "passive")
			(uuid "3ecd52ed-e9b6-4abe-9c0e-b3fedfd445ed")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 37 "+3V3")
			(pintype "passive")
			(uuid "981f8c83-0ab3-4281-a228-13a8672e31e5")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(uuid "4674aa0b-b56c-454e-a4bf-8ed79c385e5e")
		(at 35.142858 40.58 90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R4"
			(at 3.81 -1.92 90)
			(layer "F.SilkS")
			(uuid "33ccc797-5c6b-485d-8aea-3ef758c51a66")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "180"
			(at 3.81 1.92 90)
			(layer "F.Fab")
			(uuid "4def138d-372c-44ab-821f-fcad8e72c4a6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "99873579-ff52-4831-89ae-dfb835b437bb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4846f2c5-c18e-4926-b0e6-a0fba5463a20")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c10cf97e-e9ec-4537-95e8-7035df785bb7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/98cc9bb7-a6bb-4cad-bced-cd34a966891d/4ab64e29-964f-40b2-bf58-c546b31cd3eb")
		(sheetname "Triac Circuit1")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 5.73 -0.92)
			(end 1.89 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "552f7274-f6fb-4415-89b5-e4c1f1bc84b1")
		)
		(fp_line
			(start 1.89 -0.92)
			(end 1.89 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d73ed189-a5ca-487c-addf-e87bccaa66ed")
		)
		(fp_line
			(start 6.68 0)
			(end 5.73 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "acf0d0cf-231b-49b5-a47c-afbfcd038cdb")
		)
		(fp_line
			(start 0.94 0)
			(end 1.89 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a628366d-5450-444a-9f76-e725317a3e43")
		)
		(fp_line
			(start 5.73 0.92)
			(end 5.73 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "efb2fb00-c567-46ea-9633-7848906914e6")
		)
		(fp_line
			(start 1.89 0.92)
			(end 5.73 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f811ae77-a908-45ea-9d98-01bddad82cff")
		)
		(fp_line
			(start 8.57 -1.05)
			(end -0.95 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b47cd1ed-7e15-4c65-b4dc-5f4efa7cb151")
		)
		(fp_line
			(start -0.95 -1.05)
			(end -0.95 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "52d61fa0-f685-4009-895b-6145392c4a48")
		)
		(fp_line
			(start 8.57 1.05)
			(end 8.57 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "57d6ec87-f935-4c6f-a32a-a7246096baa3")
		)
		(fp_line
			(start -0.95 1.05)
			(end 8.57 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f82bc10a-a82b-4e2d-8c00-732608d3f579")
		)
		(fp_line
			(start 5.61 -0.8)
			(end 2.01 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6bfc96f2-6efc-413f-94a0-f042bd3e3473")
		)
		(fp_line
			(start 2.01 -0.8)
			(end 2.01 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "017a7348-2914-4887-9485-aab0bf97f88b")
		)
		(fp_line
			(start 7.62 0)
			(end 5.61 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "879d9e81-c6bb-4561-b220-21288696203d")
		)
		(fp_line
			(start 0 0)
			(end 2.01 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e2205149-ac88-4c43-b752-092c89b81082")
		)
		(fp_line
			(start 5.61 0.8)
			(end 5.61 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "94f54918-1f02-4b09-bbe5-26977e1baccf")
		)
		(fp_line
			(start 2.01 0.8)
			(end 5.61 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b176aa48-c0a5-4d73-b0d5-1e19f731dc19")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
			(uuid "c598c30f-085e-43ee-8e4a-e018d1172a13")
			(effects
				(font
					(size 0.72 0.72)
					(thickness 0.108)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "Net-(R4-Pad1)")
			(pintype "passive")
			(uuid "fedee279-3ff4-4c31-a2d2-a1610a815d38")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/Triac Circuit1/High_Voltage_L")
			(pintype "passive")
			(uuid "159b8188-10d3-409f-91f8-e7334f491674")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-6_W7.62mm"
		(layer "F.Cu")
		(uuid "49afd879-dfd7-46bc-8da6-94f594fd213e")
		(at 38 172.795)
		(descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U20"
			(at 4.44 -15.49 0)
			(layer "F.SilkS")
			(uuid "57ba2219-d71c-4606-87f8-58f1f2b8b5ac")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "H11AA1"
			(at 3.81 7.41 0)
			(layer "F.Fab")
			(uuid "7950cede-acd3-4349-baf5-9f8c0b68ddcd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "51db65b1-eec7-44fa-bc3b-f27d9df72926")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.vishay.com/docs/83608/h11aa1.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c85abc31-e0f7-4d0b-930d-1f2d69898534")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "AC/DC NPN Optocoupler, DIP-6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "98965020-60b6-453c-96c7-755edbd76538")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm*")
		(path "/eb409310-6102-43e5-b48c-2438ac1942c0/2b6fa8d2-7a33-45e1-b250-775e27348972")
		(sheetname "ZeroCrossDetection")
		(sheetfile "ZeroCrossDetection.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7b3af574-6480-4c63-92ee-89a9a500ed5e")
		)
		(fp_line
			(start 1.16 6.41)
			(end 6.46 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "75cd533c-e4a0-44ae-8b4f-bb3b070af1ba")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e0bf15c8-f229-4f78-a469-c0ba25003409")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "33b99edd-0591-4c0d-af29-bb9de497a9f9")
		)
		(fp_line
			(start 6.46 6.41)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7fcd14d8-74cf-4d84-be69-271ec649afb6")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e7167229-497a-4fe0-9b01-3d61f9414334")
		)
		(fp_line
			(start -1.1 -1.55)
			(end -1.1 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "47c871b4-1058-4b3e-b94f-d2225dfcf462")
		)
		(fp_line
			(start -1.1 6.6)
			(end 8.7 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "88a2f6ec-3e30-4b96-8150-73a4c3059eb6")
		)
		(fp_line
			(start 8.7 -1.55)
			(end -1.1 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b5bd4047-41d9-4073-afe4-da8c3b51e06c")
		)
		(fp_line
			(start 8.7 6.6)
			(end 8.7 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5c106776-c352-44cd-8bef-b206d5e46a6c")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5b14e36f-a2e9-4ed4-a4bd-07d343be618a")
		)
		(fp_line
			(start 0.635 6.35)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "67abf103-49ce-4668-aaf9-04f2c00126b7")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0a7ea169-b4ce-4b28-8729-f9c78c698982")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "de69d787-502f-497a-a063-eaca0a73bb58")
		)
		(fp_line
			(start 6.985 6.35)
			(end 0.635 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2f544299-afea-4241-9055-f0caf08f178c")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.54 0)
			(layer "F.Fab")
			(uuid "eb22c9b1-bd95-4240-8748-df378e20920a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "Net-(R49-Pad2)")
			(pintype "passive")
			(uuid "3bf1e299-a488-4a84-9e09-458848be80a3")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 233 "Net-(R50-Pad2)")
			(pintype "passive")
			(uuid "6dca7a57-0f81-48a1-a077-e1a8e0585fb0")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 221 "unconnected-(U20-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "bf8696ae-0978-4246-9687-02b5863fc8af")
		)
		(pad "4" thru_hole oval
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "GND")
			(pintype "passive")
			(uuid "73ed2b38-1354-4af0-a036-f7bc3037235b")
		)
		(pad "5" thru_hole oval
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 168 "/ZeroCrossDetection/OUT")
			(pintype "passive")
			(uuid "ac89f7e3-ebda-49a5-978b-32a613de6985")
		)
		(pad "6" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 220 "unconnected-(U20-Pad6)")
			(pintype "passive")
			(uuid "27d9cd53-5524-4adb-9bed-2db0a78f734c")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-6_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "4a07a8e8-6846-4538-80a5-80cad08e082a")
		(at 48.194642 95.8 180)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q12"
			(at 0 -2.4 0)
			(layer "F.SilkS")
			(uuid "ecaf5f1e-848e-4cd4-acff-b55731464456")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BC818"
			(at 0 2.4 0)
			(layer "F.Fab")
			(uuid "71a73abb-f9d7-4711-a6d5-509d20266ace")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "96670667-4496-47e8-8b7b-14f2cb2a420b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC818-D.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "2a52662a-3c74-4676-a4e6-c09c032cc057")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "84f2e541-1f2d-4991-9781-84f9f246ff43")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/6eb41966-4a54-4fd9-a1be-49d2f272d785/00e550ea-8431-483d-ac3c-b4a719825546")
		(sheetname "Triac Circuit5")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 1.56)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "22197d36-913e-447f-8538-afee086d55da")
		)
		(fp_line
			(start 0 1.56)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "78c12a98-3a8c-47fb-88f0-56d96b769578")
		)
		(fp_line
			(start 0 -1.56)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "688fcb87-466b-4cf0-b17d-5214842088ef")
		)
		(fp_line
			(start 0 -1.56)
			(end -1.675 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1f85e2aa-237a-498f-9e45-93db7d688873")
		)
		(fp_line
			(start 1.92 1.7)
			(end 1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "775ee452-c8dd-40ce-a66d-453442637445")
		)
		(fp_line
			(start 1.92 -1.7)
			(end -1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e05d9c53-d098-4759-a39f-d112256b2cc3")
		)
		(fp_line
			(start -1.92 1.7)
			(end 1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ada6e493-fbfa-4c38-b597-27a9dd201e08")
		)
		(fp_line
			(start -1.92 -1.7)
			(end -1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e89a174e-6ccd-4992-8095-ed7a26885675")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d1e49cc9-6390-436e-bb3f-bb5f012e72cc")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "26d2f877-b968-44b2-af6d-d7d53c6c2900")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a804f064-eaff-41bc-8686-27055634cdf4")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c33b107b-1aff-4b75-9a63-3e1303147a6e")
		)
		(fp_line
			(start -0.65 -1.125)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "64bf095d-1ee7-4092-ab87-e70e9bb37ee3")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "0d2d1880-7d00-451e-acb9-8b63edc560c2")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 68 "Net-(Q12-B)")
			(pinfunction "B")
			(pintype "input")
			(uuid "5a57fe3e-1f96-46a8-9ac8-ee5bdd959162")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "GND")
			(pinfunction "E")
			(pintype "passive")
			(uuid "7b85f813-61ba-47f6-8856-57c2e7e2fb18")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 70 "Net-(Q12-C)")
			(pinfunction "C")
			(pintype "passive")
			(uuid "424e7985-7887-4b7f-9bce-0171d404b571")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "4aeb7948-fc53-4a5e-aef9-9e9aa63ee8eb")
		(at 48.480358 39.84)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "1dde0047-db7d-4844-8d6d-016b0724182c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "53535873-a06d-43e6-87ef-4c1a42c92498")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8af5938c-9332-4fdf-a806-883f2ba6051b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "5b17aa44-2cf2-4680-bfbc-b61acdf5ecca")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "18d38c90-c86c-4341-8e0c-a31d692c6cd8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/98cc9bb7-a6bb-4cad-bced-cd34a966891d/de24ad75-a874-4d54-a682-b1d6f2079d30")
		(sheetname "Triac Circuit1")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "acbebdfb-4725-4cb6-8eec-c00ceaaf2590")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f15d58cd-5e6e-4d8f-b907-03a268401006")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "954cffcd-eada-43c5-8a1c-9e811b4fa8f0")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5ea0d8da-c408-4c23-9c2b-889364c24a9f")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e7c1b9f0-9c5a-4a68-b47d-b958bebbd6f9")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "87194f08-5e9a-42c0-9f4d-046389bbdf12")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "213c1450-0245-46e7-b4c5-97f4c876e428")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dfac2436-d5e2-4ab4-8f5c-2f2df55f4ee9")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "15164e2e-03d9-487f-8822-38ddbe6eafb8")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c3290eac-a66b-4e5f-bf80-ebf800e8c557")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "0b77073e-214c-417e-8288-c84a6a7713cc")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 110 "Net-(R5-Pad1)")
			(pintype "passive")
			(uuid "0926cae5-efc9-4c6f-8418-37ec0e83cf32")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 37 "+3V3")
			(pintype "passive")
			(uuid "0321ec3e-644d-4d73-b6e0-0c9e6e2f565d")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(uuid "500ab741-9e15-4c9f-809f-66649e4c72d5")
		(at 33.4 158 90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R55"
			(at 2.54 -1.92 90)
			(layer "F.SilkS")
			(uuid "8ec1c758-46f2-487c-aa2c-4d568f5f9abb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "220k"
			(at 2.54 1.92 90)
			(layer "F.Fab")
			(uuid "ee1e72da-661c-44c7-8f97-3a8327a20d54")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "528361a2-010a-4e31-87ee-378940ba9dbb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "748ac65a-2ae9-4096-87eb-8f536df0ff60")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "70f07021-3ffd-4fac-929e-8cf4a3853fd1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/e9267efd-e7bf-4ed4-9938-23d638b0f804/a8ed06bc-ef8c-4560-b835-f2ef8ce81949")
		(sheetname "ZeroCrossDetection1")
		(sheetfile "ZeroCrossDetection.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 0.62 -0.92)
			(end 4.46 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0beed406-2acd-4c6e-b9e0-3ccf8f7ef4ac")
		)
		(fp_line
			(start 0.62 0.92)
			(end 4.46 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "190a3739-41f4-46d3-9a0b-932d0428780a")
		)
		(fp_line
			(start 6.03 -1.05)
			(end -0.95 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6725c6b2-a8d7-4626-ab6e-ba1e08241e70")
		)
		(fp_line
			(start -0.95 -1.05)
			(end -0.95 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "44fedd63-d086-44ed-b72e-59d9620aa36e")
		)
		(fp_line
			(start 6.03 1.05)
			(end 6.03 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7a75f950-8656-468f-8f02-c84ad16aa7c1")
		)
		(fp_line
			(start -0.95 1.05)
			(end 6.03 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4630b39c-5e8c-46ce-83dc-5e915fc1d5b7")
		)
		(fp_line
			(start 4.34 -0.8)
			(end 0.74 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c822fba0-0a25-44e5-90b2-bea3d30a2995")
		)
		(fp_line
			(start 0.74 -0.8)
			(end 0.74 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "def1fae0-8c6b-4312-88e0-6be14a1e930e")
		)
		(fp_line
			(start 5.08 0)
			(end 4.34 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "96340908-422d-45e6-8fec-9b5d384ad449")
		)
		(fp_line
			(start 0 0)
			(end 0.74 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b56cd937-c582-4297-81e2-22bb6f79e931")
		)
		(fp_line
			(start 4.34 0.8)
			(end 4.34 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "26cbd4ab-03a6-4454-95a8-2b2be670061b")
		)
		(fp_line
			(start 0.74 0.8)
			(end 4.34 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "61a369e1-7d2e-49d8-92fa-88b1eebb7ea7")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 90)
			(layer "F.Fab")
			(uuid "90dfa7b7-4b06-4064-8ee2-320a7d56cec0")
			(effects
				(font
					(size 0.72 0.72)
					(thickness 0.108)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 229 "Net-(J18-Pin_2)")
			(pintype "passive")
			(uuid "ee398a38-d550-4cf2-a403-c708c4e49c95")
		)
		(pad "2" thru_hole oval
			(at 5.08 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 235 "Net-(R55-Pad2)")
			(pintype "passive")
			(uuid "3ec07a43-d88b-4e57-a6e5-5b49f613a546")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(uuid "50f20aa4-bc05-4527-8c1e-fd8ec6fd7785")
		(at 35.2 25.34 90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R1"
			(at 3.81 -1.92 90)
			(layer "F.SilkS")
			(uuid "bb4126b2-3939-4469-92c7-d619a74d70b8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "180"
			(at 3.81 1.92 90)
			(layer "F.Fab")
			(uuid "b8032843-0455-497f-ae4c-84e5dd4400a1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6158f630-4f75-414f-9da7-223b4a53dce9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1564420d-6083-4c0f-97e6-af3e4332d9b8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a14df1c8-c465-45c8-a596-9f76d7d96959")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/84e52baa-d126-4c4f-b1c5-63bb27b07c2b/4ab64e29-964f-40b2-bf58-c546b31cd3eb")
		(sheetname "Triac Circuit")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 5.73 -0.92)
			(end 1.89 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9edb754c-b535-4884-ba0f-3d49722e3d9a")
		)
		(fp_line
			(start 1.89 -0.92)
			(end 1.89 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6e1e7344-1acb-4822-81e9-93b29e2987c6")
		)
		(fp_line
			(start 6.68 0)
			(end 5.73 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "47bbe4c2-17d6-444f-b31c-e9140cb54720")
		)
		(fp_line
			(start 0.94 0)
			(end 1.89 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a976f73a-5f34-432f-b426-279bc689978f")
		)
		(fp_line
			(start 5.73 0.92)
			(end 5.73 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "62718477-26a8-4482-aafa-99229704ade8")
		)
		(fp_line
			(start 1.89 0.92)
			(end 5.73 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b652a961-b28f-4825-a0cd-23b4e2ac5687")
		)
		(fp_line
			(start 8.57 -1.05)
			(end -0.95 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6cea73f6-e735-4d34-8189-8d45aa8e669a")
		)
		(fp_line
			(start -0.95 -1.05)
			(end -0.95 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1e20085e-2d92-45a0-920f-bdce65abd177")
		)
		(fp_line
			(start 8.57 1.05)
			(end 8.57 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6f57e84c-5857-4218-895d-50351c1f96df")
		)
		(fp_line
			(start -0.95 1.05)
			(end 8.57 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "98cab01d-c3f1-469b-84de-10e9ebed15f0")
		)
		(fp_line
			(start 5.61 -0.8)
			(end 2.01 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ca57f38c-3e22-4707-9104-eb41ba14368d")
		)
		(fp_line
			(start 2.01 -0.8)
			(end 2.01 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "17cc9bdb-77ca-4173-9d30-2de946d7449a")
		)
		(fp_line
			(start 7.62 0)
			(end 5.61 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "761dad1e-72c0-4464-bec0-5396dcb51094")
		)
		(fp_line
			(start 0 0)
			(end 2.01 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6871f750-494d-4170-9949-c3f42bb5c345")
		)
		(fp_line
			(start 5.61 0.8)
			(end 5.61 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0e114d61-eeda-4a43-b550-6a799ca9a2c0")
		)
		(fp_line
			(start 2.01 0.8)
			(end 5.61 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "30bf04e4-b4fa-4436-8228-2a4813a6285b")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
			(uuid "ae0ba340-6c87-415d-95c1-a8d40ffc1e48")
			(effects
				(font
					(size 0.72 0.72)
					(thickness 0.108)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(R1-Pad1)")
			(pintype "passive")
			(uuid "8681d179-18fa-4e88-93ee-0ec0ec3b1783")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/Triac Circuit/High_Voltage_L")
			(pintype "passive")
			(uuid "fc754d18-574e-4042-8b43-cc388482c64f")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "52f4745a-2df5-4fcf-8961-5bf25f24178e")
		(at 48.594642 100.8)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R17"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "6819519b-4c38-4208-ae21-012afdf0efae")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "3531e487-a35b-4e14-9da3-0ba85e7e2416")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "37b04426-1eee-4245-b29d-ea8abf4024a7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b9d5e119-dadf-45b6-a893-8e92fb0a4c0e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "1b235454-bb63-4e00-8d17-f087a065b16a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/6eb41966-4a54-4fd9-a1be-49d2f272d785/de24ad75-a874-4d54-a682-b1d6f2079d30")
		(sheetname "Triac Circuit5")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "036a0daa-9bce-4c09-8d06-9ec23b203ba4")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dae7dfd4-4d54-404d-9064-0cf2e70c48d1")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "be8717d6-69b4-4a3b-a556-c9a53e511977")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b7eefff0-5b15-4afd-a66a-75ef59bfff3b")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6525d1fd-c612-44fb-a25b-8369bdabdcbd")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a9ddb53d-8fed-4306-b044-5410faa36c7b")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fc3b6088-0e3a-4392-b3f5-41e20c63696b")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "04138705-8f1a-4dc1-883f-1158d41d9a41")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "71f00852-589f-45f4-8ced-0c4863afa4a5")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4bd5f5a8-d810-401e-9a06-e1bd6e8f3297")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "279e5936-5475-41b3-ae3f-6adbc9e65345")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 114 "Net-(R17-Pad1)")
			(pintype "passive")
			(uuid "52fa1d2b-6b51-46bb-b5a2-64a3c26a1980")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 37 "+3V3")
			(pintype "passive")
			(uuid "c6f3c930-eda9-4b06-8102-d72464874e6c")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "5567103a-f850-44bf-9d46-ca49121f61a9")
		(at 45.8 169.92)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R53"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "cd4cb466-1a7b-4683-bc12-1031080cacf8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "1k"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "2bc69abb-e8d7-4e3c-a8d8-8007ac1ca93b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d7938d91-6f5b-4740-ab22-3ee71cde7b8a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "203e7d5a-edc2-4b9f-a694-4cc48b22aae1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "044428f0-ac60-4d9d-b183-c07204e2c51e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/eb409310-6102-43e5-b48c-2438ac1942c0/547580b6-9698-46ab-b758-90ae2111cb33")
		(sheetname "ZeroCrossDetection")
		(sheetfile "ZeroCrossDetection.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c77e6733-b332-4eb0-aca4-f2833092fb6c")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7575feed-0697-437b-9f72-7d0c2d2c213d")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4639a891-f92b-4942-8b2b-b75bed894604")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "edb25439-14fa-4c9e-9591-f140266ad95e")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c4ba225a-d659-4633-a5f2-9d8f35cca6b7")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "21de8b28-4426-4417-9bdf-d3d0cda7c4f5")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "144fb7ce-ae2f-45cb-a1f2-a33f96e19eab")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "08b0c9ab-4441-4e86-af34-e9e09c752542")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "87c0cdf4-fd4f-4aee-ade5-bf08a132b62b")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0e6290af-fc08-4423-a649-c2f8bc6c541c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "3b565dc9-2c47-4a8d-b1e9-948215e0fb43")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 168 "/ZeroCrossDetection/OUT")
			(pintype "passive")
			(uuid "da528bf3-390b-4e79-8245-b46c7c424eb5")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 167 "+3.3V")
			(pintype "passive")
			(uuid "b5247bfb-be95-49fe-a29d-af8a3f1395c7")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "5676772a-4d7f-41df-ba62-9ea61802e888")
		(at 53.542855 104.6 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R42"
			(at 0 -1.82 180)
			(layer "F.SilkS")
			(uuid "f9cde911-c801-4b9e-93ab-fb62debb5864")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at -3.64 0 180)
			(layer "F.Fab")
			(uuid "65ceed9f-12e5-414e-81de-3fe6801fb4ff")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "a72f2f2f-80b4-4c14-b07a-8296d7627b2b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "29a91e47-0a11-4e3a-86d4-c700fdfed142")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "735532b9-6791-42af-8022-779b69275829")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/4a948621-4b4c-41c9-b07f-b928eecc9e1e/ca31a324-056f-45d6-b948-82e97db62734")
		(sheetname "Triac Circuit13")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f6b309ed-b272-42a6-bfd7-1ce69dd0cd40")
		)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4e2cde59-810a-4dea-8810-52da90c1106e")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "14994ebf-f361-4ec4-8ce0-083a3e51f68e")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2e5af9c0-c36c-4efa-9541-3967c8b3210f")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ebd09f57-f1eb-4035-9778-e725368edccc")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4ea61ad8-a7cb-40bb-9227-523ac7869c4f")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fb83b60f-7c1b-416f-a27e-b479a51fe4b2")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0114ca45-b1d3-440a-b90c-f02a309cd1c2")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e258da40-22ce-4dff-bf7b-8ecf9aa2b432")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "58080ffb-6648-4172-9f25-e3adb2eed5a7")
		)
		(fp_text user "${REFERENCE}"
			(at 3.04 0.01 180)
			(layer "F.Fab")
			(uuid "12fa2f78-4760-40d1-bb1a-cac098e3f8a3")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 152 "Net-(Q28-B)")
			(pintype "passive")
			(uuid "61b910f8-4d7b-40ca-a86c-cdd8c54bc2ba")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 136 "/Triac Circuit13/Enable")
			(pintype "passive")
			(uuid "07632588-aa67-4d0c-9f3c-c3871588eec8")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(uuid "56be091e-2dc4-4ed3-b011-c7f328219736")
		(at 66.942855 86.42 -90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R37"
			(at 3.809999 -1.92 -90)
			(layer "F.SilkS")
			(uuid "289807d3-cc9a-4979-a601-ebdd4e9d40ac")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "180"
			(at 3.81 1.919999 -90)
			(layer "F.Fab")
			(uuid "eec63f9a-7ef0-4d85-b529-7db692182e75")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "03d307c7-6eac-4ffc-bb6e-0defd4198e07")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bf6e583f-a9c5-4c3d-882c-0d43248e48ed")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bdf18f5b-edca-472c-9616-4638bd12e243")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/fb144577-8e6f-488b-ba1b-870763a27401/4ab64e29-964f-40b2-bf58-c546b31cd3eb")
		(sheetname "Triac Circuit12")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.89 0.92)
			(end 5.73 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bd7af8d7-bf05-4bfb-a3eb-3d2db953740b")
		)
		(fp_line
			(start 5.73 0.92)
			(end 5.73 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d447749b-26d0-4f46-a5c1-554764c77107")
		)
		(fp_line
			(start 0.94 0)
			(end 1.89 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8c7aeea0-60eb-4e6b-99bd-903dbf18d46e")
		)
		(fp_line
			(start 6.68 0)
			(end 5.73 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c1fbb28c-bde5-4c1f-bfbd-afba1702b8b3")
		)
		(fp_line
			(start 1.89 -0.92)
			(end 1.89 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a277bfca-2248-4eb4-b959-1594b60d6230")
		)
		(fp_line
			(start 5.73 -0.92)
			(end 1.89 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f9ddd24a-8f10-4d3e-82eb-87c612be347b")
		)
		(fp_line
			(start -0.95 1.05)
			(end 8.57 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8148f79b-ed49-4591-b163-60210e82a7b2")
		)
		(fp_line
			(start 8.57 1.05)
			(end 8.57 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "30fd0785-b83f-4775-b8b3-54ea10d1cee4")
		)
		(fp_line
			(start -0.95 -1.05)
			(end -0.95 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b3036f59-4751-49de-a152-e5b830705599")
		)
		(fp_line
			(start 8.57 -1.05)
			(end -0.95 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "99532550-9c9e-45d7-85c6-4c7482cfb03e")
		)
		(fp_line
			(start 2.01 0.8)
			(end 5.61 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ddea4cdc-81a3-46c9-b139-e3cfeda7cd38")
		)
		(fp_line
			(start 5.61 0.8)
			(end 5.61 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "58e4d331-218e-448e-a4f2-4cad89078309")
		)
		(fp_line
			(start 0 0)
			(end 2.01 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bd438cee-ac7a-4bd9-8acb-ceabae5b2706")
		)
		(fp_line
			(start 7.62 0)
			(end 5.61 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "773b76cd-5204-4a1e-9eec-3fae9d48c402")
		)
		(fp_line
			(start 2.01 -0.8)
			(end 2.01 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7c57468c-7968-4493-8bd8-cc7098af9aa4")
		)
		(fp_line
			(start 5.61 -0.8)
			(end 2.01 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "711bb09a-0b92-49a4-bfc9-65eda25e06e7")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 -90)
			(layer "F.Fab")
			(uuid "99528353-7ef8-46c6-bb4f-2d720e8232e3")
			(effects
				(font
					(size 0.72 0.72)
					(thickness 0.108)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(R37-Pad1)")
			(pintype "passive")
			(uuid "32a75cc6-ed90-46b4-8f58-d4d2ef578f6d")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 84 "/Triac Circuit12/High_Voltage_L")
			(pintype "passive")
			(uuid "c94877fa-45a1-44c7-b73d-1ba8609ac7b5")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(uuid "582b43e4-faa3-4868-9813-5994efe15e03")
		(at 35.8 170.58 -90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R49"
			(at 2.54 -1.92 90)
			(layer "F.SilkS")
			(uuid "8af6ad93-3e25-4578-ab2f-5157390a95bb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "220k"
			(at 2.54 1.92 90)
			(layer "F.Fab")
			(uuid "6bc392b1-c1e4-4a01-95ea-4c515d4f0224")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "01d959bb-584e-4bf1-aac0-d458b2f45c79")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c30a489b-46df-4d70-9b78-efc11c193c82")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ca366934-3b09-4ea7-a052-390b46d103a6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/eb409310-6102-43e5-b48c-2438ac1942c0/651d23d0-fccd-4821-a525-06dced80ce07")
		(sheetname "ZeroCrossDetection")
		(sheetfile "ZeroCrossDetection.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 0.62 0.92)
			(end 4.46 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "30a3412c-582e-431f-868d-dce4b1c04394")
		)
		(fp_line
			(start 0.62 -0.92)
			(end 4.46 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f069a0c3-b367-4737-a5f6-fab8771167a3")
		)
		(fp_line
			(start -0.95 1.05)
			(end 6.03 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f5da8651-d75b-4849-96fb-25e15a615970")
		)
		(fp_line
			(start 6.03 1.05)
			(end 6.03 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d5b3c1e7-25cb-4757-800e-3cb6e13b77a3")
		)
		(fp_line
			(start -0.95 -1.05)
			(end -0.95 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "674990e4-edf4-4eb6-a59a-31ee812f5f35")
		)
		(fp_line
			(start 6.03 -1.05)
			(end -0.95 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e648e2e2-a082-415b-b539-b50f8562b525")
		)
		(fp_line
			(start 0.74 0.8)
			(end 4.34 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fcbc04d3-d3ea-470f-81ec-995b54adeb0e")
		)
		(fp_line
			(start 4.34 0.8)
			(end 4.34 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e8c6cf3b-b761-4c21-9ebe-71cb2dbdf65f")
		)
		(fp_line
			(start 0 0)
			(end 0.74 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5d744499-16b7-4a43-83d4-1dfddac46425")
		)
		(fp_line
			(start 5.08 0)
			(end 4.34 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "460ec896-c9ee-4711-a008-262c947a8cb5")
		)
		(fp_line
			(start 0.74 -0.8)
			(end 0.74 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0da4f2fa-ea5a-4557-8323-020d9ae4c264")
		)
		(fp_line
			(start 4.34 -0.8)
			(end 0.74 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b1680167-13c2-497e-ac4e-9066949eb7b6")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 90)
			(layer "F.Fab")
			(uuid "b0adcaaa-d258-43f1-bae1-9414c6640e92")
			(effects
				(font
					(size 0.72 0.72)
					(thickness 0.108)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 227 "Net-(J17-Pin_1)")
			(pintype "passive")
			(uuid "0f84c5c5-5e53-46f8-ace5-2fe7f75ace61")
		)
		(pad "2" thru_hole oval
			(at 5.08 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 232 "Net-(R49-Pad2)")
			(pintype "passive")
			(uuid "6394e45d-15ce-460a-87f5-595560db4a88")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(uuid "5844d5fb-73a5-46e0-985f-90b1e06d055c")
		(at 32.855 20.46 -90)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "Q1"
			(at 6.04 -2.445 90)
			(layer "F.SilkS")
			(uuid "57d72fac-34bb-4fcb-93e5-47f4a2cb624a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BTA16-600B"
			(at 2.54 2.5 90)
			(layer "F.Fab")
			(uuid "07acd63a-8c05-4991-8de7-f0499dfcf152")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "c975513d-b371-4017-87cf-b9f3bdec80d2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "197a040f-821e-4703-a826-9dc65089e8eb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "83c7ada1-328a-4bf8-8846-8e2c28f42508")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO?220*")
		(path "/84e52baa-d126-4c4f-b1c5-63bb27b07c2b/d1257be0-2394-4f08-8984-f580162b15f9")
		(sheetname "Triac Circuit")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.58 1.371)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "13d08a09-ae6e-47a1-84c7-49c885f23c5b")
		)
		(fp_line
			(start -2.58 -1.76)
			(end 7.66 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1b9a94b9-849b-404d-98aa-5e4fd22da882")
		)
		(fp_line
			(start -2.58 -3.27)
			(end -2.58 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "784819ef-ef77-4812-a72e-605baad7b077")
		)
		(fp_line
			(start -2.58 -3.27)
			(end 7.66 -3.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2e5c0b0f-435e-4182-8ce0-3d6350815692")
		)
		(fp_line
			(start 0.69 -3.27)
			(end 0.69 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2d5c0dd6-70f2-4d6b-9f62-463045338623")
		)
		(fp_line
			(start 4.391 -3.27)
			(end 4.391 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dd2ee54c-ea12-409c-9f8b-c9689d895736")
		)
		(fp_line
			(start 7.66 -3.27)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6d9f5112-4616-49ea-abee-dcc0827c7433")
		)
		(fp_line
			(start -2.71 1.51)
			(end 7.79 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "311e9b90-e805-4780-9589-17e425e93b4e")
		)
		(fp_line
			(start 7.79 1.51)
			(end 7.79 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f4dbeb9e-7b49-4092-bd1d-357500c7aa98")
		)
		(fp_line
			(start -2.71 -3.4)
			(end -2.71 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "db3c415c-a58a-431c-9e2b-5d53e5b2ea6e")
		)
		(fp_line
			(start 7.79 -3.4)
			(end -2.71 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ef1a0562-f043-497b-b13f-448cde3f97df")
		)
		(fp_line
			(start -2.46 1.25)
			(end 7.54 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e3c3e1f7-6f04-4594-b2e2-d103b115c6f7")
		)
		(fp_line
			(start 7.54 1.25)
			(end 7.54 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4e38dc06-a5af-4063-a831-c9446c31a0cc")
		)
		(fp_line
			(start -2.46 -1.88)
			(end 7.54 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "da2daaf6-308d-40a6-afdd-e5d72e2ccdd8")
		)
		(fp_line
			(start -2.46 -3.15)
			(end -2.46 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0461e41a-ab69-4819-9795-4b469bc90896")
		)
		(fp_line
			(start 0.69 -3.15)
			(end 0.69 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "161666cf-ff12-4654-9c04-5d59a466cfcb")
		)
		(fp_line
			(start 4.39 -3.15)
			(end 4.39 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "37eadce5-9648-4784-ab99-2d9678d1980b")
		)
		(fp_line
			(start 7.54 -3.15)
			(end -2.46 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "caeb2849-eced-49d9-a657-18549eae4141")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 -4.27 90)
			(layer "F.Fab")
			(uuid "bbb3421b-fcf6-487a-b8ec-38a98d0beb90")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/Triac Circuit/High_Voltage_L")
			(pinfunction "A1")
			(pintype "passive")
			(uuid "b4af7dea-9de5-4458-85a7-c37b86a59ac6")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/Triac Circuit/High_Voltage_Out")
			(pinfunction "A2")
			(pintype "passive")
			(uuid "4f4475e9-4d86-4b03-97d0-9a1b6bf04fb3")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(Q1-G)")
			(pinfunction "G")
			(pintype "input")
			(uuid "ce5b6edb-fb68-4125-a9b1-1d5e53f0032d")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "58867153-a750-4014-9142-6d8e4d585fc2")
		(at 48.1375 19.6 180)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q2"
			(at 0 -2.4 0)
			(layer "F.SilkS")
			(uuid "682a9c22-6356-441d-a7f8-e90affac61e9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BC818"
			(at 0 2.4 0)
			(layer "F.Fab")
			(uuid "9ed8b38a-f47b-4e8e-8f9f-1b4152e52320")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "b5e3a53f-fb61-45e9-a640-11cd8c59eb6f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC818-D.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "7dd0df73-c58d-4014-b0fe-d77900d3bb30")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "ffff83a2-8b6f-4cce-aba7-bcaa752b52f1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/84e52baa-d126-4c4f-b1c5-63bb27b07c2b/00e550ea-8431-483d-ac3c-b4a719825546")
		(sheetname "Triac Circuit")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 1.56)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c7e1a7a8-dfda-4894-942c-d4276e56bc46")
		)
		(fp_line
			(start 0 1.56)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b778ed46-305e-4e50-adc2-ea6f44ef16e9")
		)
		(fp_line
			(start 0 -1.56)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4d7ceaf8-0a40-4731-a64b-738211a314dd")
		)
		(fp_line
			(start 0 -1.56)
			(end -1.675 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2c113f63-88dc-45fb-993d-89ab1c8b48a3")
		)
		(fp_line
			(start 1.92 1.7)
			(end 1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2501f449-d2f3-4f09-973c-15f425dbcf34")
		)
		(fp_line
			(start 1.92 -1.7)
			(end -1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "58e84f2f-d51b-412b-8423-6ca197eb6116")
		)
		(fp_line
			(start -1.92 1.7)
			(end 1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fa963c7e-beca-4913-a98c-a2898f060e5e")
		)
		(fp_line
			(start -1.92 -1.7)
			(end -1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9aba2c46-2500-4859-881f-0777e0035edc")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0b8c84da-17f9-4a1b-b847-cb9704086cb9")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "57950bae-15c9-459e-b485-17cbdab81fd1")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c42927ec-0298-4335-a462-79990776dcc3")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8803d8a0-1571-4368-829a-ad2086f22c1c")
		)
		(fp_line
			(start -0.65 -1.125)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "13e5e0b1-0c3e-4074-a082-4e2359d83807")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b77f6b5b-84cf-4fac-a324-fbbe8a6692c0")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 40 "Net-(Q2-B)")
			(pinfunction "B")
			(pintype "input")
			(uuid "75d2aa63-91ed-4835-945d-43a844972103")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "GND")
			(pinfunction "E")
			(pintype "passive")
			(uuid "4c26600d-4a40-4f8e-9fea-5d6030a619a9")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 44 "Net-(Q2-C)")
			(pinfunction "C")
			(pintype "passive")
			(uuid "6ce68dd4-958a-4cf6-a225-f2692378aea2")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
		(layer "F.Cu")
		(uuid "5cf9a8f8-8d0c-4d56-aee3-5fefebf5207d")
		(at 25.142855 20.4 -90)
		(descr "Terminal Block Phoenix MKDS-3-2-5.08, 2 pins, pitch 5.08mm, size 10.2x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-3-2-5.08 pitch 5.08mm size 10.2x11.2mm^2 drill 1.3mm pad 2.6mm")
		(property "Reference" "J1"
			(at 3.1 -3 90)
			(layer "F.SilkS")
			(uuid "06c6a5b3-683e-493e-bef1-555b681408d7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 2.54 6.36 -90)
			(layer "F.Fab")
			(uuid "66569049-bdaf-420e-8b66-3fb9f09d260a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "3c1a16c6-cc11-4550-9de7-f27c62067b7f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "f56f7d8b-4795-4de9-9d28-d89df09c6b3b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "78ba6983-43f5-40a1-b8c5-a1ad5ac53478")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/84e52baa-d126-4c4f-b1c5-63bb27b07c2b/60e4d8a3-c16e-48cd-a1fd-61f2968ecc7b")
		(sheetname "Triac Circuit")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.84 5.6)
			(end -2.34 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "309751d9-182e-4e3a-9a87-2c86041e7e7f")
		)
		(fp_line
			(start -2.6 5.36)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2cb4bf08-0def-4ae8-9da3-9e9e9a893e6b")
		)
		(fp_line
			(start -2.84 4.86)
			(end -2.84 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5713edc4-dbd3-4fd4-99ec-4a62b2c2ad57")
		)
		(fp_line
			(start -2.6 4.8)
			(end 7.68 4.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "216f9283-073d-4d83-9d5e-4a9b3cfaa77d")
		)
		(fp_line
			(start -2.6 2.3)
			(end 7.68 2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "67d201a8-4167-44d6-a7d5-2d0f1f1dfbef")
		)
		(fp_line
			(start -1.282 1.547)
			(end -1.388 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e80dadbd-77fc-4d88-9e6e-19ca7cd271e5")
		)
		(fp_line
			(start -1.548 1.281)
			(end -1.654 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6f28794f-e4e7-4238-a585-7b3ce1ba0c25")
		)
		(fp_line
			(start 4.073 1.274)
			(end 3.693 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "56096aa8-3d5d-440a-b9bc-2e2e57cb3d73")
		)
		(fp_line
			(start 3.822 0.992)
			(end 3.427 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2c08ae74-7b9c-4e04-bd10-6f9ddc1e0017")
		)
		(fp_line
			(start 1.654 -1.388)
			(end 1.547 -1.281)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7d60b79e-e2e0-4274-91cc-ac4089db3510")
		)
		(fp_line
			(start 6.734 -1.388)
			(end 6.339 -0.992)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "120ae78b-1541-47dd-a3aa-0c4a4d8bbe9f")
		)
		(fp_line
			(start 1.388 -1.654)
			(end 1.281 -1.547)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e124c697-dd1c-465c-a026-02eae88f7ffd")
		)
		(fp_line
			(start 6.468 -1.654)
			(end 6.088 -1.274)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8c3611ac-fba8-401e-9b8b-fa08afdc4a61")
		)
		(fp_line
			(start -2.6 -3.9)
			(end 7.68 -3.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e54ebade-ef60-4ae1-a202-2eaed4e86ac9")
		)
		(fp_line
			(start -2.6 -5.96)
			(end -2.6 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c230e031-725c-4fd3-b219-c48ae4a57383")
		)
		(fp_line
			(start -2.6 -5.96)
			(end 7.68 -5.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3ac23d14-71f6-43df-bbc5-a8a8a270ecbe")
		)
		(fp_line
			(start 7.68 -5.96)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e8246ef0-4800-43fa-a1e7-20b3180096a5")
		)
		(fp_circle
			(center 0 0)
			(end 2.18 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "c0e089c3-7715-4942-be02-fc405a86c126")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.26 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "df00e188-fcdf-43e1-8adc-23307a08e04f")
		)
		(fp_line
			(start -3.04 5.8)
			(end 8.13 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f58948ac-b42a-47c3-aa5d-52f63314a7f0")
		)
		(fp_line
			(start 8.13 5.8)
			(end 8.13 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3fceeb4e-0866-4e0f-b995-a48f909861be")
		)
		(fp_line
			(start -3.04 -6.4)
			(end -3.04 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "05cb48e2-4f4d-4b1f-89cd-0c72be354f85")
		)
		(fp_line
			(start 8.13 -6.4)
			(end -3.04 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ebc7a662-a90a-4fba-a1ea-d2ad72e5469d")
		)
		(fp_line
			(start -2.04 5.3)
			(end -2.54 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "82614943-8e0e-4335-b646-b1b533900bf3")
		)
		(fp_line
			(start 7.62 5.3)
			(end -2.04 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eee2e806-d09c-4456-808f-211cb9ac8e96")
		)
		(fp_line
			(start -2.54 4.8)
			(end 7.62 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "113c20c7-722e-4869-8253-e2fa28fd8ef1")
		)
		(fp_line
			(start -2.54 4.8)
			(end -2.54 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "513400c9-b37b-4f6e-9f2d-fce5c2d6d5a6")
		)
		(fp_line
			(start -2.54 2.3)
			(end 7.62 2.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1dc1ef10-fe8c-4cf9-a3e5-36cb26b61987")
		)
		(fp_line
			(start 1.517 -1.273)
			(end -1.273 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "90b96a4b-8774-414e-bb83-5573aae468f2")
		)
		(fp_line
			(start 6.597 -1.273)
			(end 3.808 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d00abd1a-7c0f-4e43-8e86-bc0966d28761")
		)
		(fp_line
			(start 1.273 -1.517)
			(end -1.517 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1d78752e-918d-492c-8ba2-9558391573c8")
		)
		(fp_line
			(start 6.353 -1.517)
			(end 3.564 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7154fd44-4bec-4c9e-a908-353430be81e4")
		)
		(fp_line
			(start -2.54 -3.9)
			(end 7.62 -3.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "594de972-8eb1-4ac1-99c2-75e34528a61f")
		)
		(fp_line
			(start -2.54 -5.9)
			(end 7.62 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8d0d7b39-34fe-45c1-899a-ef00a0c4546b")
		)
		(fp_line
			(start 7.62 -5.9)
			(end 7.62 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9cce208a-ce5b-4a18-874b-b0f19575cf00")
		)
		(fp_circle
			(center 0 0)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "4e03f0fb-d947-421e-9795-a6c3be6167e5")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.08 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "9be0e79e-f000-4aba-b78d-d2cc86d3f657")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 3.1 -90)
			(layer "F.Fab")
			(uuid "5dfe3b9d-6f63-4f2f-891a-eb829a695910")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/Triac Circuit/High_Voltage_L")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "4dcdb79b-5f48-4368-967f-d0db226688b8")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/Triac Circuit/High_Voltage_Out")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "8d432e52-0416-4a96-935f-8de9bf71ea57")
		)
		(model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "6140d072-b0e8-4b07-aaca-d27a6e8d4548")
		(at 48.566071 85.56)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "6638538f-f932-4bd6-8120-74a1546bc24e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "ef89a2e7-57a2-4e9b-991f-dd9c032265d6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "5e374e5e-6c31-4f64-b823-de7db0d0470f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6adb6f76-4645-4843-8407-0b9dc10f4133")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c9d984e3-fdac-40eb-8daa-21025db7aaa7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/e56f6699-6dcd-4f6f-a67f-2156f450d5f1/de24ad75-a874-4d54-a682-b1d6f2079d30")
		(sheetname "Triac Circuit4")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dada5c22-9373-4c37-8289-5a3f62e1ba4a")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "138f1fbb-621c-4b3d-866f-d0f01f5345b4")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dab6e69e-b04b-49de-a5b0-6bfd93d1b727")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "957f16fa-bb45-48bd-b5bf-f7830bc095a0")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d24c6be2-8ac7-45e1-8763-f7cece561b1e")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "98bed692-3cc3-491d-9ff4-00c72419b228")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3afa396b-8049-437a-a3d8-2e32d0a9ef0b")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "898d376c-b19a-4b12-81af-46bfa82eef7a")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1897c6f0-0029-4a73-959a-e649eb302704")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c2967859-8d1a-4f04-bc79-f379b9f42772")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "4439d3b2-c461-456a-a7ae-08ca2cfba33e")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 113 "Net-(R14-Pad1)")
			(pintype "passive")
			(uuid "06e30020-3c0b-4f60-8a20-1c9553f609aa")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 37 "+3V3")
			(pintype "passive")
			(uuid "24dca066-d001-4b61-9333-c835b9072dea")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "631167f5-11a2-46cd-80e9-ce323cd1eec7")
		(at 48.571429 113.84)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R21"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "295ef628-c172-4ca6-b849-68bed9ee0fd3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at -3.64 0 0)
			(layer "F.Fab")
			(uuid "cef193f8-2ef3-4354-968c-c85e0a458480")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d96fc900-3ad9-48b2-bdcf-93cd47eb5c5d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "60cc25a0-28c8-4a6c-8523-d6e52371b527")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ffeb42a8-6a5e-486e-a9ec-25809bde3f90")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/4a841339-199f-4bc7-a6bd-fe2a9936827c/ca31a324-056f-45d6-b948-82e97db62734")
		(sheetname "Triac Circuit6")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "864830c7-6e74-464c-9714-07feda4a225a")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "79395739-5b58-4aae-aef4-d23a7b2201c1")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f772600e-0a79-4334-9a2c-f939adb9f123")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "74431cdb-becf-4371-bc33-f12440bb6a8f")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ba3a3e4f-d4a5-47f8-af26-edcfc7202ede")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9f29fe8b-aeb2-4a87-ac21-421acd3d0294")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f65a8ff4-9ef5-4c4b-b009-ce0c191676f3")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4c948936-5cf5-4724-8bae-d406483597f4")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4e1e4056-bdea-443a-a4bc-23adfcd1398a")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a04c2fb6-47c0-447b-8853-4d3b4de121f6")
		)
		(fp_text user "${REFERENCE}"
			(at 3.04 0.01 0)
			(layer "F.Fab")
			(uuid "1399f001-fcc8-44ad-93cd-45f556537d9b")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 72 "Net-(Q14-B)")
			(pintype "passive")
			(uuid "202c767e-2e2a-4c2c-8882-e5163666a93f")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 31 "/Triac Circuit6/Enable")
			(pintype "passive")
			(uuid "db4b3fd7-8808-4be0-88b9-faa4d762c095")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(uuid "673f1a23-6661-4620-90df-f91c1a23f2f1")
		(at 66.942855 40.7 -90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R28"
			(at 3.809999 -1.92 -90)
			(layer "F.SilkS")
			(uuid "73ebc6da-2ddb-49ec-9ee2-635f0b90dbc3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "180"
			(at 3.81 1.919999 -90)
			(layer "F.Fab")
			(uuid "136a9584-b430-434f-a646-1cb3a90d1fd0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "013d7377-ea58-41c8-bfa0-2a1b46e219eb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4cc40aa9-ad95-4db7-b220-6af4d934a337")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3a690344-2834-4e17-b8c1-ceb174029762")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/f251f0b5-0f8b-4418-bbfe-69d55a4bdeb8/4ab64e29-964f-40b2-bf58-c546b31cd3eb")
		(sheetname "Triac Circuit9")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.89 0.92)
			(end 5.73 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ffee72ab-5512-4e36-aba1-2c5d5600574f")
		)
		(fp_line
			(start 5.73 0.92)
			(end 5.73 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "30d3b3ea-c41c-4b0e-a4d2-bbe7c9a6242e")
		)
		(fp_line
			(start 0.94 0)
			(end 1.89 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3fe9fce4-ea14-46a0-ab4b-0ef24750aa78")
		)
		(fp_line
			(start 6.68 0)
			(end 5.73 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c66b001f-0e30-46c4-a92d-42a8b4e16c27")
		)
		(fp_line
			(start 1.89 -0.92)
			(end 1.89 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "21003c6d-36e0-424b-a08f-28bd000f35da")
		)
		(fp_line
			(start 5.73 -0.92)
			(end 1.89 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6e7b8211-1cf6-4937-84d5-dbe0bce7643c")
		)
		(fp_line
			(start -0.95 1.05)
			(end 8.57 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c055ed88-108d-4bec-b1ab-b9a36eeef867")
		)
		(fp_line
			(start 8.57 1.05)
			(end 8.57 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ac28fae6-f6b3-44b5-b59d-fdab9065f2fb")
		)
		(fp_line
			(start -0.95 -1.05)
			(end -0.95 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6fd3f879-f1e7-4f90-a50b-2cc3161fb838")
		)
		(fp_line
			(start 8.57 -1.05)
			(end -0.95 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7f8c428a-bd5f-46a1-a22d-4c9c11a14da0")
		)
		(fp_line
			(start 2.01 0.8)
			(end 5.61 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "369b9afc-5cf5-43e8-bc71-ec2bc5e00b74")
		)
		(fp_line
			(start 5.61 0.8)
			(end 5.61 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2cd7b204-e529-4294-930c-946216cd53e7")
		)
		(fp_line
			(start 0 0)
			(end 2.01 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c5b03551-cc49-46c9-9a21-d68d109a15b1")
		)
		(fp_line
			(start 7.62 0)
			(end 5.61 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6e6f55fb-28b6-4398-badc-50b2d8a7a3e2")
		)
		(fp_line
			(start 2.01 -0.8)
			(end 2.01 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "de6c4f1b-8469-447a-a6f2-d03655bcc44e")
		)
		(fp_line
			(start 5.61 -0.8)
			(end 2.01 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2a49e47c-0940-43db-a5f7-b1b833bd9922")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 -90)
			(layer "F.Fab")
			(uuid "6a6f1d40-6abb-46a9-9dc7-1bde25c28ddd")
			(effects
				(font
					(size 0.72 0.72)
					(thickness 0.108)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "Net-(R28-Pad1)")
			(pintype "passive")
			(uuid "fdd527e0-ebc1-4384-a8a8-ed5e593c26d0")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "/Triac Circuit9/High_Voltage_L")
			(pintype "passive")
			(uuid "2048db1e-b5f6-4dab-8192-e3b9668f738f")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "684607bd-211e-40d9-a47f-bb3e33b20117")
		(at 47.994645 50.08 180)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q6"
			(at 0 -2.4 0)
			(layer "F.SilkS")
			(uuid "4ff56fa2-3c3a-4373-ade0-3785a916b8df")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BC818"
			(at 0 2.4 0)
			(layer "F.Fab")
			(uuid "a9874138-47d6-4717-8d84-1db5054334fe")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "344e2cd5-033d-43d0-8413-9b6129f552a8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC818-D.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "0be9786a-9e10-4858-ac62-a1cb9fed963f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "4c41f99f-647f-40f3-9410-e81fd8b86aa0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/fef2553d-539f-40e4-b7bd-376e44ab9a6f/00e550ea-8431-483d-ac3c-b4a719825546")
		(sheetname "Triac Circuit2")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 1.56)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a5b62c69-1530-4ecb-8e6e-fe9b91bbaf5e")
		)
		(fp_line
			(start 0 1.56)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "29c9ab3c-179d-4a21-983e-789d5802bcd7")
		)
		(fp_line
			(start 0 -1.56)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4aaa8103-5b4d-4edd-85a8-30b9e80ac82b")
		)
		(fp_line
			(start 0 -1.56)
			(end -1.675 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ab67e45d-14f8-48b3-b4c0-7884c02ae89c")
		)
		(fp_line
			(start 1.92 1.7)
			(end 1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "efc90e55-63df-41f9-9816-3670eb46d7ee")
		)
		(fp_line
			(start 1.92 -1.7)
			(end -1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3776a875-86aa-4650-a200-273f1cda3915")
		)
		(fp_line
			(start -1.92 1.7)
			(end 1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f9c32a29-a822-4724-a643-d39c14a0f54e")
		)
		(fp_line
			(start -1.92 -1.7)
			(end -1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3111d343-97f9-49fb-a847-612a93b84511")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "15a35f11-d3ab-404a-a5b0-c9d7154da534")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "815b72e2-7d82-4923-9f16-1cc74f6eaf4b")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5d323f8c-85db-4029-af0a-53671a049e20")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0c199c3e-1524-4fcc-a6b3-d7f6badf958f")
		)
		(fp_line
			(start -0.65 -1.125)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9bd5c299-c1d9-40d4-b761-370ae0130323")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "e74d9745-c487-4c4d-a93e-669a906b2dab")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 53 "Net-(Q6-B)")
			(pinfunction "B")
			(pintype "input")
			(uuid "0e2d0eb3-e758-422d-8f55-28a46eb97228")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "GND")
			(pinfunction "E")
			(pintype "passive")
			(uuid "1cc8da55-bbd6-478a-bead-eb959f2937a0")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 56 "Net-(Q6-C)")
			(pinfunction "C")
			(pintype "passive")
			(uuid "a6fb8178-832d-4f41-8c17-2e7b218ded53")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "684befe8-dac4-40e1-b237-1d5bd7669ea2")
		(at 69.2625 179.6)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "D2"
			(at 0 -2.4 0)
			(layer "F.SilkS")
			(uuid "8713886d-555b-4370-8b13-4a1b90825512")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MMBZxx"
			(at 0 2.4 0)
			(layer "F.Fab")
			(uuid "00cc30fc-a7b0-4bed-b504-b542f28c5051")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "626b62d8-4687-47ef-ae8d-29cb106c877c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/MMBZ5V6ALT1-D.PDF"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "011881df-f7fd-4b7a-9b2e-877bede2d214")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Double Zener Diode, Common Anode, 225mW, SOT-23"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "63639bba-d2de-4fcc-ae16-b1afad831f9f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/fc3afc4a-653b-4560-bf07-0ff91e73ac09")
		(sheetname "Główny")
		(sheetfile "16_ChannelPowerControlBoard.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -1.56)
			(end -0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "93cdc4a2-ad70-4a4c-87c9-188890b5b304")
		)
		(fp_line
			(start 0 -1.56)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "68cc6757-7d12-49cb-900b-ab3cbde54bda")
		)
		(fp_line
			(start 0 1.56)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "29f0a774-2055-4822-9f31-3f58d24f6efb")
		)
		(fp_line
			(start 0 1.56)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "40fdc86e-40ec-46b0-95c7-4fd52ac62cef")
		)
		(fp_poly
			(pts
				(xy -1.1625 -1.51) (xy -1.4025 -1.84) (xy -0.9225 -1.84) (xy -1.1625 -1.51)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "77d51bbb-c9e4-4c0e-afa8-e42d0343cadf")
		)
		(fp_line
			(start -1.92 -1.7)
			(end -1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "950269ce-6c59-4034-88cf-5aec2fad0c80")
		)
		(fp_line
			(start -1.92 1.7)
			(end 1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dfa4fdf2-a0b8-4247-b31b-5166e154b128")
		)
		(fp_line
			(start 1.92 -1.7)
			(end -1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b71c75da-3022-4396-ab32-2bf79dd0850e")
		)
		(fp_line
			(start 1.92 1.7)
			(end 1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ef633e98-a040-4c5b-929c-c6fbf0be9e41")
		)
		(fp_line
			(start -0.65 -1.125)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8d428fc5-43aa-406e-8d3e-97df6b192e42")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "61e9400f-b70c-44fd-9c6a-bf1c92743f14")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "19ebeec6-d09f-48d7-baab-fed42dac71e2")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d8adcc7e-c402-4b8a-9edc-18f6192d3854")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "78b3b3a2-f04b-4228-ad3d-7bb0b95f08c4")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c337cc26-0b6c-4a4a-9e43-d29b15f07950")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 182 "Net-(U1-CANH)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "4a1eec59-1038-4c18-ac5a-aeb11af2f87a")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "GND")
			(pinfunction "K")
			(pintype "passive")
			(uuid "11dd4503-545c-434a-8194-95b1b855ac51")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 183 "unconnected-(D2-A-Pad3)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "ab84ff51-6045-41b2-b264-fb0008b84b07")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "68ca4a1f-b166-44e4-9de4-921cc676e25e")
		(at 48.166071 80.56 180)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q10"
			(at 0 -2.4 0)
			(layer "F.SilkS")
			(uuid "3e20fc98-12fc-4fe3-930a-bd9801023bf3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BC818"
			(at 0 2.4 0)
			(layer "F.Fab")
			(uuid "a9dcf096-dd6a-43cc-8567-6362956bae15")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "c817801b-7dfd-457a-be7e-be4d8ea09ba0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC818-D.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "48224de9-a309-41b5-bb0d-d62543ca233c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "016a0aec-ccb2-48c9-b04e-b228dc0af758")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/e56f6699-6dcd-4f6f-a67f-2156f450d5f1/00e550ea-8431-483d-ac3c-b4a719825546")
		(sheetname "Triac Circuit4")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 1.56)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "25b0599a-1ed6-4c03-bb89-4622a60c8ff7")
		)
		(fp_line
			(start 0 1.56)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bb0a950f-0d7b-43fb-a3ee-2ca8ccac57e0")
		)
		(fp_line
			(start 0 -1.56)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0dbaf6a3-e6d0-4931-86f3-6b8122e99059")
		)
		(fp_line
			(start 0 -1.56)
			(end -1.675 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "53d1981b-2be0-4ce9-9317-f14ac470e00c")
		)
		(fp_line
			(start 1.92 1.7)
			(end 1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "77bf71e0-1de5-4331-b769-823f4e6e60dc")
		)
		(fp_line
			(start 1.92 -1.7)
			(end -1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "77f990f4-84b6-42c3-a934-3e0593ca79bd")
		)
		(fp_line
			(start -1.92 1.7)
			(end 1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "64f1052f-2d64-4b6d-b458-ea4cce0fd72b")
		)
		(fp_line
			(start -1.92 -1.7)
			(end -1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b35d52be-4bc1-4fbf-934f-e932ba99e191")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "26f5c307-0783-45ce-9c48-b42971b92cb5")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e86d021b-277a-44b1-88d8-f49dcaa0df9a")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d3eaa2fb-4a08-4147-91a1-67452ec242a4")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "437b2a6a-489b-444e-89d4-37ca71221ee8")
		)
		(fp_line
			(start -0.65 -1.125)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "83cfae4f-ce33-483e-ab3f-74391d798f84")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "eb8600c0-9370-4b01-b0e8-0aa2daefef2c")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 62 "Net-(Q10-B)")
			(pinfunction "B")
			(pintype "input")
			(uuid "73aac6cf-f83f-41b5-97c7-d78d5e90af96")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "GND")
			(pinfunction "E")
			(pintype "passive")
			(uuid "c6f027bf-f46c-47ba-b250-7e31420da479")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 66 "Net-(Q10-C)")
			(pinfunction "C")
			(pintype "passive")
			(uuid "24d388ea-a7d9-4383-807d-2a2d277eeae9")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "694fd5f4-c111-44b1-b42c-1b87063c8ba5")
		(at 48.542858 37.64)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "2a9dc246-15a7-4c3b-a212-00808becdc42")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at -3.64 0 0)
			(layer "F.Fab")
			(uuid "ebf85c8b-1212-4d36-a69f-ecfe45ed0201")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "2bc4638a-7da4-4022-8124-292091472375")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c4a44f91-022e-489d-836a-76cdd2403fea")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "15ea0e93-5af1-4327-aea3-4bf422e8679f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/98cc9bb7-a6bb-4cad-bced-cd34a966891d/ca31a324-056f-45d6-b948-82e97db62734")
		(sheetname "Triac Circuit1")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5b6da1c6-acae-4ca8-87c1-426b8c553f9b")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b3540e45-a8cd-4dc7-8320-bbe8c718bdc3")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b6a00288-eda4-46a7-98c9-610b357038a0")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4fa2b0ed-8ed3-4071-8348-75ae75d4ae52")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6686c5fd-67b3-4c26-a60c-b979aa371890")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "706b9dd2-3531-464e-accb-a6626ab67dbc")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "97207351-f8d4-4db3-9d58-7a9819e97ecc")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "70e27f74-f7b1-45cd-a08a-ab1763b1011f")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a179d7fa-c961-4242-a060-754a50ffd1ea")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2f6cbfe8-42c7-4e33-ba50-e35c68da5d9a")
		)
		(fp_text user "${REFERENCE}"
			(at 3.04 0.01 0)
			(layer "F.Fab")
			(uuid "310c88ea-f936-439c-9bd2-56d5c9f1341b")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 46 "Net-(Q4-B)")
			(pintype "passive")
			(uuid "e87240fd-bc12-4873-bb37-c0f4e2a13cfd")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 22 "/Triac Circuit1/Enable")
			(pintype "passive")
			(uuid "09a01d93-288f-4506-a562-b85215b34258")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(uuid "697a2a42-69fd-436b-8fcf-3eb612b271b7")
		(at 66.942855 71.18 -90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R34"
			(at 3.809999 -1.92 -90)
			(layer "F.SilkS")
			(uuid "82f3d60a-6ed4-40ca-92ea-fb7c9d5ce5e6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "180"
			(at 3.81 1.919999 -90)
			(layer "F.Fab")
			(uuid "c35b0046-cfdd-43c9-a2b7-a71b31204120")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ea070f9e-c8cd-422c-ba85-cf572517cba5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7330333f-1bc5-4c24-b1e2-3b82670b7449")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "09dc0e79-2fc6-46d2-ba7e-de0fb05ed29e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/15d8fe7c-2a9b-438f-a777-3e4687188af1/4ab64e29-964f-40b2-bf58-c546b31cd3eb")
		(sheetname "Triac Circuit11")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.89 0.92)
			(end 5.73 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "83d888ee-b8c6-44d8-89ab-7f565209cff3")
		)
		(fp_line
			(start 5.73 0.92)
			(end 5.73 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "00770962-4e52-4163-8004-8f62cfbca153")
		)
		(fp_line
			(start 0.94 0)
			(end 1.89 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e0b5a63e-12c4-46d9-994e-d8ac78b91101")
		)
		(fp_line
			(start 6.68 0)
			(end 5.73 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "37831d34-fa36-4126-a844-d63374764870")
		)
		(fp_line
			(start 1.89 -0.92)
			(end 1.89 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f0208f79-ca60-4bea-b8c3-5c4a4672535d")
		)
		(fp_line
			(start 5.73 -0.92)
			(end 1.89 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4a5b8e4b-ff35-468b-97b4-ef7f357c8f4f")
		)
		(fp_line
			(start -0.95 1.05)
			(end 8.57 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "23be35f0-0c63-4a20-96f7-730ca0b2d44f")
		)
		(fp_line
			(start 8.57 1.05)
			(end 8.57 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "71ccd979-b966-4a5b-aefc-d9e17cf3813a")
		)
		(fp_line
			(start -0.95 -1.05)
			(end -0.95 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c71c6ab9-cb57-4f81-9d70-09e7d00bd746")
		)
		(fp_line
			(start 8.57 -1.05)
			(end -0.95 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3c22d671-3a15-4e91-9530-9373dfb1ae0a")
		)
		(fp_line
			(start 2.01 0.8)
			(end 5.61 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ef49308e-9ef6-4c88-8226-485e4ac877af")
		)
		(fp_line
			(start 5.61 0.8)
			(end 5.61 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6d1a3fc5-9152-4a7c-9ce0-95e51cdf0902")
		)
		(fp_line
			(start 0 0)
			(end 2.01 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "276a687a-1340-49d4-8c90-c2dca3356e49")
		)
		(fp_line
			(start 7.62 0)
			(end 5.61 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4d9cf2da-9bb1-43dc-847e-5331cdb3dee7")
		)
		(fp_line
			(start 2.01 -0.8)
			(end 2.01 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b235bdbc-18a7-4d6a-8dd0-5da55ed2bf6f")
		)
		(fp_line
			(start 5.61 -0.8)
			(end 2.01 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "83e4cfc1-6369-4914-aa0b-388860f72bc5")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 -90)
			(layer "F.Fab")
			(uuid "92a6bb7b-1048-492e-b5e9-32a8a9603e78")
			(effects
				(font
					(size 0.72 0.72)
					(thickness 0.108)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "Net-(R34-Pad1)")
			(pintype "passive")
			(uuid "97019155-25a4-49bc-a4b9-632989d77b6d")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "/Triac Circuit11/High_Voltage_L")
			(pintype "passive")
			(uuid "694cebf9-6bdd-4103-8a2b-588c96ec772c")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "6a8966b6-9610-4b5c-a019-337ab9285a9b")
		(at 48.451787 131.28)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R23"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "26304721-3025-4167-b313-a19b4e457048")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "a11b0b34-46f6-4093-b130-6794fa4510ac")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0357d3a3-af41-4f0b-8323-a084b11122d9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ceac36d8-abd9-4429-a404-9bdbbac9ebe4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8b5ca446-46b7-46ca-a3ab-88e1b7b9fc8a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/6df26bae-1f6b-42ab-99b6-42742cd98df0/de24ad75-a874-4d54-a682-b1d6f2079d30")
		(sheetname "Triac Circuit7")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "11173a2a-fdb2-4eba-8e37-3a011a23ae81")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "de31db1f-f5ca-4beb-9035-29f8fbd23108")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "de3f92e0-4878-4399-9347-02c3c08fe336")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "90df1fd2-e5b5-44a8-82fb-4b45c3cac27a")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b82579e7-51cb-46ae-b9fa-6edc2ed4584b")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "37cffda0-972f-4614-afd8-624d227d8789")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f5c178f6-b94a-4f43-8110-1487be45993d")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a588503f-bfbe-4ef3-8416-c64f4500177d")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2980d5df-44e6-4da9-ab83-93b412dbc91e")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "42353731-ab6b-4616-8d2c-88bc8f815665")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "112681f3-2309-41e7-ab4d-ca7f67ed5762")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 116 "Net-(R23-Pad1)")
			(pintype "passive")
			(uuid "78cb64ca-e798-45a8-84a7-ba9cc81bb085")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 37 "+3V3")
			(pintype "passive")
			(uuid "aa72883f-dbae-4c82-a017-56e4f58e6892")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
		(layer "F.Cu")
		(uuid "7508fc71-447c-46db-bfcd-4c7d109fb777")
		(at 77 106.6 90)
		(descr "Terminal Block Phoenix MKDS-3-2-5.08, 2 pins, pitch 5.08mm, size 10.2x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-3-2-5.08 pitch 5.08mm size 10.2x11.2mm^2 drill 1.3mm pad 2.6mm")
		(property "Reference" "J14"
			(at 3.1 -2.999999 -90)
			(layer "F.SilkS")
			(uuid "f634bf8c-571f-4822-ab7f-158b8d4c6b16")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 2.539999 6.36 90)
			(layer "F.Fab")
			(uuid "dd3a965d-5f6b-41b5-891c-56701d202214")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "bfd68037-095c-4d96-9acd-a53f21eda69c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "b935bcf3-4c2f-4c1b-824e-92e2fe397cf6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "d28bf017-e444-4884-aa6b-22c5cab283ca")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/4a948621-4b4c-41c9-b07f-b928eecc9e1e/60e4d8a3-c16e-48cd-a1fd-61f2968ecc7b")
		(sheetname "Triac Circuit13")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 7.68 -5.96)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aaee1d20-ccf5-48f3-9bb5-e5ecb0069759")
		)
		(fp_line
			(start -2.6 -5.96)
			(end 7.68 -5.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "802558a7-7611-44a3-9da1-06fdd2a97718")
		)
		(fp_line
			(start -2.6 -5.96)
			(end -2.6 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "50f3bec8-7d55-4de4-b222-5f0e47eb3542")
		)
		(fp_line
			(start -2.6 -3.9)
			(end 7.68 -3.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1d6e4ab8-e9d6-46b8-bfa5-1597993c60b7")
		)
		(fp_line
			(start 6.468 -1.654)
			(end 6.088 -1.274)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1c3c539a-1999-467f-accb-0a932da2240c")
		)
		(fp_line
			(start 1.388 -1.654)
			(end 1.281 -1.547)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fd48d3c5-5f38-40ca-aa9a-db44b86443b5")
		)
		(fp_line
			(start 6.734 -1.388)
			(end 6.339 -0.992)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8eff4418-02cb-4748-9294-6683775e0c32")
		)
		(fp_line
			(start 1.654 -1.388)
			(end 1.547 -1.281)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1d8848c4-4375-4828-8796-7ba62c412778")
		)
		(fp_line
			(start 3.822 0.992)
			(end 3.427 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "613e6078-9dce-4e13-8d1e-63db2d932f25")
		)
		(fp_line
			(start 4.073 1.274)
			(end 3.693 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "731bb622-e8c1-4ad5-92aa-d2a8d5f74c4b")
		)
		(fp_line
			(start -1.548 1.281)
			(end -1.654 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f74b1901-ed1c-41ad-9403-057f78ac29ed")
		)
		(fp_line
			(start -1.282 1.547)
			(end -1.388 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "98b6514a-b5ab-4929-a5cc-19112b47e9ea")
		)
		(fp_line
			(start -2.6 2.3)
			(end 7.68 2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "01b9abea-e95e-421e-83db-3e9d0996d8bc")
		)
		(fp_line
			(start -2.6 4.8)
			(end 7.68 4.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "baa955b9-6ba6-452b-9b4a-c7afddf4019c")
		)
		(fp_line
			(start -2.84 4.86)
			(end -2.84 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2b6d724e-d816-4de6-8d23-d93a52afec17")
		)
		(fp_line
			(start -2.6 5.36)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b0f8b419-119f-41ba-9f1a-1382b25493e1")
		)
		(fp_line
			(start -2.84 5.6)
			(end -2.34 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "67c17864-ec3e-4374-84b8-041b1b4cf990")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.26 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "bd8734e5-401e-47d2-a710-1985f40a3c3d")
		)
		(fp_circle
			(center 0 0)
			(end 2.18 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "c3f9cc43-617c-4857-a03f-2aa21dd67829")
		)
		(fp_line
			(start 8.13 -6.4)
			(end -3.04 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d2f99e95-5017-468d-a1d7-80b05ac0795e")
		)
		(fp_line
			(start -3.04 -6.4)
			(end -3.04 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "37a08eeb-0498-4901-aed0-51998b2c5f44")
		)
		(fp_line
			(start 8.13 5.8)
			(end 8.13 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "53e197ee-d04d-43ee-9718-f88a19771f8b")
		)
		(fp_line
			(start -3.04 5.8)
			(end 8.13 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "46cc946e-0887-4a95-a2da-4594ed4e02c9")
		)
		(fp_line
			(start 7.62 -5.9)
			(end 7.62 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f58406e4-4048-41bc-a56c-19b55ca29dbf")
		)
		(fp_line
			(start -2.54 -5.9)
			(end 7.62 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c2a4646a-9310-494a-aff2-7b09edced54d")
		)
		(fp_line
			(start -2.54 -3.9)
			(end 7.62 -3.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2a90cae3-44fc-4d66-bd0d-68f914a7b601")
		)
		(fp_line
			(start 6.353 -1.517)
			(end 3.564 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4efb1c05-3260-44aa-9a10-1c820090e346")
		)
		(fp_line
			(start 1.273 -1.517)
			(end -1.517 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dbf84198-d4ed-4633-b34e-920e2cb6f6a1")
		)
		(fp_line
			(start 6.597 -1.273)
			(end 3.808 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8c779d64-6408-46df-bfdb-51fef9b0bd17")
		)
		(fp_line
			(start 1.517 -1.273)
			(end -1.273 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "996aaad5-938f-4650-838b-f688c9586f3b")
		)
		(fp_line
			(start -2.54 2.3)
			(end 7.62 2.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0efef3d0-728f-4cf2-96bd-66950e8ea4e2")
		)
		(fp_line
			(start -2.54 4.8)
			(end -2.54 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "df96a11a-4dac-4447-ba73-12b1b0bc10e9")
		)
		(fp_line
			(start -2.54 4.8)
			(end 7.62 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f0a7ff1c-859b-4ec6-ae36-9329e9ecec73")
		)
		(fp_line
			(start 7.62 5.3)
			(end -2.04 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fd2aa157-1bc6-4dc4-9002-83aceaa926ad")
		)
		(fp_line
			(start -2.04 5.3)
			(end -2.54 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7a60909c-ec2e-41d6-8034-b9aa70609b18")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.08 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "81431303-3590-4eae-a95b-64803288d02d")
		)
		(fp_circle
			(center 0 0)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "568c8722-4c1f-4651-b8b6-248481255078")
		)
		(fp_text user "${REFERENCE}"
			(at 2.539999 3.1 90)
			(layer "F.Fab")
			(uuid "e39fb411-c75f-4b1b-9d25-edc1219ed72c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 85 "/Triac Circuit13/High_Voltage_L")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "59da9697-ffe9-4cb4-b8fc-422afb9493ba")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/Triac Circuit13/High_Voltage_Out")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "e40fe98a-9a9f-4f8e-9a70-e0aa0d7fedb1")
		)
		(model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(uuid "752fc55c-e76e-432a-bc83-693481fcb78d")
		(at 35.057145 55.82 90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R7"
			(at 3.81 -1.92 90)
			(layer "F.SilkS")
			(uuid "054c1b85-9359-4a0e-90f2-54c777b09926")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "180"
			(at 3.81 1.92 90)
			(layer "F.Fab")
			(uuid "92e36513-98ff-499c-a850-cde4dc75aad2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "37eb3d60-bfd9-404e-9b56-7a2f535bd090")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4fa2cc7d-33b0-4568-b1a9-bd9fd94fe4a9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2747cae2-e520-4d07-86b1-fdbfb2b9b45c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/fef2553d-539f-40e4-b7bd-376e44ab9a6f/4ab64e29-964f-40b2-bf58-c546b31cd3eb")
		(sheetname "Triac Circuit2")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 5.73 -0.92)
			(end 1.89 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c1061824-0aa6-4a19-80ff-80e23520eb3f")
		)
		(fp_line
			(start 1.89 -0.92)
			(end 1.89 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3a470d24-994d-46fb-b840-c89a5e3acd9c")
		)
		(fp_line
			(start 6.68 0)
			(end 5.73 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "553e3752-4a9a-4a7c-9f31-781f8ba734cd")
		)
		(fp_line
			(start 0.94 0)
			(end 1.89 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "58f68de1-091a-471c-b214-64503e91f6c0")
		)
		(fp_line
			(start 5.73 0.92)
			(end 5.73 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f16b88a6-1838-4dd0-b092-8cb1863e7ef4")
		)
		(fp_line
			(start 1.89 0.92)
			(end 5.73 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "34359503-c6c6-45f8-be1d-68cf7ec4d6ef")
		)
		(fp_line
			(start 8.57 -1.05)
			(end -0.95 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3f2e600d-deed-406c-af45-bc17bbefc2d2")
		)
		(fp_line
			(start -0.95 -1.05)
			(end -0.95 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "97aee16a-65fc-41d2-a733-1b1700c5a9c0")
		)
		(fp_line
			(start 8.57 1.05)
			(end 8.57 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a8bc64ac-9bdd-455d-a1ed-31967f877e93")
		)
		(fp_line
			(start -0.95 1.05)
			(end 8.57 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "96d6ca9e-40f6-4b17-839c-5e5b4d6f29cd")
		)
		(fp_line
			(start 5.61 -0.8)
			(end 2.01 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7cb4d0b0-fe7c-459c-ae03-5eb54b142982")
		)
		(fp_line
			(start 2.01 -0.8)
			(end 2.01 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6f08ce61-4071-4abe-863e-27fd2e9ccbe2")
		)
		(fp_line
			(start 7.62 0)
			(end 5.61 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5177c27c-f90b-4026-92b0-8b89eac57c76")
		)
		(fp_line
			(start 0 0)
			(end 2.01 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "01a0a230-306c-4474-a899-ff56262b1758")
		)
		(fp_line
			(start 5.61 0.8)
			(end 5.61 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6ac7081a-45df-445f-ae7f-a5c9dd1adbc5")
		)
		(fp_line
			(start 2.01 0.8)
			(end 5.61 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dc53e54f-b624-4e52-a6bd-dce7bd065bfd")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
			(uuid "8879322b-cb8d-4fbf-a142-193403323fc7")
			(effects
				(font
					(size 0.72 0.72)
					(thickness 0.108)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "Net-(R7-Pad1)")
			(pintype "passive")
			(uuid "542ac014-d656-454e-ac87-f9b357449ae6")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/Triac Circuit2/High_Voltage_L")
			(pintype "passive")
			(uuid "74ef8f9e-15ca-436b-8799-0cbe95293627")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "78122292-07ad-49c4-b498-7401d1b7b596")
		(at 48.485716 68.12)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "76a45538-7d08-4c91-a8b1-e99187824be3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at -3.64 0 0)
			(layer "F.Fab")
			(uuid "46da584b-17e7-4565-bc9f-8b592fa475aa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c542fca5-d9ef-407b-adb5-de2f17807f4d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "605ec5ea-7cc3-4b45-bb30-356a3ab3eeb1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "781d6bc8-5df1-46b3-847d-10ce89f92c36")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1abc9394-30bb-4ef5-a1be-aa230dbd1566/ca31a324-056f-45d6-b948-82e97db62734")
		(sheetname "Triac Circuit3")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e2d92c44-d5f1-4abb-8fbb-b5f1dcb76fd8")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8747310d-7bb8-4685-acef-5aed659a8c76")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4281a0c9-fcd8-4a3a-b34c-1c027443b7aa")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "911e458a-c00a-4d73-b032-b38b455659b8")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3212c425-c411-4011-a581-8baffa4d28e1")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6819d8a4-bef4-4f32-b6cd-3b793390edf1")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f248b6d2-2118-4767-85b6-d07965d159e9")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0155977b-38c6-4d03-80d0-f61b117e1f83")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "15290291-2549-4336-a949-1259936bbab2")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4946c7fa-370b-450f-a712-0a10ad14f18e")
		)
		(fp_text user "${REFERENCE}"
			(at 3.04 0.01 0)
			(layer "F.Fab")
			(uuid "19bc7e7e-30d0-4e52-95e6-9bf7de2b568b")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 59 "Net-(Q8-B)")
			(pintype "passive")
			(uuid "60006d9a-50b7-4dff-aca9-8a3f0778cdc4")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 25 "/Triac Circuit3/Enable")
			(pintype "passive")
			(uuid "cc86ea4e-86cf-4f4f-9f48-04b49c4b5fd2")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-6_W7.62mm"
		(layer "F.Cu")
		(uuid "792bc067-c6b7-483e-8928-932cece83895")
		(at 57.142855 117.915)
		(descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U16"
			(at 3.599999 -2.33 180)
			(layer "F.SilkS")
			(uuid "0ba27d95-6f7e-46ce-951e-3c56f1e6c968")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MOC3021M"
			(at 3.81 7.409999 180)
			(layer "F.Fab")
			(uuid "55032069-73a9-482f-8693-096e71f76e9a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "47ab5b09-6b62-4fcc-a33b-eb93c9cd6ada")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3023M-D.PDF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f97ddd3d-a4dc-4ef4-8711-c24d6b227515")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9a9c6ca2-ba5f-41ab-9a8d-d0ad689f92e0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*")
		(path "/683a6cfc-1cb6-4c63-ae1f-c9d1fdc220d0/0262e914-5435-478f-be04-ece49b8102cf")
		(sheetname "Triac Circuit14")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d3d215e4-e8eb-4995-aae4-231dc8f54968")
		)
		(fp_line
			(start 1.16 6.41)
			(end 6.46 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "43d430b9-e1f3-4f89-888b-fe384ac1a501")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a2bc0192-6b90-4fc4-9a6c-575297fa7f54")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "71897ff1-eccb-4712-8a24-94f36c9cf2a4")
		)
		(fp_line
			(start 6.46 6.41)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "504f85a6-d7d0-4780-9b97-4ec3ccc5effc")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2c6b04de-c372-4fc4-8428-7755b68a4be7")
		)
		(fp_line
			(start -1.1 -1.55)
			(end -1.1 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d7e4f9b1-f941-4479-aace-935ab15a7e3c")
		)
		(fp_line
			(start -1.1 6.6)
			(end 8.7 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "60e4b632-b812-49ed-a35c-e3934eb6f7ac")
		)
		(fp_line
			(start 8.7 -1.55)
			(end -1.1 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "12ccb10b-72d8-439b-a7d9-16f3afc89703")
		)
		(fp_line
			(start 8.7 6.6)
			(end 8.7 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "041e55b9-bdfe-48f4-9da9-fa68b641e3d4")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "110eb0b3-9f42-413c-8554-8a7b4ffc0cfd")
		)
		(fp_line
			(start 0.635 6.35)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2091ce2b-f456-451f-b844-133e7e3705b6")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9f21c515-3aa1-44ad-b0f8-0fcea2912ecf")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a477772b-8ea4-4c71-b2b4-e23b5c5847a1")
		)
		(fp_line
			(start 6.985 6.35)
			(end 0.635 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5c25cc84-45d2-4ad7-91d1-b67f6b4b491c")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.539999 180)
			(layer "F.Fab")
			(uuid "a1cc9fe7-8874-4c75-8257-faf41b4e6787")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 125 "Net-(R44-Pad1)")
			(pintype "passive")
			(uuid "ea31f4bc-d9e6-4bc9-81f5-baf2d4b7a365")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 156 "Net-(Q30-C)")
			(pintype "passive")
			(uuid "b858d624-0634-4c8e-99c3-73c9f3f3653c")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "unconnected-(U16-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "86d28f27-0427-45d9-8892-6ac3b054beb1")
		)
		(pad "4" thru_hole oval
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 154 "Net-(Q29-G)")
			(pintype "passive")
			(uuid "3f7c3056-6d51-46c1-8d41-c6d038ed2ed5")
		)
		(pad "5" thru_hole oval
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 107 "unconnected-(U16-NC-Pad5)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "23b8dc77-329e-4fb0-add1-4a230cea097a")
		)
		(pad "6" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "Net-(R43-Pad1)")
			(pintype "passive")
			(uuid "ca74615d-f76c-41e8-8cd0-e0ac7fdcf05b")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-6_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "79e2f0c8-67c7-4822-912a-bfefb7447fda")
		(at 48.514287 129.08)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R24"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "5f23ccf3-ec1a-4dd1-8f0a-0430bcbee28b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at -3.64 0 0)
			(layer "F.Fab")
			(uuid "35c609f9-352f-4c85-9d67-585c7489a901")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b36a5907-b70d-4aa4-82a5-8c9d4d45bdbc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d4eb7dfb-ddad-40ac-8513-66e9f7be9cfa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "245e60dd-3af7-4b3e-a89d-da3a13aa88a8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/6df26bae-1f6b-42ab-99b6-42742cd98df0/ca31a324-056f-45d6-b948-82e97db62734")
		(sheetname "Triac Circuit7")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "260a063d-601d-4ab7-899e-b152bac081ed")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "23d35687-89bf-4cdc-87c6-80e91910a1b5")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "550c820d-e7db-4041-b6f7-f5c9700443db")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c6a4d814-3443-4e90-8c83-4f44c1c33a30")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6bd9f3aa-d4fa-4a08-8adf-fe9de5f6b829")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "841b60a4-3888-4360-a243-d963cd11ff0b")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "920b1566-9775-4a0f-87ef-e76c57484711")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "077ffb99-1963-4e46-a9b2-3ff435a9e6e6")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "56a6243c-1598-45e5-bfe0-832d04778962")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e0b7f899-9704-4714-ac7e-6f176d9f76bb")
		)
		(fp_text user "${REFERENCE}"
			(at 3.04 0.01 0)
			(layer "F.Fab")
			(uuid "6636101f-621a-4b4e-9672-a9efe1298b31")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 74 "Net-(Q16-B)")
			(pintype "passive")
			(uuid "b8b149e4-65a4-4964-83b6-fe55de9bebc9")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 32 "/Triac Circuit7/Enable")
			(pintype "passive")
			(uuid "706c7d9e-7199-40e6-b700-2d77bf0a1288")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-6_W7.62mm"
		(layer "F.Cu")
		(uuid "7a5c04d8-4b2a-42ea-93eb-f1a895105cb8")
		(at 57.142855 56.955)
		(descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U12"
			(at 3.599999 -2.33 180)
			(layer "F.SilkS")
			(uuid "dbd0bf2a-8083-47e5-baec-4c20fe4c729b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MOC3021M"
			(at 3.81 7.409999 180)
			(layer "F.Fab")
			(uuid "1c9173c9-1b13-4e1a-a767-50c3cb70e481")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0a83f088-133c-4e81-a021-5bf45521ec14")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3023M-D.PDF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "72b89f54-3342-4e85-9fe4-a14c283cb020")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3e5d786e-413c-4ea5-87c5-edebb27a277f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*")
		(path "/d20c900a-3d9a-4460-9d5d-3ed4d11c2b93/0262e914-5435-478f-be04-ece49b8102cf")
		(sheetname "Triac Circuit10")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c1d4cceb-cfd8-4c63-8da1-573e6f48d27c")
		)
		(fp_line
			(start 1.16 6.41)
			(end 6.46 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c5980761-740f-44fd-b228-c80f70c2c1f0")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8626fde0-4ab4-49c9-83fe-7bcbb0e45c57")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "201e6961-443f-414b-8f34-ce902a32f494")
		)
		(fp_line
			(start 6.46 6.41)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7f55b141-fe51-48ed-900b-f14ab1f254ce")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "55129be4-c0fe-4dfc-97b1-e97035a0554e")
		)
		(fp_line
			(start -1.1 -1.55)
			(end -1.1 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b97784db-bd4e-408d-b9bf-ee9f28886a66")
		)
		(fp_line
			(start -1.1 6.6)
			(end 8.7 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dd92823e-0b32-431b-a63b-50b5481ef4a0")
		)
		(fp_line
			(start 8.7 -1.55)
			(end -1.1 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2ddaede4-0752-4e3a-a115-8ead2acbdee9")
		)
		(fp_line
			(start 8.7 6.6)
			(end 8.7 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "df501597-a283-4fb3-a999-c45cac51fc24")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b59b9840-207b-471d-b642-240a032a6c2a")
		)
		(fp_line
			(start 0.635 6.35)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "09f25109-2ee8-4acf-a0a8-54bbfea6e37f")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f531cf63-3049-4e93-b687-dd6e15af114f")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "de8375e2-1f46-4a51-9e43-1e92e74a85b2")
		)
		(fp_line
			(start 6.985 6.35)
			(end 0.635 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a05bfddc-ae81-49c9-be10-719142f2893e")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.539999 180)
			(layer "F.Fab")
			(uuid "3364bfec-b816-4d7c-9cbb-f7d45a86448f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "Net-(R32-Pad1)")
			(pintype "passive")
			(uuid "ab149d56-a848-4045-9bd3-ab11f19f2d2c")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 144 "Net-(Q22-C)")
			(pintype "passive")
			(uuid "da98ecdc-94ce-47c2-8fff-adcf971ea33d")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "unconnected-(U12-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "a5b484b7-5976-42c5-a17b-bb9cd0672c74")
		)
		(pad "4" thru_hole oval
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 142 "Net-(Q21-G)")
			(pintype "passive")
			(uuid "5170ed62-a2d6-4abd-80ec-b9595c586355")
		)
		(pad "5" thru_hole oval
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "unconnected-(U12-NC-Pad5)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "a8158678-6340-4ef5-ae1f-b6fc1ee328dd")
		)
		(pad "6" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "Net-(R31-Pad1)")
			(pintype "passive")
			(uuid "5a0f9562-ab33-4bf2-8a4c-c0307fb46006")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-6_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "7e7eb2ad-d01c-487a-b57c-e73d47029860")
		(at 53.542855 135.08 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R48"
			(at 0 -1.82 180)
			(layer "F.SilkS")
			(uuid "ce21ff00-00b8-4ed8-9417-82388977baeb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at -3.64 0 180)
			(layer "F.Fab")
			(uuid "eec042a4-4204-4b32-91b3-c391b24c19f9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "144d14a1-271d-4d42-ac9c-97b37e69fc79")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "96e457f9-c13f-45a4-a284-2b136ec5a9f5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "9ffe190b-774a-4aaa-93a4-4c696b9fa71c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/4b0c0d83-8522-4ffe-8435-2c6bf5567543/ca31a324-056f-45d6-b948-82e97db62734")
		(sheetname "Triac Circuit15")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "20d6438e-3f03-4032-b454-c6fd028feb0f")
		)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2f5fce7c-333b-455f-a556-9864c16ee1c7")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f49073cb-5776-41d0-b97c-29fb541456ea")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "de8868e1-8f9f-4333-b98b-aacb7a59be35")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4aa01502-a87f-4de6-abc3-8a09d0f4c429")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1af20749-b6d6-4466-adc5-a072e877da5f")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dff99b7d-44b4-4c8b-a979-a916e87bc0d1")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f6dfbb3b-b43f-42d3-96ef-f25f5dec1e4e")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0c926f8b-4916-443b-b8d5-b5866414d198")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f2432da9-7fb9-4817-b2fc-dc1f41d2c4ed")
		)
		(fp_text user "${REFERENCE}"
			(at 3.04 0.01 180)
			(layer "F.Fab")
			(uuid "f133713c-73bd-4c6e-9876-adc9f926d7c4")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 158 "Net-(Q32-B)")
			(pintype "passive")
			(uuid "447b9602-1535-4e33-be0c-f61d248bb6ba")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 138 "/Triac Circuit15/Enable")
			(pintype "passive")
			(uuid "cf464e87-8b79-46de-8ca0-227206f63b62")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_QFP:LQFP-32_7x7mm_P0.8mm"
		(layer "F.Cu")
		(uuid "812f5f42-f9c5-4b41-9954-23499ec3c248")
		(at 62.4 156.625)
		(descr "LQFP, 32 Pin (https://www.nxp.com/docs/en/package-information/SOT358-1.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "LQFP QFP")
		(property "Reference" "U18"
			(at 0 -5.88 0)
			(layer "F.SilkS")
			(uuid "5ab0000d-ba88-4be2-873a-e84b05214d57")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "STM32G030K8Tx"
			(at 0 5.88 0)
			(layer "F.Fab")
			(uuid "3a3b39fc-403e-4695-b20e-94641a8cbb85")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1b18e8cc-98f4-4922-b3ed-ddfefc1de40d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stm32g030k8.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7f3bf87a-8de5-44e9-b3f6-fe9a2290723b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "STMicroelectronics Arm Cortex-M0+ MCU, 64KB flash, 8KB RAM, 64 MHz, 2.0-3.6V, 29 GPIO, LQFP32"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "560845af-fa9b-4da7-a5c5-eb324385702f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "LQFP*7x7mm*P0.8mm*")
		(path "/4d206a41-fa20-4a4d-9368-a273bc378e93")
		(sheetname "Główny")
		(sheetfile "16_ChannelPowerControlBoard.kicad_sch")
		(attr smd)
		(fp_line
			(start -3.61 -3.61)
			(end -3.61 -3.31)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c0bed968-c4c3-46eb-a90b-24d97280370f")
		)
		(fp_line
			(start -3.61 3.61)
			(end -3.61 3.31)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "023554fa-9959-4cb7-b211-5eedda859bef")
		)
		(fp_line
			(start -3.31 -3.61)
			(end -3.61 -3.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9a43631b-99d2-4cc3-8f2b-e4e5a4492e3a")
		)
		(fp_line
			(start -3.31 3.61)
			(end -3.61 3.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "69a57a36-41a6-4908-87f8-7bcf602b300c")
		)
		(fp_line
			(start 3.31 -3.61)
			(end 3.61 -3.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4a3f83db-9263-4b53-9633-aa31e7d9ebd7")
		)
		(fp_line
			(start 3.31 3.61)
			(end 3.61 3.61)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "57900f1b-c263-4c7e-a25b-9f826e0c460c")
		)
		(fp_line
			(start 3.61 -3.61)
			(end 3.61 -3.31)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1c27cdca-81e8-4299-ada7-b2c359cfc88d")
		)
		(fp_line
			(start 3.61 3.61)
			(end 3.61 3.31)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "598f12f7-8129-4509-9052-7eb232da891b")
		)
		(fp_poly
			(pts
				(xy -4.2125 -3.31) (xy -4.5525 -3.78) (xy -3.8725 -3.78) (xy -4.2125 -3.31)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "c6e97b32-0d9b-409f-8b59-82029f12139d")
		)
		(fp_line
			(start -5.18 -3.3)
			(end -5.18 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "afe1493d-abd5-444e-936c-da97ce66bd8c")
		)
		(fp_line
			(start -5.18 3.3)
			(end -5.18 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ce80c7ba-d065-4c65-993a-4901dee8454c")
		)
		(fp_line
			(start -3.75 -3.75)
			(end -3.75 -3.3)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c5e070e7-8467-415f-a4a6-114567814358")
		)
		(fp_line
			(start -3.75 -3.3)
			(end -5.18 -3.3)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "58afab41-82d4-44af-9f21-0b995aec6cef")
		)
		(fp_line
			(start -3.75 3.3)
			(end -5.18 3.3)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5336c0f3-44e4-4040-a725-64493f1a656d")
		)
		(fp_line
			(start -3.75 3.75)
			(end -3.75 3.3)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4482103a-cd38-4948-99f7-e23e0024a756")
		)
		(fp_line
			(start -3.3 -5.18)
			(end -3.3 -3.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4402776c-a7bf-4a88-8a2d-8728b62f5737")
		)
		(fp_line
			(start -3.3 -3.75)
			(end -3.75 -3.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bee61c2a-2156-45d5-976c-80e2fce161c3")
		)
		(fp_line
			(start -3.3 3.75)
			(end -3.75 3.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4984fef6-fdc6-46f7-a25e-7fe44a5f18e4")
		)
		(fp_line
			(start -3.3 5.18)
			(end -3.3 3.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5f2b10a2-302d-4f35-9471-be8eb405be50")
		)
		(fp_line
			(start 0 -5.18)
			(end -3.3 -5.18)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "855164bd-b2d2-453d-b493-cbbe28531030")
		)
		(fp_line
			(start 0 -5.18)
			(end 3.3 -5.18)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6e8520f6-fc32-4bf3-99cb-07c391abe460")
		)
		(fp_line
			(start 0 5.18)
			(end -3.3 5.18)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "70961f87-4e89-4439-b584-ed87dd6f0fff")
		)
		(fp_line
			(start 0 5.18)
			(end 3.3 5.18)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "af2f16f2-4981-4de7-a070-36c4eab7a25f")
		)
		(fp_line
			(start 3.3 -5.18)
			(end 3.3 -3.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f422d234-8917-4e63-b3f4-ba7edaf9f595")
		)
		(fp_line
			(start 3.3 -3.75)
			(end 3.75 -3.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a8336234-1dd9-4bda-91e5-f1535646acdd")
		)
		(fp_line
			(start 3.3 3.75)
			(end 3.75 3.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f17c3efe-bf35-42e9-95b7-00b72abb15c2")
		)
		(fp_line
			(start 3.3 5.18)
			(end 3.3 3.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "30e749f8-0eac-453e-ba20-770dcd2bd960")
		)
		(fp_line
			(start 3.75 -3.75)
			(end 3.75 -3.3)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3173aa08-4b1f-435b-97eb-63416390096e")
		)
		(fp_line
			(start 3.75 -3.3)
			(end 5.18 -3.3)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3cbfe8c9-7d24-4381-ae31-1f2d26ddfd25")
		)
		(fp_line
			(start 3.75 3.3)
			(end 5.18 3.3)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "001c3ac7-e231-4a7a-af96-93c89e6e9c77")
		)
		(fp_line
			(start 3.75 3.75)
			(end 3.75 3.3)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "832a81c8-5fc8-46b8-aa62-d35df8f48899")
		)
		(fp_line
			(start 5.18 -3.3)
			(end 5.18 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b3fe8833-4bc7-498e-bf7c-6d1713f40faa")
		)
		(fp_line
			(start 5.18 3.3)
			(end 5.18 0)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d43753c0-b440-4d85-92ac-75a67cfa3545")
		)
		(fp_line
			(start -3.5 -2.5)
			(end -2.5 -3.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d3e59227-5fcf-40ae-ba5d-8f7294494412")
		)
		(fp_line
			(start -3.5 3.5)
			(end -3.5 -2.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ad536d49-8327-4a0e-827e-cce2a3c5bdf4")
		)
		(fp_line
			(start -2.5 -3.5)
			(end 3.5 -3.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "560957f9-932f-4ba0-bef0-e6d02c25b9ce")
		)
		(fp_line
			(start 3.5 -3.5)
			(end 3.5 3.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c052e0b9-26fe-420b-9d65-c79a79867ff7")
		)
		(fp_line
			(start 3.5 3.5)
			(end -3.5 3.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7f458aa6-fe2a-4897-b645-c7947203ea23")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "fd76d354-f47b-4d01-94a2-d4aa824369ba")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -4.175 -2.8)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 192 "unconnected-(U18-PB9-Pad1)")
			(pinfunction "PB9")
			(pintype "bidirectional")
			(uuid "35355bda-761c-487d-bf90-386a33250eae")
		)
		(pad "2" smd roundrect
			(at -4.175 -2)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 201 "unconnected-(U18-PC14-Pad2)")
			(pinfunction "PC14")
			(pintype "bidirectional")
			(uuid "842acd26-6e51-42d6-81d5-19f2f1b1dd44")
		)
		(pad "3" smd roundrect
			(at -4.175 -1.2)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 211 "unconnected-(U18-PC15-Pad3)")
			(pinfunction "PC15")
			(pintype "bidirectional")
			(uuid "e17bb474-62ba-4264-ac2c-799b9e130afb")
		)
		(pad "4" smd roundrect
			(at -4.175 -0.4)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 167 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
			(uuid "a1be0d62-8edc-44bc-a542-77e6cf4a975c")
		)
		(pad "5" smd roundrect
			(at -4.175 0.4)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(uuid "84b98633-f998-431f-811c-658c7d8443e3")
		)
		(pad "6" smd roundrect
			(at -4.175 1.2)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 193 "NRST")
			(pinfunction "NRST")
			(pintype "input")
			(uuid "375c9b0e-2e50-460e-9e55-dff9679ea7db")
		)
		(pad "7" smd roundrect
			(at -4.175 2)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 207 "unconnected-(U18-PA0-Pad7)")
			(pinfunction "PA0")
			(pintype "bidirectional")
			(uuid "b3289f5d-d9ea-4718-a880-2b02db99a0e3")
		)
		(pad "8" smd roundrect
			(at -4.175 2.8)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 185 "unconnected-(U18-PA1-Pad8)")
			(pinfunction "PA1")
			(pintype "bidirectional")
			(uuid "0a484838-f78d-4912-b427-3dcf47aba803")
		)
		(pad "9" smd roundrect
			(at -2.8 4.175)
			(size 0.5 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 188 "unconnected-(U18-PA2-Pad9)")
			(pinfunction "PA2")
			(pintype "bidirectional")
			(uuid "1e2e1d73-9574-4633-9ad0-1689d3675d8a")
		)
		(pad "10" smd roundrect
			(at -2 4.175)
			(size 0.5 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 189 "unconnected-(U18-PA3-Pad10)")
			(pinfunction "PA3")
			(pintype "bidirectional")
			(uuid "20174d42-90d1-4bc6-953f-7658ae57e464")
		)
		(pad "11" smd roundrect
			(at -1.2 4.175)
			(size 0.5 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 198 "unconnected-(U18-PA4-Pad11)")
			(pinfunction "PA4")
			(pintype "bidirectional")
			(uuid "611066ed-0859-4537-a9b6-ca8ffee29f8f")
		)
		(pad "12" smd roundrect
			(at -0.4 4.175)
			(size 0.5 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 199 "SPI1_SCK")
			(pinfunction "PA5")
			(pintype "bidirectional")
			(uuid "73db8ea2-0181-4789-b2a6-760ed2c77022")
		)
		(pad "13" smd roundrect
			(at 0.4 4.175)
			(size 0.5 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 197 "SPI1_MISO")
			(pinfunction "PA6")
			(pintype "bidirectional")
			(uuid "533c4007-5f0e-496c-a46b-e090303338c6")
		)
		(pad "14" smd roundrect
			(at 1.2 4.175)
			(size 0.5 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 212 "SPI1_MOSI")
			(pinfunction "PA7")
			(pintype "bidirectional")
			(uuid "e614ebfe-7884-49f8-8175-3e5f839b3e16")
		)
		(pad "15" smd roundrect
			(at 2 4.175)
			(size 0.5 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 205 "unconnected-(U18-PB0-Pad15)")
			(pinfunction "PB0")
			(pintype "bidirectional")
			(uuid "a75c4a6a-2b0f-4658-ae1d-8d98a358f0bb")
		)
		(pad "16" smd roundrect
			(at 2.8 4.175)
			(size 0.5 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 214 "unconnected-(U18-PB1-Pad16)")
			(pinfunction "PB1")
			(pintype "bidirectional")
			(uuid "fe3f527d-7214-47de-abec-f36a086e8468")
		)
		(pad "17" smd roundrect
			(at 4.175 2.8)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 210 "unconnected-(U18-PB2-Pad17)")
			(pinfunction "PB2")
			(pintype "bidirectional")
			(uuid "d61e646e-a527-4b09-8d05-f6cf8037d4a1")
		)
		(pad "18" smd roundrect
			(at 4.175 2)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 208 "unconnected-(U18-PA8-Pad18)")
			(pinfunction "PA8")
			(pintype "bidirectional")
			(uuid "b63e2dcd-eb10-4247-8046-3acdb9c5a7b9")
		)
		(pad "19" smd roundrect
			(at 4.175 1.2)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 194 "unconnected-(U18-PA9{slash}NC-Pad19)")
			(pinfunction "PA9/NC")
			(pintype "bidirectional")
			(uuid "37f5506f-fd7c-4161-ab70-c08cb812f085")
		)
		(pad "20" smd roundrect
			(at 4.175 0.4)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 200 "unconnected-(U18-PC6-Pad20)")
			(pinfunction "PC6")
			(pintype "bidirectional")
			(uuid "7f7865b0-db69-4ab6-81c5-25705e79e80d")
		)
		(pad "21" smd roundrect
			(at 4.175 -0.4)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 206 "unconnected-(U18-PA10{slash}NC-Pad21)")
			(pinfunction "PA10/NC")
			(pintype "bidirectional")
			(uuid "adf15c51-ca81-4256-b989-cca3ee42b978")
		)
		(pad "22" smd roundrect
			(at 4.175 -1.2)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 209 "unconnected-(U18-PA11{slash}PA9-Pad22)")
			(pinfunction "PA11/PA9")
			(pintype "bidirectional")
			(uuid "b9694375-f5b4-4a2e-b911-5678690cb3a0")
		)
		(pad "23" smd roundrect
			(at 4.175 -2)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 204 "unconnected-(U18-PA12{slash}PA10-Pad23)")
			(pinfunction "PA12/PA10")
			(pintype "bidirectional")
			(uuid "9fff7776-ca53-4937-b879-57feae1d4ed3")
		)
		(pad "24" smd roundrect
			(at 4.175 -2.8)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 202 "SWDIO")
			(pinfunction "PA13")
			(pintype "bidirectional")
			(uuid "89cab371-3afc-4ba5-9ba8-8d55b2105ae5")
		)
		(pad "25" smd roundrect
			(at 2.8 -4.175)
			(size 0.5 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 213 "SWDCLK")
			(pinfunction "PA14")
			(pintype "bidirectional")
			(uuid "ed371387-925b-41dc-ab35-985c0e505ad4")
		)
		(pad "26" smd roundrect
			(at 2 -4.175)
			(size 0.5 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 195 "unconnected-(U18-PA15-Pad26)")
			(pinfunction "PA15")
			(pintype "bidirectional")
			(uuid "41ba29f7-0b97-4b1d-8301-1ea5804e3c7a")
		)
		(pad "27" smd roundrect
			(at 1.2 -4.175)
			(size 0.5 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 196 "unconnected-(U18-PB3-Pad27)")
			(pinfunction "PB3")
			(pintype "bidirectional")
			(uuid "4f317032-d866-4c51-ad5c-4aaef5c05e8f")
		)
		(pad "28" smd roundrect
			(at 0.4 -4.175)
			(size 0.5 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 203 "unconnected-(U18-PB4-Pad28)")
			(pinfunction "PB4")
			(pintype "bidirectional")
			(uuid "9bbeef53-2881-4a75-9a83-f90d286fea45")
		)
		(pad "29" smd roundrect
			(at -0.4 -4.175)
			(size 0.5 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 191 "unconnected-(U18-PB5-Pad29)")
			(pinfunction "PB5")
			(pintype "bidirectional")
			(uuid "3458e5a2-bf50-4cd9-be96-f78e99ffc0b1")
		)
		(pad "30" smd roundrect
			(at -1.2 -4.175)
			(size 0.5 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 190 "unconnected-(U18-PB6-Pad30)")
			(pinfunction "PB6")
			(pintype "bidirectional")
			(uuid "2b3ce015-88fd-425d-9b80-cbd25cdf0c6f")
		)
		(pad "31" smd roundrect
			(at -2 -4.175)
			(size 0.5 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 187 "unconnected-(U18-PB7-Pad31)")
			(pinfunction "PB7")
			(pintype "bidirectional")
			(uuid "1716df16-3a62-4ea4-b4a0-54ed7bbdae28")
		)
		(pad "32" smd roundrect
			(at -2.8 -4.175)
			(size 0.5 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 186 "unconnected-(U18-PB8-Pad32)")
			(pinfunction "PB8")
			(pintype "bidirectional")
			(uuid "0fe83b1b-2359-45e0-a174-c7b2485f336c")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_QFP.3dshapes/LQFP-32_7x7mm_P0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "82118478-c769-4e93-8016-54af5fe46508")
		(at 53.542855 89.36 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R39"
			(at 0 -1.82 180)
			(layer "F.SilkS")
			(uuid "c84755cb-4efd-4cd9-b4c9-cbf2e492cb5c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at -3.64 0 180)
			(layer "F.Fab")
			(uuid "41caf97f-c01d-49b8-8225-611c11850817")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "dd7a1265-173c-4be6-963a-9531827ae42e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "bf1e196e-bcfa-41d2-bdf4-3e378c2991c4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "63cbc647-ca89-4814-86f2-eab017cde81a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/fb144577-8e6f-488b-ba1b-870763a27401/ca31a324-056f-45d6-b948-82e97db62734")
		(sheetname "Triac Circuit12")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5ac09499-36ac-4382-80a3-f9a46e2e4e9b")
		)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b34bc460-130b-4399-8a99-8d9dac72e927")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c956e012-de03-415a-8747-9335ef9cf41b")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0c62fc33-3086-4f58-b488-8c41b975b0ac")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3938f0d4-62be-4378-94bd-e070f126a8bf")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c63e1f50-3466-402f-b4f3-04e169a49b85")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "12811468-7564-4eed-b30b-e4f461b1b115")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "24047b8b-8504-4ce6-ad2b-e7ab81ef34ef")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "771e03f3-9f97-442a-a238-18973b234c1f")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a5820357-aefc-4e54-afc1-d7fbdb61094c")
		)
		(fp_text user "${REFERENCE}"
			(at 3.04 0.01 180)
			(layer "F.Fab")
			(uuid "ca2fd8b7-e4d3-419a-a0cc-a8b1f32d3e05")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 149 "Net-(Q26-B)")
			(pintype "passive")
			(uuid "cfc07e4b-d234-462e-9250-a9a7d9d4386b")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 135 "/Triac Circuit12/Enable")
			(pintype "passive")
			(uuid "ce7709e8-9d69-44d9-bda8-89cdcce30ae9")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(uuid "84400124-a364-49d2-87b8-d48509f0693e")
		(at 69.287855 121.78 90)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "Q29"
			(at 6.04 -2.444999 -90)
			(layer "F.SilkS")
			(uuid "6f8e71a4-2176-493e-9c32-76ce5e0edeb2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BTA16-600B"
			(at 2.539999 2.5 -90)
			(layer "F.Fab")
			(uuid "af5fe6df-1e72-4395-bcff-ba4b0c50fb54")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "7af0ecba-b434-4dfb-ab2e-1147a7fdf8e3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "523fe130-b476-4ba6-8035-6714361d6549")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "f0ed2535-a7b4-4be1-af5c-b48ef59d11a9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO?220*")
		(path "/683a6cfc-1cb6-4c63-ae1f-c9d1fdc220d0/d1257be0-2394-4f08-8984-f580162b15f9")
		(sheetname "Triac Circuit14")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 7.66 -3.27)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6fe7ffa9-3f8d-40bf-b12f-67142876c067")
		)
		(fp_line
			(start 4.391 -3.27)
			(end 4.391 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7d620f6d-8e9a-43f0-b370-c2826bc923bf")
		)
		(fp_line
			(start 0.69 -3.27)
			(end 0.69 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fd1eb576-162e-4f09-af98-466179ed4fb0")
		)
		(fp_line
			(start -2.58 -3.27)
			(end 7.66 -3.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "916c72fd-c081-4995-be8d-82fe62f17cbf")
		)
		(fp_line
			(start -2.58 -3.27)
			(end -2.58 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "debbff3d-5e9f-4cb6-89be-3e8c15a2e53b")
		)
		(fp_line
			(start -2.58 -1.76)
			(end 7.66 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6d7e88b6-bfec-422a-b9d2-f0bc1508a472")
		)
		(fp_line
			(start -2.58 1.371)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f960d475-c3a2-4027-85b1-062557d005e3")
		)
		(fp_line
			(start 7.79 -3.4)
			(end -2.71 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0270e0a6-b021-478f-a11f-54153e9b7570")
		)
		(fp_line
			(start -2.71 -3.4)
			(end -2.71 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9ca2944a-5f87-43d0-91ac-8386634e9ff2")
		)
		(fp_line
			(start 7.79 1.51)
			(end 7.79 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "531040cd-be1e-492e-a9d0-7b0f868e7e0b")
		)
		(fp_line
			(start -2.71 1.51)
			(end 7.79 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "534740e4-600b-47f1-9c1b-3571a54e5e98")
		)
		(fp_line
			(start 7.54 -3.15)
			(end -2.46 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "771c997b-3ad9-4882-81e7-8d23f831f651")
		)
		(fp_line
			(start 4.39 -3.15)
			(end 4.39 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c4500a6e-6e4b-473d-b44a-6ad726578932")
		)
		(fp_line
			(start 0.69 -3.15)
			(end 0.69 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ba6d248c-4564-4021-a1ad-ee85ec76db90")
		)
		(fp_line
			(start -2.46 -3.15)
			(end -2.46 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "725027ad-93ed-43b5-ab2d-53c8b3f33cdd")
		)
		(fp_line
			(start -2.46 -1.88)
			(end 7.54 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9771e3ae-d303-41bf-9211-321360f23936")
		)
		(fp_line
			(start 7.54 1.25)
			(end 7.54 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3e3f3b50-6261-4e7e-95ed-d288ce2b8f1c")
		)
		(fp_line
			(start -2.46 1.25)
			(end 7.54 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e2643019-b054-4b47-933c-fabb4d6e1fa1")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 -4.27 -90)
			(layer "F.Fab")
			(uuid "1a67831c-e2f8-4cd5-bad3-baf583871ce9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 86 "/Triac Circuit14/High_Voltage_L")
			(pinfunction "A1")
			(pintype "passive")
			(uuid "0f3d4c10-a867-4c0d-bc32-e0f13ab32651")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/Triac Circuit14/High_Voltage_Out")
			(pinfunction "A2")
			(pintype "passive")
			(uuid "1133729e-c697-45f4-8fef-ea32f92d350c")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 154 "Net-(Q29-G)")
			(pinfunction "G")
			(pintype "input")
			(uuid "a2c39a4d-83dc-4081-a254-ffbfda5b4d5e")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "86227af7-458e-451e-8459-7cbcb1dae1fa")
		(at 54.005355 92.159999)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q26"
			(at 0 -2.4 180)
			(layer "F.SilkS")
			(uuid "55240a0e-a6ea-4ab9-90fe-5be2444a69f6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BC818"
			(at 0 2.4 180)
			(layer "F.Fab")
			(uuid "6c237c4b-7656-4be2-82c7-beada31dcc91")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "1aadf057-89e6-43f9-9054-ffdd96c441da")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC818-D.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "bea37142-d18c-42bd-a66c-dbeaa600b15c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "cbd95576-f9be-4dd0-b0e4-d5736d1e2dfa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/fb144577-8e6f-488b-ba1b-870763a27401/00e550ea-8431-483d-ac3c-b4a719825546")
		(sheetname "Triac Circuit12")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -1.56)
			(end -1.675 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b483386b-c072-4ddc-bf71-e73e56ced5d1")
		)
		(fp_line
			(start 0 -1.56)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3cad4741-6eb1-452a-8624-8c80aa81ba42")
		)
		(fp_line
			(start 0 1.56)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1f60e0ee-75e0-4bf2-b01e-7a393c98bdc3")
		)
		(fp_line
			(start 0 1.56)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "37caaf6e-c6fa-4ae5-9509-d27277c4430d")
		)
		(fp_line
			(start -1.92 -1.7)
			(end -1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7a9db63c-7a70-44f6-94dd-c3e17e2c63b7")
		)
		(fp_line
			(start -1.92 1.7)
			(end 1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3e9f5ef2-c927-48ef-a592-b7d811ba5dae")
		)
		(fp_line
			(start 1.92 -1.7)
			(end -1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "50acf9c0-aae4-48b2-adb4-22d41a64c401")
		)
		(fp_line
			(start 1.92 1.7)
			(end 1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "663e7561-9c2d-41ab-82f5-6dca68d33420")
		)
		(fp_line
			(start -0.65 -1.125)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "376cc8a6-e7f7-462c-9735-d8216893388b")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "36d79264-249a-4d3b-8c7b-372473cdc826")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1450cdbe-1fe8-4da3-a945-ff8bbb2abade")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cbd8d600-bd09-4beb-bfa9-cbda1969520e")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "958608e9-53d6-4975-9cb7-4feb32db5479")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
			(uuid "a991d959-6333-446f-885e-5633986cf66a")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 149 "Net-(Q26-B)")
			(pinfunction "B")
			(pintype "input")
			(uuid "7c3cf0b0-7bbc-4c06-87aa-5cb7d64c9312")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "GND")
			(pinfunction "E")
			(pintype "passive")
			(uuid "38fd3a3b-6f6f-4b25-a539-ffb43bbdd116")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 150 "Net-(Q26-C)")
			(pinfunction "C")
			(pintype "passive")
			(uuid "0a8d6ff9-3234-4b0a-b083-25af9a7f130c")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-6_W7.62mm"
		(layer "F.Cu")
		(uuid "87075827-2a63-4793-a53a-b052d667272f")
		(at 57.142855 26.475)
		(descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U10"
			(at 3.599999 -2.33 180)
			(layer "F.SilkS")
			(uuid "a6185b8c-b6cf-4619-9992-935189b69d53")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MOC3021M"
			(at 3.81 7.409999 180)
			(layer "F.Fab")
			(uuid "abdf41c8-82a7-4afe-b8c3-585ab26b530a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7482999f-c96a-4085-b7b5-828fa1fa7dee")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3023M-D.PDF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b52f9f80-796e-4d3a-bf6b-0c9a6246186c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e72a72f5-66c2-42d7-9126-de31a852db2a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*")
		(path "/a837c47c-5707-46fe-8eca-0b07e116b13e/0262e914-5435-478f-be04-ece49b8102cf")
		(sheetname "Triac Circuit8")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0c1c4130-b0f1-4c39-99fc-50e1671b76ee")
		)
		(fp_line
			(start 1.16 6.41)
			(end 6.46 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "86e15f0b-2209-4c60-889f-4e8897f46b98")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "82d224e4-e5ff-4fb4-a360-431218977fce")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1fd2320b-9703-4725-b3db-2f877cbfb008")
		)
		(fp_line
			(start 6.46 6.41)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7f3450bf-ea7b-4401-9d06-4d6e319d1edc")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "83ce90fc-981e-4781-ad75-35bdbffef571")
		)
		(fp_line
			(start -1.1 -1.55)
			(end -1.1 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "27f88e6c-f5c2-4312-a307-aa919cf7aae2")
		)
		(fp_line
			(start -1.1 6.6)
			(end 8.7 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b2d22856-b361-46a0-b4b5-24f80e2f148b")
		)
		(fp_line
			(start 8.7 -1.55)
			(end -1.1 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7146a149-22ba-44be-aa0e-03dc127a95f0")
		)
		(fp_line
			(start 8.7 6.6)
			(end 8.7 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e5acf7b3-6e0c-4813-8779-e4304a70e021")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4503476c-7777-4ac3-83f1-5d39e3357fe6")
		)
		(fp_line
			(start 0.635 6.35)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ce368fe0-cebd-4ac6-b8b1-64f983848e06")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d25e0a37-47de-44ac-82e2-524abcc976ee")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c8fcc847-e81a-441b-b334-9d1280ddd59a")
		)
		(fp_line
			(start 6.985 6.35)
			(end 0.635 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2941f621-50d5-4f40-a32e-e5fbf02ed3b2")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.539999 180)
			(layer "F.Fab")
			(uuid "75508209-134a-4414-b6cc-214980165cfa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 117 "Net-(R26-Pad1)")
			(pintype "passive")
			(uuid "acd19519-e243-4544-85ac-4909bda5cb8d")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 130 "Net-(Q18-C)")
			(pintype "passive")
			(uuid "fec4ccb1-4ef5-4803-801b-757c7260314a")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "unconnected-(U10-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "c4a9e0b6-afe2-446d-933e-446da272e9e3")
		)
		(pad "4" thru_hole oval
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "Net-(Q17-G)")
			(pintype "passive")
			(uuid "35c6ffdd-4b71-48c7-a741-411216e83c31")
		)
		(pad "5" thru_hole oval
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 98 "unconnected-(U10-NC-Pad5)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "a375fc57-3892-453f-9243-fc8ad09ca32b")
		)
		(pad "6" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "Net-(R25-Pad1)")
			(pintype "passive")
			(uuid "a4238159-9024-4582-ab0b-a91ed344518e")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-6_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "886be42c-fd14-4941-81d0-913a6e9a1445")
		(at 53.605355 41.44 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R29"
			(at 0 -1.82 180)
			(layer "F.SilkS")
			(uuid "e4eb3b17-67ec-483c-b364-2c2e868deb31")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at 0 1.82 180)
			(layer "F.Fab")
			(uuid "81690ddc-52da-4e57-9697-121195e080f7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "0c34eaf3-2e25-4968-aaf5-7f2930eba125")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "b24e0c00-48ba-4e76-997b-993c2ba4447e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "3930b019-1c00-4d23-bd7b-d87d6abb377b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/f251f0b5-0f8b-4418-bbfe-69d55a4bdeb8/de24ad75-a874-4d54-a682-b1d6f2079d30")
		(sheetname "Triac Circuit9")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e3eaf111-bc41-455a-bb2a-5ab9c26e4476")
		)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b1fd19e9-b123-4f64-8826-a87022032eaa")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f9c00ace-0a01-444d-83ad-4825322a8a75")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1584a71f-4f16-40a9-894f-d8cda010c590")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2a89d50b-da68-4826-badb-bee7affe32bb")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "71a7b73c-d036-4734-a9f6-9b058aab384c")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e3b0fb3f-e742-4ccf-9e31-113b4000cd56")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "698f78c6-f7be-4144-a62d-c84e19b2b37a")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f897bf4d-e523-4f39-88e4-37e1f1020fc2")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "924bacd1-3111-48bd-9f99-1c91e7df7ffc")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
			(uuid "274bc00a-30d9-43c3-bf81-6c26b9d5a47f")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 118 "Net-(R29-Pad1)")
			(pintype "passive")
			(uuid "420f84c0-53f1-4159-9a4c-ecc4f896b154")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 37 "+3V3")
			(pintype "passive")
			(uuid "06df1408-1036-4b2b-921e-9e2b6a56c407")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "893457fa-9ce1-44a2-92ee-274c62ff4408")
		(at 53.605355 26.2 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R26"
			(at 0 -1.82 180)
			(layer "F.SilkS")
			(uuid "cc57d5ec-8f9b-4f01-be86-4533ad2e465b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at 0 1.82 180)
			(layer "F.Fab")
			(uuid "2b47d334-06cf-4371-bb32-aca87e8ffed9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "6dee6682-04e7-421b-94a9-419f11d9d358")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "7f1782d9-f033-4bca-bdce-bd6a4b49e6f2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "9d3dd106-6339-4433-be2c-8b896a13e5ea")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/a837c47c-5707-46fe-8eca-0b07e116b13e/de24ad75-a874-4d54-a682-b1d6f2079d30")
		(sheetname "Triac Circuit8")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b02256e3-974c-4d07-aecd-e34fa4ab64b5")
		)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bd96d904-856f-4249-9472-e137e4562252")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e7ebd2f8-f531-4976-8fc5-b8e56cc83b5a")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8357cf99-3bc0-4750-943a-2115e97e1929")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "180e8e83-9a41-497a-9edf-8a8e5b946fa9")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "50375a2f-40be-46e6-a0dc-65b6fb20390e")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cdc05588-e21b-4cff-91a1-080c7973a969")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7a0040f4-86f5-47f7-9781-f7fb2554c7ea")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "02aeccf9-438f-4467-bea1-f2936a33789c")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f8c29f85-a1cf-4f1c-8d4b-68e7f1bc0667")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
			(uuid "bf14cce3-0749-4930-9a17-3bd0515e0e86")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 117 "Net-(R26-Pad1)")
			(pintype "passive")
			(uuid "4001a1f9-2103-4bbf-9b3e-d0245c6c795b")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 37 "+3V3")
			(pintype "passive")
			(uuid "5bfda7f6-ef24-4596-bf0c-f197def9dbdd")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "8ed014b1-6814-4d3f-8163-d41ad6c671d2")
		(at 48.423216 70.32)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "42fb9d62-bf6a-406d-88d7-81fa3b4958a6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "58e8ae14-dd23-4ec7-bb0d-d7a8f98a5e90")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "399c30bb-c120-4294-8b7c-f7c36c0ebfe9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b14d8f91-7e7b-4556-9ad7-60e068d8c400")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "aba39115-b8aa-4448-bf91-f4e5c749681f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1abc9394-30bb-4ef5-a1be-aa230dbd1566/de24ad75-a874-4d54-a682-b1d6f2079d30")
		(sheetname "Triac Circuit3")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "29257146-c6e2-421d-bc12-02033899e02c")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "db287ee9-6156-470b-9cad-8e9af55c7d41")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4f5312d4-2e42-4701-b3cc-05b0ab2b36fd")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "acfd09ad-c415-4331-920a-194eb9019599")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9f969b5c-318b-4b47-a099-2cb5ec0438ed")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9578c90e-cc61-46b5-baff-f63f9e15d61b")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "df28666f-d294-4ff3-b1d1-d3bb924a5ccd")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b00f2302-205a-43be-8dc4-37e92633690d")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d46ce96e-f5e5-4e3f-bc76-f3e80a6c5499")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0b1dc74d-9936-47fe-ab80-b5683ad08ad8")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d1d6bd6c-7b5e-4592-893b-91e4e6788f76")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 112 "Net-(R11-Pad1)")
			(pintype "passive")
			(uuid "7ef2a9b0-a98e-4862-b734-e1989d9344df")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 37 "+3V3")
			(pintype "passive")
			(uuid "f75edaa6-9f81-47de-87eb-d5c87900865b")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(uuid "9144490d-f81b-4d9d-b0a2-7d79581dae9c")
		(at 61.8 171.4)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(uuid "a624e18e-20e8-4106-bbe8-570382adf711")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100n"
			(at 0 1.85 0)
			(layer "F.Fab")
			(uuid "9eb54568-7e66-4961-9adf-df1be12913e6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0f026e34-19ce-46ae-b899-c3bbe740b03a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c2feb4f2-959f-4f3b-8b2d-0ef1e531f5e2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9663a07d-076a-4108-9bde-b3d5a451acbf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/a614d879-0000-4b79-8a3e-164a44d89b2d")
		(sheetname "Główny")
		(sheetfile "16_ChannelPowerControlBoard.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.711252 -0.91)
			(end 0.711252 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cc991cc4-3c1d-4ce5-92b2-5611232c1636")
		)
		(fp_line
			(start -0.711252 0.91)
			(end 0.711252 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c6d8e276-5f0a-4e39-af1e-c93b220f1cbb")
		)
		(fp_line
			(start -2.3 -1.15)
			(end 2.3 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "78e25717-4d7b-4a61-8323-753f0ff122e7")
		)
		(fp_line
			(start -2.3 1.15)
			(end -2.3 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f7f37919-d4f0-4e24-b54b-a1c7aff2dc07")
		)
		(fp_line
			(start 2.3 -1.15)
			(end 2.3 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a8ab4718-7373-47c8-afd7-41de02cba0dc")
		)
		(fp_line
			(start 2.3 1.15)
			(end -2.3 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c01de928-9fc5-4ecf-a67b-f98db8c497ec")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8f130d95-9f6a-411e-9121-a0ec30c78da6")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fd4f7390-cf58-4ddd-9553-84c6b6d951b4")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ce896281-02d4-4508-b151-3fb3b2315655")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7528cc64-01f4-4ccb-81c0-36c970253f5d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "4cccb301-6656-4611-a0fb-77564b60eb55")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 167 "+3.3V")
			(pintype "passive")
			(uuid "b1635c5e-b69f-481c-8d1d-246e9c7626fc")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 41 "GND")
			(pintype "passive")
			(uuid "7d56aba1-810d-4230-9f26-0757b64924fb")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
		(layer "F.Cu")
		(uuid "9262c7d3-8469-461f-b560-6292a46b6254")
		(at 77 76.12 90)
		(descr "Terminal Block Phoenix MKDS-3-2-5.08, 2 pins, pitch 5.08mm, size 10.2x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-3-2-5.08 pitch 5.08mm size 10.2x11.2mm^2 drill 1.3mm pad 2.6mm")
		(property "Reference" "J12"
			(at 3.1 -2.999999 -90)
			(layer "F.SilkS")
			(uuid "38b995ac-8310-4e92-a94a-ec30869824a0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 2.539999 6.36 90)
			(layer "F.Fab")
			(uuid "10ccc71f-f1fc-494e-b784-a874c336030e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "4e46f480-353c-4bec-b59d-54e8eef456e2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "b35a32de-39d5-4eaa-bd01-9ce501398e9f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "64588fce-6f67-4e23-b690-0736b403a786")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/15d8fe7c-2a9b-438f-a777-3e4687188af1/60e4d8a3-c16e-48cd-a1fd-61f2968ecc7b")
		(sheetname "Triac Circuit11")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 7.68 -5.96)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e60161be-1adf-409f-a472-1c3d595a7354")
		)
		(fp_line
			(start -2.6 -5.96)
			(end 7.68 -5.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "98a71573-7212-4afb-8e5c-1b3b24009e7c")
		)
		(fp_line
			(start -2.6 -5.96)
			(end -2.6 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4e96162a-5de2-4923-96f8-7b97cc9dad72")
		)
		(fp_line
			(start -2.6 -3.9)
			(end 7.68 -3.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a6fc9a45-2166-4e6e-ad34-1ef98dbd7716")
		)
		(fp_line
			(start 6.468 -1.654)
			(end 6.088 -1.274)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "79b96319-85b3-45a7-aeb3-6a4ab2740d91")
		)
		(fp_line
			(start 1.388 -1.654)
			(end 1.281 -1.547)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0d36eb42-32cb-44b9-9aa0-578183671f41")
		)
		(fp_line
			(start 6.734 -1.388)
			(end 6.339 -0.992)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5d56988e-e5cb-4b84-9028-4275b1d04868")
		)
		(fp_line
			(start 1.654 -1.388)
			(end 1.547 -1.281)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5006dc39-2741-438f-8652-1b9aa4319511")
		)
		(fp_line
			(start 3.822 0.992)
			(end 3.427 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fcffa06a-40b7-4a79-945e-341511b10932")
		)
		(fp_line
			(start 4.073 1.274)
			(end 3.693 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "59163c3b-63f0-4a76-b54f-1839ed1edbe7")
		)
		(fp_line
			(start -1.548 1.281)
			(end -1.654 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c30f1a51-17ae-412c-974e-4dd97eb5fb18")
		)
		(fp_line
			(start -1.282 1.547)
			(end -1.388 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9e84735d-0d5b-4746-b424-9e7a5260ed6f")
		)
		(fp_line
			(start -2.6 2.3)
			(end 7.68 2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "90402ec7-76c3-4c7b-81d8-983eaa1321d1")
		)
		(fp_line
			(start -2.6 4.8)
			(end 7.68 4.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d420a6c4-d026-4205-98ee-76ae8fa5d549")
		)
		(fp_line
			(start -2.84 4.86)
			(end -2.84 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a647275b-b5af-4909-aa05-16e63de8c665")
		)
		(fp_line
			(start -2.6 5.36)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6cb1c237-c53f-45f3-93ac-9e88d95efc65")
		)
		(fp_line
			(start -2.84 5.6)
			(end -2.34 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3bcb5a29-5f09-4d94-9799-5a7f54d5f71e")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.26 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "9a3c204c-c71f-4a7a-bbfa-d14dd7391652")
		)
		(fp_circle
			(center 0 0)
			(end 2.18 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "78847686-6e89-4011-9e64-500c593add76")
		)
		(fp_line
			(start 8.13 -6.4)
			(end -3.04 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f906dc84-a073-4ec3-9540-a2d8ad25812f")
		)
		(fp_line
			(start -3.04 -6.4)
			(end -3.04 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7e23f358-3d3c-47bf-80b1-861b8b6e7af5")
		)
		(fp_line
			(start 8.13 5.8)
			(end 8.13 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4048e3a5-e294-4db7-b926-9dae56ac7602")
		)
		(fp_line
			(start -3.04 5.8)
			(end 8.13 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a0c9c4a9-5d4a-44e0-8940-a05531d6688e")
		)
		(fp_line
			(start 7.62 -5.9)
			(end 7.62 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "57d65c61-f16c-42aa-b17f-0d565ed4473b")
		)
		(fp_line
			(start -2.54 -5.9)
			(end 7.62 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "517e1904-e54f-47d3-bcb8-d2ae0f2f9360")
		)
		(fp_line
			(start -2.54 -3.9)
			(end 7.62 -3.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "879d676a-027e-4f33-ae0d-0d7054e37d38")
		)
		(fp_line
			(start 6.353 -1.517)
			(end 3.564 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7e0e0247-8248-4c36-81d8-0756d233074d")
		)
		(fp_line
			(start 1.273 -1.517)
			(end -1.517 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "de3c4d96-f468-4293-8ba2-8a3a4b805486")
		)
		(fp_line
			(start 6.597 -1.273)
			(end 3.808 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "39f767d1-1c08-4046-bfe3-8e6a68fe3784")
		)
		(fp_line
			(start 1.517 -1.273)
			(end -1.273 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "69222cb4-6fba-4b74-a317-39d2bce722d2")
		)
		(fp_line
			(start -2.54 2.3)
			(end 7.62 2.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b756ffa8-6406-4bdf-8b0d-99613c890965")
		)
		(fp_line
			(start -2.54 4.8)
			(end -2.54 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "46012864-c5e1-445c-ac57-189e31d535ef")
		)
		(fp_line
			(start -2.54 4.8)
			(end 7.62 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f60ee0ae-191f-490a-9dd5-f3394f819457")
		)
		(fp_line
			(start 7.62 5.3)
			(end -2.04 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6a368ce9-914e-4a84-aa38-2ea439fd8adc")
		)
		(fp_line
			(start -2.04 5.3)
			(end -2.54 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fc494129-1d3f-4752-92fd-4f61e658356b")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.08 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "d6364173-10c9-49ae-b776-99a38dd447ff")
		)
		(fp_circle
			(center 0 0)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "75b2616a-3e18-4c3e-8176-1fc94aff2304")
		)
		(fp_text user "${REFERENCE}"
			(at 2.539999 3.1 90)
			(layer "F.Fab")
			(uuid "43e12912-a769-43a3-8789-0167502f051f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "/Triac Circuit11/High_Voltage_L")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "8641ae86-ef62-4152-b8c0-412a7020f617")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/Triac Circuit11/High_Voltage_Out")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "576ae2d2-537b-4443-9002-c47766762658")
		)
		(model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "957e9a31-fe72-479d-b7f2-df9cf6c008d9")
		(at 48.5375 24.6)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "3c631775-11b2-4b15-be0a-4b7b5cf7f52c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "2cbc1cfc-b41e-4aa6-bf2e-16f7894b9ced")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9fbc5fa4-5494-4504-b5b8-d0518e8a81fc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e417fb31-c649-4ebb-a5e6-b842c7d946c6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a8a75f39-2fda-4915-b1fa-acb78ff8e1bf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/84e52baa-d126-4c4f-b1c5-63bb27b07c2b/de24ad75-a874-4d54-a682-b1d6f2079d30")
		(sheetname "Triac Circuit")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eb99dc54-c4d5-4298-9fa5-024926db07e0")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8b67475b-2dfe-4c7a-9f99-f6a5cacd99a3")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ceeb0327-4cc2-46d0-a4af-992e3118c62b")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "71fcf42b-cb1c-4471-ac52-a706e00d433a")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "55e99d50-ea3f-4a5c-bb2d-0fd3481a65bf")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "829e259f-de2c-484c-b57e-0a456e927642")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "32a4a78f-ffe4-417c-9edb-125c14548da1")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6eda8dfc-f393-465e-a3fa-34099e7a7f4b")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a9d624df-8c46-475e-8426-7c6c1821151c")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a999fd5c-aa07-4f5f-93ea-89c3da83d0da")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "34e75712-68c6-42e3-a967-fadf955c5d9a")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 109 "Net-(R2-Pad1)")
			(pintype "passive")
			(uuid "2d4a5bfd-ff6f-44c8-9ee2-ad15f0db0cbd")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 37 "+3V3")
			(pintype "passive")
			(uuid "f2e0c42a-9c8b-42a0-851a-6026d45c1ff3")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(uuid "95e02dbe-c49e-4798-aa7f-6a25f9baf92f")
		(at 66.942855 132.14 -90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R46"
			(at 3.809999 -1.92 -90)
			(layer "F.SilkS")
			(uuid "1676e5e0-d334-4d69-b2a7-c269f26a10f0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "180"
			(at 3.81 1.919999 -90)
			(layer "F.Fab")
			(uuid "e68d8fae-ec8d-461a-8366-acefa8255f2e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "172356fb-945c-41df-8843-fe9f0b84d736")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b883a3f8-72e3-4594-be6b-29aabd15edac")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3909bb15-b076-470c-b49a-2a1e7f88c7d5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/4b0c0d83-8522-4ffe-8435-2c6bf5567543/4ab64e29-964f-40b2-bf58-c546b31cd3eb")
		(sheetname "Triac Circuit15")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.89 0.92)
			(end 5.73 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6a6d6476-b06a-4e6b-91ca-d726f082d3ee")
		)
		(fp_line
			(start 5.73 0.92)
			(end 5.73 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7c8ce594-14f9-4032-a46a-21b90d6a75f7")
		)
		(fp_line
			(start 0.94 0)
			(end 1.89 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "db7203d0-55ef-4351-849f-7d82f403e902")
		)
		(fp_line
			(start 6.68 0)
			(end 5.73 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5a8a0da2-dd84-46b9-a884-65b3936e3049")
		)
		(fp_line
			(start 1.89 -0.92)
			(end 1.89 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "af318606-ccb0-49e2-9b6c-b163aadae591")
		)
		(fp_line
			(start 5.73 -0.92)
			(end 1.89 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e2ba173a-a392-4dc7-90a6-10c290426c84")
		)
		(fp_line
			(start -0.95 1.05)
			(end 8.57 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3fbe0165-be52-445d-a48d-b19af38d4f2a")
		)
		(fp_line
			(start 8.57 1.05)
			(end 8.57 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e1b7664e-720d-420a-8441-bc8f43c45fbd")
		)
		(fp_line
			(start -0.95 -1.05)
			(end -0.95 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d38db0bd-d2d1-4af4-a143-259c8fb94da7")
		)
		(fp_line
			(start 8.57 -1.05)
			(end -0.95 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d9fd282b-40b1-4d11-bc0a-4eddb365bfa5")
		)
		(fp_line
			(start 2.01 0.8)
			(end 5.61 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "954068f6-1930-40a2-9063-7a70f23126ef")
		)
		(fp_line
			(start 5.61 0.8)
			(end 5.61 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6053fd97-095a-4b19-b371-52be39d28e32")
		)
		(fp_line
			(start 0 0)
			(end 2.01 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "80875d35-66f7-458b-800a-5ab7756c9a0d")
		)
		(fp_line
			(start 7.62 0)
			(end 5.61 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "86201414-1462-43c4-a180-04c8ce7b30f6")
		)
		(fp_line
			(start 2.01 -0.8)
			(end 2.01 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ec95470c-1d46-4a54-84ad-d6f3487103e4")
		)
		(fp_line
			(start 5.61 -0.8)
			(end 2.01 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "753fcf59-b76f-45bf-a1b2-35a6930671d9")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 -90)
			(layer "F.Fab")
			(uuid "dd4c833a-4eef-4d65-8803-1a6cd5a7f39d")
			(effects
				(font
					(size 0.72 0.72)
					(thickness 0.108)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 88 "Net-(R46-Pad1)")
			(pintype "passive")
			(uuid "6729d324-becd-4ed5-83fc-9c35aa3bfac6")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 87 "/Triac Circuit15/High_Voltage_L")
			(pintype "passive")
			(uuid "6444f158-8477-44bc-a6c6-16705054fdde")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(uuid "96246be5-951f-4e93-be8b-e193a76283a7")
		(at 75.2 166.4)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U1"
			(at 0 -3.4 0)
			(layer "F.SilkS")
			(uuid "bb361cca-9498-4e3b-9784-6e175a433d0c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MCP2562-E-SN"
			(at 0 3.4 0)
			(layer "F.Fab")
			(uuid "e2832c66-cd31-4294-80b1-f09651576a1a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "36a00c7f-8c5c-47c3-8d71-e6eaea5fd5f6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/25167A.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "02115636-449e-40ad-8968-db6988d2e083")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "High-Speed CAN Transceiver, 1Mbps, 5V supply, Vio pin, -40C to +125C, SOIC-8"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "68e36519-06b4-48c2-b34f-ad4afad3f3ee")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm*")
		(path "/69cbc739-ee51-49ef-b6c8-ef6b58c80989")
		(sheetname "Główny")
		(sheetfile "16_ChannelPowerControlBoard.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -2.56)
			(end -1.95 -2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7046a32c-44da-4b41-925b-9d3145bf13f9")
		)
		(fp_line
			(start 0 -2.56)
			(end 1.95 -2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "55f0fd58-8e8d-456c-85e1-0f8bc2045ea2")
		)
		(fp_line
			(start 0 2.56)
			(end -1.95 2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bafab68d-aba7-42f9-975d-d36364e91fd7")
		)
		(fp_line
			(start 0 2.56)
			(end 1.95 2.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8f392eb6-eff8-4961-ab76-8876ab280c4b")
		)
		(fp_poly
			(pts
				(xy -2.7 -2.465) (xy -2.94 -2.795) (xy -2.46 -2.795) (xy -2.7 -2.465)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "2c153ad8-fdfa-46ef-a120-7f46157261cb")
		)
		(fp_line
			(start -3.7 -2.7)
			(end -3.7 2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0732615c-793e-4cdd-a4fc-e9bc502207a3")
		)
		(fp_line
			(start -3.7 2.7)
			(end 3.7 2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "87955090-f10b-4901-acea-048a431772ec")
		)
		(fp_line
			(start 3.7 -2.7)
			(end -3.7 -2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8222f2fa-17ed-4ca2-888e-055a4c92551d")
		)
		(fp_line
			(start 3.7 2.7)
			(end 3.7 -2.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "14dc3aa3-e6f3-40b6-87df-dd9008f2ec6b")
		)
		(fp_line
			(start -1.95 -1.475)
			(end -0.975 -2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bf073c7c-a47d-4c1c-85d4-67f1fa1d5973")
		)
		(fp_line
			(start -1.95 2.45)
			(end -1.95 -1.475)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cb4f5992-0765-418d-9043-01b2e211e9ea")
		)
		(fp_line
			(start -0.975 -2.45)
			(end 1.95 -2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "73f73cde-9281-4814-ba86-6b6fa631a19c")
		)
		(fp_line
			(start 1.95 -2.45)
			(end 1.95 2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e25f27f0-5aae-4dd3-a748-115a41f94039")
		)
		(fp_line
			(start 1.95 2.45)
			(end -1.95 2.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b9080d6e-71a3-4370-b0cc-7d45bfc7c6bc")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "b3f412d6-718c-4b26-b8ed-3f490112ee57")
			(effects
				(font
					(size 0.98 0.98)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 184 "Net-(U1-TXD)")
			(pinfunction "TXD")
			(pintype "input")
			(uuid "c7eaf8ac-aef8-455b-afc8-8fc3f77d9f86")
		)
		(pad "2" smd roundrect
			(at -2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(uuid "92d5d46e-bf31-4724-9d78-fd5112599b02")
		)
		(pad "3" smd roundrect
			(at -2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 167 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
			(uuid "b75330d6-30f6-4dd0-bee4-af6b70b7e6dd")
		)
		(pad "4" smd roundrect
			(at -2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 179 "Net-(U1-RXD)")
			(pinfunction "RXD")
			(pintype "output")
			(uuid "2f4d74fb-b4bb-4726-8b74-f5406e220b83")
		)
		(pad "5" smd roundrect
			(at 2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 177 "unconnected-(U1-Vio-Pad5)")
			(pinfunction "Vio")
			(pintype "power_in")
			(uuid "25dce587-1834-4350-a8d1-001f706ab98e")
		)
		(pad "6" smd roundrect
			(at 2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 181 "Net-(U1-CANL)")
			(pinfunction "CANL")
			(pintype "bidirectional")
			(uuid "b96817b5-c9a4-4077-a195-b7ab2a65dd7a")
		)
		(pad "7" smd roundrect
			(at 2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 182 "Net-(U1-CANH)")
			(pinfunction "CANH")
			(pintype "bidirectional")
			(uuid "2752da85-8e08-49da-875c-42c424e02fb8")
		)
		(pad "8" smd roundrect
			(at 2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 180 "unconnected-(U1-STBY-Pad8)")
			(pinfunction "STBY")
			(pintype "input")
			(uuid "740d61aa-90f8-4bdc-aafb-db10be57258f")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
		(layer "F.Cu")
		(uuid "985627e1-dadc-4969-84b1-fe0240f83775")
		(at 25.8 172.6 -90)
		(descr "Terminal Block Phoenix MKDS-3-2-5.08, 2 pins, pitch 5.08mm, size 10.2x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-3-2-5.08 pitch 5.08mm size 10.2x11.2mm^2 drill 1.3mm pad 2.6mm")
		(property "Reference" "J17"
			(at 2.54 -6.96 90)
			(layer "F.SilkS")
			(uuid "f8c27845-1c0d-409a-ab2f-9ae905da596a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 2.54 6.36 90)
			(layer "F.Fab")
			(uuid "dd838498-a82c-47c3-af73-ae9deedd07ad")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cc444411-ad1f-4503-adcb-f0fa6d535b74")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "53b42878-b69a-4cbe-a29f-062ff96e8daf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "81c4149d-d4c8-4635-ac54-91f7a8e546ea")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/eb409310-6102-43e5-b48c-2438ac1942c0/8337496e-1761-4ed3-ac07-07d584382a3f")
		(sheetname "ZeroCrossDetection")
		(sheetfile "ZeroCrossDetection.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.84 5.6)
			(end -2.34 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "13eb6cfd-dbf3-4ed5-a28e-79ee324516ba")
		)
		(fp_line
			(start -2.6 5.36)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dd865085-8f63-47be-a884-b12ebc23cb3a")
		)
		(fp_line
			(start -2.84 4.86)
			(end -2.84 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f46ddf7a-d97f-4a41-b701-bdec9c3507f9")
		)
		(fp_line
			(start -2.6 4.8)
			(end 7.68 4.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5425899a-04a3-48c0-9116-ce23dd2362d8")
		)
		(fp_line
			(start -2.6 2.3)
			(end 7.68 2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0e2f1161-f625-433c-939c-0b3295f023aa")
		)
		(fp_line
			(start -1.282 1.547)
			(end -1.388 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "efa5a385-9dcf-408e-be08-a0593770efa4")
		)
		(fp_line
			(start -1.548 1.281)
			(end -1.654 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "35b452d0-0d3f-45dc-b472-6f86d6938776")
		)
		(fp_line
			(start 4.073 1.274)
			(end 3.693 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b4926330-9b1a-4e1b-a383-e239d1de5544")
		)
		(fp_line
			(start 3.822 0.992)
			(end 3.427 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d2aae777-ff9e-44e1-a2df-02edb4f39f20")
		)
		(fp_line
			(start 1.654 -1.388)
			(end 1.547 -1.281)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c97fdfbb-4150-4564-b3fb-280e6e1ab245")
		)
		(fp_line
			(start 6.734 -1.388)
			(end 6.339 -0.992)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f82e0d85-0618-45fe-b51e-6dbd5c8bd287")
		)
		(fp_line
			(start 1.388 -1.654)
			(end 1.281 -1.547)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6efb960e-046d-4be7-81a2-163f91f8c221")
		)
		(fp_line
			(start 6.468 -1.654)
			(end 6.088 -1.274)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9fbbcea8-aa43-402f-a022-a326e40bcdfe")
		)
		(fp_line
			(start -2.6 -3.9)
			(end 7.68 -3.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "86e71941-bc36-4e6c-b5bd-778e70a1e1e6")
		)
		(fp_line
			(start -2.6 -5.96)
			(end -2.6 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1cc0d4a3-2cea-4039-9cf9-2c8f2f8538b5")
		)
		(fp_line
			(start -2.6 -5.96)
			(end 7.68 -5.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "771040d8-0df8-46d7-a761-8a68e4a19956")
		)
		(fp_line
			(start 7.68 -5.96)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6d94d19f-0565-4694-bb50-aca81f11dd15")
		)
		(fp_circle
			(center 0 0)
			(end 2.18 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "c0282253-e3d0-43d4-b1f4-dad13a230e2e")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.26 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "8dbceb15-7aca-454f-8b04-2b67894217bd")
		)
		(fp_line
			(start -3.04 5.8)
			(end 8.13 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "03296ab6-ea19-4438-a8de-b58db3a44776")
		)
		(fp_line
			(start 8.13 5.8)
			(end 8.13 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5cc12e1a-b616-43f0-8a59-74060ac9d93b")
		)
		(fp_line
			(start -3.04 -6.4)
			(end -3.04 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ff904837-72b5-4b56-b9dc-b006e0f3c20d")
		)
		(fp_line
			(start 8.13 -6.4)
			(end -3.04 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bebae440-ae24-4c3e-94a5-6dc06c7f3172")
		)
		(fp_line
			(start -2.04 5.3)
			(end -2.54 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "be353095-6d37-4c72-a7ec-841424d8708e")
		)
		(fp_line
			(start 7.62 5.3)
			(end -2.04 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bb4d87cf-511d-4424-ad2e-099e7b2baf73")
		)
		(fp_line
			(start -2.54 4.8)
			(end 7.62 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3c9e997c-c3e7-46b3-999b-49635d864e98")
		)
		(fp_line
			(start -2.54 4.8)
			(end -2.54 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c471349a-01f7-4d52-a9f0-46600a04d39c")
		)
		(fp_line
			(start -2.54 2.3)
			(end 7.62 2.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "57d6eaef-bdb9-4075-9179-7928391c6229")
		)
		(fp_line
			(start 1.517 -1.273)
			(end -1.273 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4d5e335a-67fe-4f17-b69f-6f68cdd64174")
		)
		(fp_line
			(start 6.597 -1.273)
			(end 3.808 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "97a7efa6-5fa0-450d-9bf5-db51bc0b8782")
		)
		(fp_line
			(start 1.273 -1.517)
			(end -1.517 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2114a03a-8978-46fd-a252-878825b0b715")
		)
		(fp_line
			(start 6.353 -1.517)
			(end 3.564 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ce0dda3c-8496-4b1b-b577-5c586923ef75")
		)
		(fp_line
			(start -2.54 -3.9)
			(end 7.62 -3.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0fd07284-a710-4413-91bb-b0203cf7c8c6")
		)
		(fp_line
			(start -2.54 -5.9)
			(end 7.62 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f52bd206-9a3c-4ce1-9653-e402a3d82c84")
		)
		(fp_line
			(start 7.62 -5.9)
			(end 7.62 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a856bc77-90f4-41f8-9951-3eafd4178cc4")
		)
		(fp_circle
			(center 0 0)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "a5b91cc5-8027-405a-b9b2-ee7d01f56af7")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.08 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "65f68451-4529-4c3a-a8b8-22142a5b7d80")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 3.1 90)
			(layer "F.Fab")
			(uuid "c2f73a59-d3c6-4708-bd13-40cb08802075")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 227 "Net-(J17-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "c138b6a9-c158-4670-a747-8f543847242d")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 226 "Net-(J17-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "b6d2a5d8-42ad-4199-b47a-f26d2faee92f")
		)
		(model "${KICAD8_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-6_W7.62mm"
		(layer "F.Cu")
		(uuid "99170411-3aa6-4159-85f4-561736144db3")
		(at 38 151.675)
		(descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U21"
			(at 4.44 -15.49 0)
			(layer "F.SilkS")
			(uuid "d230d29e-9b78-41e2-bf50-b04ab2f569a2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "H11AA1"
			(at 3.81 7.41 0)
			(layer "F.Fab")
			(uuid "9d720e9f-9500-4999-8a24-9c4c7385c8c5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8ca3050a-216a-4d14-84df-04bf06d42a4e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.vishay.com/docs/83608/h11aa1.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6b48de39-fa40-4134-8a59-f1ebe0428dca")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "AC/DC NPN Optocoupler, DIP-6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "735cf893-98f3-44a2-ac0b-f48f0826a389")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm*")
		(path "/e9267efd-e7bf-4ed4-9938-23d638b0f804/2b6fa8d2-7a33-45e1-b250-775e27348972")
		(sheetname "ZeroCrossDetection1")
		(sheetfile "ZeroCrossDetection.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9c551f44-e26f-45aa-880e-ecb513bb5f7a")
		)
		(fp_line
			(start 1.16 6.41)
			(end 6.46 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "34ba0519-db59-476b-a652-45aa8724597c")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "54c39166-e94b-4bda-9033-09331d41905c")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eee7069c-f2c4-4dcc-a4d9-aad637de0eda")
		)
		(fp_line
			(start 6.46 6.41)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c7e5c989-12c7-4ec4-bb94-b5db6b40eebe")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0c04b521-ce7e-4d1b-b05c-4d0725326727")
		)
		(fp_line
			(start -1.1 -1.55)
			(end -1.1 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b245de16-99dd-4c4c-8cce-5753859ec24f")
		)
		(fp_line
			(start -1.1 6.6)
			(end 8.7 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0230f662-7aae-4ddc-b63a-110d9b13bb6a")
		)
		(fp_line
			(start 8.7 -1.55)
			(end -1.1 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "29be08fc-fd71-42e5-ad13-ee67c2b3ddd8")
		)
		(fp_line
			(start 8.7 6.6)
			(end 8.7 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a3a7a2c1-ad43-44be-81a1-6be28351a6f2")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "16b5acc2-e7ae-48fc-9bfe-a2f24431dff9")
		)
		(fp_line
			(start 0.635 6.35)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e052e894-b31f-4bcd-9e2b-362046d883c6")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "68bd412c-19eb-49ab-9ef3-92c20c39db57")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "db5258f0-9c3e-4df6-9b92-8c45997a343f")
		)
		(fp_line
			(start 6.985 6.35)
			(end 0.635 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a7f22318-185e-4ae2-9783-104b4896652d")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.54 0)
			(layer "F.Fab")
			(uuid "1f8f7799-2960-4950-9780-536207d28f5b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 234 "Net-(R54-Pad2)")
			(pintype "passive")
			(uuid "c30cea00-eda3-425e-b583-32e85e18a2b3")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 235 "Net-(R55-Pad2)")
			(pintype "passive")
			(uuid "807e5431-c056-4dfe-a926-91a250d2fc52")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 222 "unconnected-(U21-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "54230e6e-296b-4fb5-ae6d-164d075ebd8e")
		)
		(pad "4" thru_hole oval
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "GND")
			(pintype "passive")
			(uuid "53f2a169-ce97-4950-b688-5fa162d6b9d2")
		)
		(pad "5" thru_hole oval
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 169 "/ZeroCrossDetection1/OUT")
			(pintype "passive")
			(uuid "78f51ef9-8a50-4556-b110-a4084413520b")
		)
		(pad "6" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 223 "unconnected-(U21-Pad6)")
			(pintype "passive")
			(uuid "ec7c3999-3d87-4ec5-918b-5a24f1dab2d4")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-6_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(uuid "9e099eea-917b-4397-8877-a4b231b69c7d")
		(at 35.114287 132.02 90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R22"
			(at 3.81 -1.92 90)
			(layer "F.SilkS")
			(uuid "35547f00-a329-41ca-ae47-f42633128aed")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "180"
			(at 3.81 1.92 90)
			(layer "F.Fab")
			(uuid "bb2ae2ef-be60-4fdf-aae6-ec08cd76c36c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6ab62f53-3750-4030-8402-93c38a9e0c46")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4ed89218-5b01-4de8-a0fd-f9ed2431ee70")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ce37bdc1-f1b8-4bce-929b-62d892505567")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/6df26bae-1f6b-42ab-99b6-42742cd98df0/4ab64e29-964f-40b2-bf58-c546b31cd3eb")
		(sheetname "Triac Circuit7")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 5.73 -0.92)
			(end 1.89 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b2729368-bd52-4e46-82d7-abf905e4bf83")
		)
		(fp_line
			(start 1.89 -0.92)
			(end 1.89 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7ce89920-9732-4ed4-8868-c905cf0e70d5")
		)
		(fp_line
			(start 6.68 0)
			(end 5.73 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6825387a-7c93-4967-a978-e2a9b840909c")
		)
		(fp_line
			(start 0.94 0)
			(end 1.89 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "378ce18b-08c5-460c-b766-e24d806f3253")
		)
		(fp_line
			(start 5.73 0.92)
			(end 5.73 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "acff6c3f-919e-4be9-a706-13685653e52f")
		)
		(fp_line
			(start 1.89 0.92)
			(end 5.73 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3efee7a3-c1d0-4d41-9c7b-fda4cb760918")
		)
		(fp_line
			(start 8.57 -1.05)
			(end -0.95 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "db4a489d-af0d-438c-b3f7-fb6990b65df7")
		)
		(fp_line
			(start -0.95 -1.05)
			(end -0.95 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7ce18872-c5f1-4f1e-ad90-cbdfb2a98b37")
		)
		(fp_line
			(start 8.57 1.05)
			(end 8.57 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3b250dea-448b-44f0-b916-d153b08d5e58")
		)
		(fp_line
			(start -0.95 1.05)
			(end 8.57 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6cfbbe27-5ec3-4bce-ab77-f3bf7c93baa5")
		)
		(fp_line
			(start 5.61 -0.8)
			(end 2.01 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b3f2051c-1b56-4f15-adfe-36c8a3c32f73")
		)
		(fp_line
			(start 2.01 -0.8)
			(end 2.01 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "813c15a1-1a51-4726-a693-a4d84a5bd147")
		)
		(fp_line
			(start 7.62 0)
			(end 5.61 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "72649a26-15b2-4f7c-801c-0f7a03c99159")
		)
		(fp_line
			(start 0 0)
			(end 2.01 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fadf44a1-357d-4b45-8295-59c5dbb6a9ab")
		)
		(fp_line
			(start 5.61 0.8)
			(end 5.61 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2ef4956b-d0e2-443f-8fa6-8df7c201e564")
		)
		(fp_line
			(start 2.01 0.8)
			(end 5.61 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ae8fc918-b9fa-4368-ab74-2efaa7afe877")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
			(uuid "827cdcba-88fb-4135-9295-db4cbd98cb2a")
			(effects
				(font
					(size 0.72 0.72)
					(thickness 0.108)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "Net-(R22-Pad1)")
			(pintype "passive")
			(uuid "b617d4ad-8bdd-4d53-b6d2-e18deea7ae94")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "/Triac Circuit7/High_Voltage_L")
			(pintype "passive")
			(uuid "26e9cb4b-3130-4614-aee5-c5f5b1ac1b2c")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(uuid "9f37a98d-e5ca-4bfa-bd4a-b98bb8cd74c2")
		(at 54.35 173.79)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(uuid "816d83b7-1721-4075-9bf0-ae4890f1d4e2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "22p"
			(at 0 1.85 0)
			(layer "F.Fab")
			(uuid "4fc52981-101f-4617-832c-459999807a56")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "3752a0a4-f9d1-4e18-b319-df58170f39ef")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c9e3e7a8-5a9e-4331-8118-4d1883ea52bd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "10d9fac1-09ad-430b-9f6c-0760ad855cc0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/d5a8abdf-d3e9-4f58-bdc3-40ada7bdd846")
		(sheetname "Główny")
		(sheetfile "16_ChannelPowerControlBoard.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.711252 -0.91)
			(end 0.711252 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fc6ea2ee-404d-43fc-87e5-60c3194c32f7")
		)
		(fp_line
			(start -0.711252 0.91)
			(end 0.711252 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6a8e159b-064c-4569-9d7e-1f7285b5af3b")
		)
		(fp_line
			(start -2.3 -1.15)
			(end 2.3 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "19d101c3-993d-4169-9231-6a3ed26925aa")
		)
		(fp_line
			(start -2.3 1.15)
			(end -2.3 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "959d6982-d350-4910-a04a-0d3dd106d37d")
		)
		(fp_line
			(start 2.3 -1.15)
			(end 2.3 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8a6d660c-857e-413f-b57e-6bb0cc3eba8d")
		)
		(fp_line
			(start 2.3 1.15)
			(end -2.3 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0d4095d3-7687-4558-8136-012f29b1cdc7")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "947ab749-28d7-480e-a863-904bbde6e31d")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ace052e3-8995-4a9f-9e79-cf73d656705b")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b77e2b1f-8a5f-4a0a-97c1-3893df31a969")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7c886e23-6b3f-4ceb-b220-d217e214e36c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "d13a6b57-3e31-4b92-a9c9-49e23f690daa")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 166 "Net-(U19-OSC1)")
			(pintype "passive")
			(uuid "a82477aa-f890-4891-8d5a-0e7018cb71f2")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 41 "GND")
			(pintype "passive")
			(uuid "d01ce3d0-f02c-4258-af9e-de6f192e944e")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "a0097a22-400e-4bca-8a2c-7f72664d6245")
		(at 53.605355 87.16 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R38"
			(at 0 -1.82 180)
			(layer "F.SilkS")
			(uuid "4214b277-5414-433e-a739-48134d9e4ba1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at 0 1.82 180)
			(layer "F.Fab")
			(uuid "02600c62-560b-4dc0-b0c6-f4baf0326d92")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "29bc6e29-949d-4c21-93d7-703a27cc465f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "877278f9-56b9-45aa-a690-658af37f26a5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "bcb55440-522e-4ef3-9309-06e34952cfec")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/fb144577-8e6f-488b-ba1b-870763a27401/de24ad75-a874-4d54-a682-b1d6f2079d30")
		(sheetname "Triac Circuit12")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "de55dfa4-4584-4596-9aaf-74360009f5be")
		)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "74189b4b-25a7-40ee-a015-a34e450cc4a6")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "300a45a1-a09f-46b0-9104-45d27c6d62cf")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ded8ac91-51c4-4b61-b9ba-bcc10fd7da12")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "976825bf-dcb9-4eb4-923c-79c5762ff86b")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5f38ac5c-7665-4b41-908e-7fe317e0224d")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b445eb42-6e91-40c5-b734-6b272ac32e48")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "54fa4cc9-654d-4d70-819a-084873369edb")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "26e967e8-703e-4d83-8177-de31b8b3fbf4")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ce589e57-a5cd-4446-a62b-eaceccd76431")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
			(uuid "428eb7e8-ff7f-499a-8606-f3a4dd9ca4a0")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 121 "Net-(R38-Pad1)")
			(pintype "passive")
			(uuid "e6a501d8-dcd0-401d-aaf9-8c827ce21545")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 37 "+3V3")
			(pintype "passive")
			(uuid "28139be8-0998-450a-87c1-03ac1f4de3cf")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "a0cf1c4d-e851-4637-ad26-695fedf8793c")
		(at 54.005355 61.679999)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q22"
			(at 0 -2.4 180)
			(layer "F.SilkS")
			(uuid "17fc9cb5-be91-4962-8400-3dee7fc3ac0a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BC818"
			(at 0 2.4 180)
			(layer "F.Fab")
			(uuid "bb26f563-460f-4c34-b032-bde5636a80c6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c70b1c33-031a-4323-b509-9c382a597750")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC818-D.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "56eb3a0f-d85a-4c84-8ae6-bb960d086f06")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e791d8ea-3886-4737-9cce-3fc3c4c4efd5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/d20c900a-3d9a-4460-9d5d-3ed4d11c2b93/00e550ea-8431-483d-ac3c-b4a719825546")
		(sheetname "Triac Circuit10")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -1.56)
			(end -1.675 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c00af652-6ec8-4cc8-9fa5-2b8bf9bf8003")
		)
		(fp_line
			(start 0 -1.56)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e32bdd55-6bd0-4c7f-ac3d-e8b695a5a5ce")
		)
		(fp_line
			(start 0 1.56)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "761ec313-ea1c-414e-8a0d-b7224d0b80f4")
		)
		(fp_line
			(start 0 1.56)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "eb9c63ac-d364-475a-b170-540032f76df2")
		)
		(fp_line
			(start -1.92 -1.7)
			(end -1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1392e04b-24bf-4148-aa91-3ad74a1cbe24")
		)
		(fp_line
			(start -1.92 1.7)
			(end 1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6c536590-9918-4c57-811a-efb6b6309264")
		)
		(fp_line
			(start 1.92 -1.7)
			(end -1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "47217092-4a19-4f6d-bd3d-fcaed40dc288")
		)
		(fp_line
			(start 1.92 1.7)
			(end 1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4e1771fb-8038-4d32-9b89-20ca49c1f65b")
		)
		(fp_line
			(start -0.65 -1.125)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "33736ea4-3c11-45bd-b08f-b56b07938a8c")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "04d4088d-2a0b-43fe-a2ba-44f623c755c5")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "15b65e24-162f-49aa-9fa4-aa0794508ea0")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3e50e7ae-80af-4bf3-b3ff-3699b31866ba")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e7a689ba-d553-4e31-ae4f-f9d7d6ddc966")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
			(uuid "27b74b0d-8a7b-4e61-8fc4-64e505022c5d")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 143 "Net-(Q22-B)")
			(pinfunction "B")
			(pintype "input")
			(uuid "38a844e6-21b4-43d6-a053-8e7cdb505694")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "GND")
			(pinfunction "E")
			(pintype "passive")
			(uuid "308e7c4b-d9e1-44e9-8b80-beafa5fb8ac2")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 144 "Net-(Q22-C)")
			(pinfunction "C")
			(pintype "passive")
			(uuid "e797c3e0-4284-49cc-b199-c700f90a4b2d")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "a1dd71fe-613b-4b21-87c1-1144b1b4681a")
		(at 48.508929 116.04)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R20"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "760aba6a-78ed-45f5-86f0-b131310c6ae3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "dc05a8f8-c637-486d-a682-73196634f808")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "88bec70b-e496-4058-a6c3-6c0cc475fed5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4a78fb0b-e6c4-4971-8444-0ad873dc7620")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "1ec96075-590b-4e68-bb12-efc852bdbd6e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/4a841339-199f-4bc7-a6bd-fe2a9936827c/de24ad75-a874-4d54-a682-b1d6f2079d30")
		(sheetname "Triac Circuit6")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dff4e086-2577-4526-9bd0-74ee2eb3480e")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "361ad93d-e263-4026-abad-6c26cc4556c0")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cda36321-ef59-4664-b885-a22aea624bb8")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0627fcd8-a86e-4a21-a05b-cf4031b0716b")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ec9bef77-1bbd-4100-b40e-98b21bf66e1b")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "82d7f940-7acc-4e3d-94c9-6043ad4aa22e")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "40c0625c-244a-48f0-b00d-1d1f5e65a87f")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2ff43d67-803c-4697-bf7e-48b0f76bb795")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2f3a8569-6c11-42cf-94b8-c5c3c49307b4")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0eb50b9a-d49c-4838-9407-9f705f22790a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "769487f7-7a56-4bc2-8c87-48eb485705b9")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 115 "Net-(R20-Pad1)")
			(pintype "passive")
			(uuid "af1b9a69-5a03-4598-bb95-d4d415377dca")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 37 "+3V3")
			(pintype "passive")
			(uuid "e12d42df-7eb9-4371-91d0-ba6bc285a262")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-6_W7.62mm"
		(layer "F.Cu")
		(uuid "a5d57aa4-43e9-495c-9022-5ead63638933")
		(at 38 162.275)
		(descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U22"
			(at 4.44 -15.49 0)
			(layer "F.SilkS")
			(uuid "b3c8da58-854b-4a5d-b987-a7d4fae92834")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "H11AA1"
			(at 3.81 7.41 0)
			(layer "F.Fab")
			(uuid "71094c0b-d0c6-4556-ba0a-60191ded269b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4bf375ff-a0d9-412b-ba51-ff2cb49f85aa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.vishay.com/docs/83608/h11aa1.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "336bd126-22ca-49cb-883c-cd9ec8ca4683")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "AC/DC NPN Optocoupler, DIP-6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a3632f51-546d-4045-bedf-5d2a1d2b16b6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm*")
		(path "/b0506013-ce11-444b-bc5e-374e3b418856/2b6fa8d2-7a33-45e1-b250-775e27348972")
		(sheetname "ZeroCrossDetection2")
		(sheetfile "ZeroCrossDetection.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ee5690f1-b2e9-40a8-a6b3-7e7d296905b2")
		)
		(fp_line
			(start 1.16 6.41)
			(end 6.46 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f3fbff1d-4bc6-4684-9766-b2fc6b371300")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fa7b70cc-1061-41a8-8705-0824189eec60")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b5b24970-2416-4138-8532-62165a7b1159")
		)
		(fp_line
			(start 6.46 6.41)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2bf2a72b-8b60-4f6a-90dd-66533d92cf7c")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dc873bbd-0b89-4317-9f61-04fd9cc8a758")
		)
		(fp_line
			(start -1.1 -1.55)
			(end -1.1 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "381fc5d8-8507-4bf4-bd15-07ea1e068fb8")
		)
		(fp_line
			(start -1.1 6.6)
			(end 8.7 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cccb6d2f-c6c4-439a-a64c-7f77b6206681")
		)
		(fp_line
			(start 8.7 -1.55)
			(end -1.1 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fa126bd3-2d96-4971-aade-867d022736ae")
		)
		(fp_line
			(start 8.7 6.6)
			(end 8.7 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e8c81f55-6d60-4906-a9fb-dca67c63b4d6")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3077530e-090c-45cc-b868-722eacff47db")
		)
		(fp_line
			(start 0.635 6.35)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e9d2e956-0399-4e1c-834f-7b0b5e44c610")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "32a638f8-9dba-44c8-b938-278f75424eb8")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b2602485-ccf8-4fb6-b820-621257349e3e")
		)
		(fp_line
			(start 6.985 6.35)
			(end 0.635 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7e49162a-39f0-4b10-9272-3800becd180e")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.54 0)
			(layer "F.Fab")
			(uuid "22f90a85-f9df-4f19-8b94-12d94529c5e4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 236 "Net-(R59-Pad2)")
			(pintype "passive")
			(uuid "34c23390-688c-4f27-90ce-64ca93b00a6c")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 237 "Net-(R60-Pad2)")
			(pintype "passive")
			(uuid "99ea1f61-0c14-4842-b38c-b5e311a7eeb5")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 225 "unconnected-(U22-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "4260188b-af4e-4c81-a29b-338b2f8df67a")
		)
		(pad "4" thru_hole oval
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "GND")
			(pintype "passive")
			(uuid "33850040-557e-4ddc-8d04-28ee0c00f5c3")
		)
		(pad "5" thru_hole oval
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 170 "/ZeroCrossDetection2/OUT")
			(pintype "passive")
			(uuid "309b20a6-d88a-4880-ae91-9ab5def4cc46")
		)
		(pad "6" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 224 "unconnected-(U22-Pad6)")
			(pintype "passive")
			(uuid "2fcdf2b4-b3cd-4de8-ba6d-2f9ad415909b")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-6_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(uuid "a7a7b8f6-7e66-43ef-863c-6ee151829075")
		(at 32.712145 50.94 -90)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "Q5"
			(at 6.04 -2.445 90)
			(layer "F.SilkS")
			(uuid "54232441-b802-4bd7-9bba-48dc89b1f757")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BTA16-600B"
			(at 2.54 2.5 90)
			(layer "F.Fab")
			(uuid "69f791c8-3fd0-47d7-a064-aab5505cf51b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "21dc0628-30e8-4b0e-923e-cba044df8806")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "dab41fe1-365c-4262-8971-3c3fcb45ee42")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "28e3451a-7e66-4e66-9363-9583776c7242")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO?220*")
		(path "/fef2553d-539f-40e4-b7bd-376e44ab9a6f/d1257be0-2394-4f08-8984-f580162b15f9")
		(sheetname "Triac Circuit2")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.58 1.371)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "50068ed6-2f22-4c6f-9c17-111688c0fdd3")
		)
		(fp_line
			(start -2.58 -1.76)
			(end 7.66 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e398ad2f-cfca-40d5-8f43-00b355ebbb52")
		)
		(fp_line
			(start -2.58 -3.27)
			(end -2.58 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ad4ecb22-3a14-4396-b5b8-ffefa729adc8")
		)
		(fp_line
			(start -2.58 -3.27)
			(end 7.66 -3.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d473b836-34a4-424b-9557-df2f68e2eb8b")
		)
		(fp_line
			(start 0.69 -3.27)
			(end 0.69 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ed496364-32fd-4147-9b54-ab941a4055e9")
		)
		(fp_line
			(start 4.391 -3.27)
			(end 4.391 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d9b053c0-0dea-432d-9a6d-cb22024bcfa5")
		)
		(fp_line
			(start 7.66 -3.27)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ff9a1477-cd6f-4b86-88c5-df881043a71a")
		)
		(fp_line
			(start -2.71 1.51)
			(end 7.79 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6b20af26-02b4-4ef6-b6ca-e9fd71615003")
		)
		(fp_line
			(start 7.79 1.51)
			(end 7.79 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d9da1069-4a25-4182-94bd-22a65aa14e5a")
		)
		(fp_line
			(start -2.71 -3.4)
			(end -2.71 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6023824e-c728-42d5-91dd-eb50a884f549")
		)
		(fp_line
			(start 7.79 -3.4)
			(end -2.71 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2cbfd710-6759-4821-91e4-c3adcffcce4a")
		)
		(fp_line
			(start -2.46 1.25)
			(end 7.54 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "37be7dc7-354d-4b7c-b8eb-e906d4bc745a")
		)
		(fp_line
			(start 7.54 1.25)
			(end 7.54 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bb22db90-9238-41c7-9527-1a3ff80bda76")
		)
		(fp_line
			(start -2.46 -1.88)
			(end 7.54 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1c4d41ac-4980-4e3a-b4f9-4a078994ec4b")
		)
		(fp_line
			(start -2.46 -3.15)
			(end -2.46 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "72c9d260-47aa-42d2-8c45-27d6417dcd83")
		)
		(fp_line
			(start 0.69 -3.15)
			(end 0.69 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a96b8617-0417-46be-a89f-dff4e7259b82")
		)
		(fp_line
			(start 4.39 -3.15)
			(end 4.39 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3920c9a9-aefb-4c0c-bd84-df5bf386bbc5")
		)
		(fp_line
			(start 7.54 -3.15)
			(end -2.46 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e30faebb-e7ef-42ea-bf66-edbbefbe5252")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 -4.27 90)
			(layer "F.Fab")
			(uuid "f563edf6-fb1d-4b94-bbe2-a02bc8de99db")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/Triac Circuit2/High_Voltage_L")
			(pinfunction "A1")
			(pintype "passive")
			(uuid "6ef612e9-1546-49ed-814b-b91586577722")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/Triac Circuit2/High_Voltage_Out")
			(pinfunction "A2")
			(pintype "passive")
			(uuid "ae2461ba-93a0-4bfa-aa43-afd88c58f82a")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(Q5-G)")
			(pinfunction "G")
			(pintype "input")
			(uuid "7633dbcb-34c3-4dc9-9dc7-f6c1c71a21df")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
		(layer "F.Cu")
		(uuid "b1c66dee-a826-42df-9589-7738fd57eb52")
		(at 77 121.84 90)
		(descr "Terminal Block Phoenix MKDS-3-2-5.08, 2 pins, pitch 5.08mm, size 10.2x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-3-2-5.08 pitch 5.08mm size 10.2x11.2mm^2 drill 1.3mm pad 2.6mm")
		(property "Reference" "J15"
			(at 3.1 -2.999999 -90)
			(layer "F.SilkS")
			(uuid "20f63ad3-1756-46d6-9b76-469172c0b3dd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 2.539999 6.36 90)
			(layer "F.Fab")
			(uuid "2b457347-f095-43ec-b5c0-0761181a87fc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "99ac14df-abbb-4d9b-a9ab-bcf56b5405f8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "675c6709-8013-499e-8e8b-0fbfa2e7b839")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "534bfc6f-2585-4437-97b7-e262cde82b66")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/683a6cfc-1cb6-4c63-ae1f-c9d1fdc220d0/60e4d8a3-c16e-48cd-a1fd-61f2968ecc7b")
		(sheetname "Triac Circuit14")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 7.68 -5.96)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e1392a73-d831-459d-9cc1-b3a27f058c6d")
		)
		(fp_line
			(start -2.6 -5.96)
			(end 7.68 -5.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "40a8bfaa-aa14-4cb5-9589-0e7142787c0a")
		)
		(fp_line
			(start -2.6 -5.96)
			(end -2.6 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1315b9fb-1da2-40a5-a000-722d9b26101d")
		)
		(fp_line
			(start -2.6 -3.9)
			(end 7.68 -3.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "286b8e01-e717-48e1-8231-52ee53e912ff")
		)
		(fp_line
			(start 6.468 -1.654)
			(end 6.088 -1.274)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ed76f3ab-5463-4b31-8d95-c566085bd655")
		)
		(fp_line
			(start 1.388 -1.654)
			(end 1.281 -1.547)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1d4ea9c5-58c5-472f-8e14-e65b186d72d0")
		)
		(fp_line
			(start 6.734 -1.388)
			(end 6.339 -0.992)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5837c1e3-167a-418e-863a-9cc24c75e41e")
		)
		(fp_line
			(start 1.654 -1.388)
			(end 1.547 -1.281)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "666b77c3-b382-4f0d-abc5-e83be74bf4c6")
		)
		(fp_line
			(start 3.822 0.992)
			(end 3.427 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0f057bfd-602d-42bc-8d2d-d4ece7003b4f")
		)
		(fp_line
			(start 4.073 1.274)
			(end 3.693 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3e12e489-17fd-456c-b979-845446630f91")
		)
		(fp_line
			(start -1.548 1.281)
			(end -1.654 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d0d7683a-fe03-4004-9112-e9d5286259b4")
		)
		(fp_line
			(start -1.282 1.547)
			(end -1.388 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bee1fbf0-928c-49bc-ad94-c01d17b1818f")
		)
		(fp_line
			(start -2.6 2.3)
			(end 7.68 2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dc1b83b4-6894-4d0d-a482-829f045c7714")
		)
		(fp_line
			(start -2.6 4.8)
			(end 7.68 4.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a2432df8-343c-4889-9dfb-1ffd82e49e18")
		)
		(fp_line
			(start -2.84 4.86)
			(end -2.84 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d8fb0261-6c2a-4c5f-815a-4f9515145e20")
		)
		(fp_line
			(start -2.6 5.36)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fb491de1-d034-4d36-99b2-c024caaa99b2")
		)
		(fp_line
			(start -2.84 5.6)
			(end -2.34 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a75fa6b4-7bed-416a-90c9-16c0bb0758e2")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.26 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "a326c425-37a5-42dc-9612-caff4bd50d85")
		)
		(fp_circle
			(center 0 0)
			(end 2.18 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "4674f36f-6f5c-459e-b0b2-c96e1ab609bc")
		)
		(fp_line
			(start 8.13 -6.4)
			(end -3.04 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "00903de7-77d7-44f0-adbb-e68d2eb22247")
		)
		(fp_line
			(start -3.04 -6.4)
			(end -3.04 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9b5452c2-22f3-406b-914f-8f0392c7ac3f")
		)
		(fp_line
			(start 8.13 5.8)
			(end 8.13 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "434b5055-96a6-48d6-8570-fac99c0b662a")
		)
		(fp_line
			(start -3.04 5.8)
			(end 8.13 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b37b6ef6-60f6-450a-8855-ebe9f059407e")
		)
		(fp_line
			(start 7.62 -5.9)
			(end 7.62 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "728b40f6-b99b-4fba-af3d-888861eed1d0")
		)
		(fp_line
			(start -2.54 -5.9)
			(end 7.62 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9a509534-f41b-478f-8a78-7de92c757607")
		)
		(fp_line
			(start -2.54 -3.9)
			(end 7.62 -3.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6169a05e-5e9c-4dad-85eb-ad19865d74c6")
		)
		(fp_line
			(start 6.353 -1.517)
			(end 3.564 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cfd5ee62-91a9-46a4-8cc1-bbb3e0f29985")
		)
		(fp_line
			(start 1.273 -1.517)
			(end -1.517 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8dd3f543-98d0-46cb-937c-46920cf90487")
		)
		(fp_line
			(start 6.597 -1.273)
			(end 3.808 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f43c826d-7f44-4944-8dc5-fc75b31eb9ec")
		)
		(fp_line
			(start 1.517 -1.273)
			(end -1.273 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9130706e-4354-4c7d-b071-15423c851c4b")
		)
		(fp_line
			(start -2.54 2.3)
			(end 7.62 2.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b448fd37-c5a8-4d05-8b90-c883936f5085")
		)
		(fp_line
			(start -2.54 4.8)
			(end -2.54 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "97a5c17e-eb0c-4aff-b70c-ec0d1200370c")
		)
		(fp_line
			(start -2.54 4.8)
			(end 7.62 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bc17eca4-f88c-4981-904b-ef0cd07087d3")
		)
		(fp_line
			(start 7.62 5.3)
			(end -2.04 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "85b95acb-722c-4485-8e96-69c305ffb860")
		)
		(fp_line
			(start -2.04 5.3)
			(end -2.54 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aa39afae-817c-409d-ba6e-4218387e9273")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.08 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "eac0e39c-a861-4806-a66a-a19e37a1f4fd")
		)
		(fp_circle
			(center 0 0)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "43fe9782-c5a4-40b7-9d76-be465868ef79")
		)
		(fp_text user "${REFERENCE}"
			(at 2.539999 3.1 90)
			(layer "F.Fab")
			(uuid "842f514f-b1b1-431e-ab4d-b236cb66b824")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 86 "/Triac Circuit14/High_Voltage_L")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "3ad557ab-76a4-440b-8340-d7bff9f9261d")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/Triac Circuit14/High_Voltage_Out")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "b156fa1a-54b5-4a39-9ed5-16176276a51f")
		)
		(model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(uuid "b2cd7dca-aef1-4e09-a300-90bf42351f7c")
		(at 66.942855 101.66 -90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R40"
			(at 3.809999 -1.92 -90)
			(layer "F.SilkS")
			(uuid "51cdc47a-1fd5-4fc3-9619-44afe994c7f5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "180"
			(at 3.81 1.919999 -90)
			(layer "F.Fab")
			(uuid "efa61d1e-b092-4237-8be6-2109bbf5be38")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e009fd8d-dc06-435d-8030-e802b5311dba")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b701fef0-dc3b-4389-ae8e-dea32aca358c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "99af4ed2-dae2-42fd-8b85-7718b998059e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/4a948621-4b4c-41c9-b07f-b928eecc9e1e/4ab64e29-964f-40b2-bf58-c546b31cd3eb")
		(sheetname "Triac Circuit13")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.89 0.92)
			(end 5.73 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "10eae1b5-111d-40a2-b473-c6c883a58bd8")
		)
		(fp_line
			(start 5.73 0.92)
			(end 5.73 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "91c1872d-a05e-4ac9-9663-f635b378273a")
		)
		(fp_line
			(start 0.94 0)
			(end 1.89 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f29006f9-9da7-4a79-ae44-c176ad4b7ff1")
		)
		(fp_line
			(start 6.68 0)
			(end 5.73 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8bcd80d4-1470-4017-8513-5edc636a0741")
		)
		(fp_line
			(start 1.89 -0.92)
			(end 1.89 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b6fe66eb-b5c6-40a6-9520-aee72bd769c7")
		)
		(fp_line
			(start 5.73 -0.92)
			(end 1.89 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dfb23087-5e28-4de8-82db-92e0069149a6")
		)
		(fp_line
			(start -0.95 1.05)
			(end 8.57 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c82be883-ce81-4dd7-a810-3648f48301f8")
		)
		(fp_line
			(start 8.57 1.05)
			(end 8.57 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e4d0c004-9c9b-43b9-a4b7-e79112f7eec3")
		)
		(fp_line
			(start -0.95 -1.05)
			(end -0.95 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b2a1114a-967a-4fb1-954d-24b50c5195ef")
		)
		(fp_line
			(start 8.57 -1.05)
			(end -0.95 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2f0ad125-5d8d-4c74-8504-e0968a0cd145")
		)
		(fp_line
			(start 2.01 0.8)
			(end 5.61 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "26b9a818-e289-4cc3-9ab4-391c7c835d5a")
		)
		(fp_line
			(start 5.61 0.8)
			(end 5.61 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "29c60583-6092-4fab-aa83-9b886815f15b")
		)
		(fp_line
			(start 0 0)
			(end 2.01 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "784b2416-7e3b-442b-b57e-2909eafb7eab")
		)
		(fp_line
			(start 7.62 0)
			(end 5.61 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e2a8d687-0a50-461c-9a03-fa18de7d06c2")
		)
		(fp_line
			(start 2.01 -0.8)
			(end 2.01 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aff14fe7-58a6-4318-bb56-4e5536010a94")
		)
		(fp_line
			(start 5.61 -0.8)
			(end 2.01 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "175f8794-145b-41bb-963f-500b5e7b224c")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 -90)
			(layer "F.Fab")
			(uuid "999733be-5df4-40ff-a28b-c6bd0ce3308d")
			(effects
				(font
					(size 0.72 0.72)
					(thickness 0.108)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(R40-Pad1)")
			(pintype "passive")
			(uuid "48567900-f34c-466e-ab5d-e06940047283")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 85 "/Triac Circuit13/High_Voltage_L")
			(pintype "passive")
			(uuid "8a315e20-c5aa-4e79-a504-28e6df12bea4")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
		(layer "F.Cu")
		(uuid "b50a57ff-20dd-412f-afa2-2fe2bd76e71c")
		(at 77 45.64 90)
		(descr "Terminal Block Phoenix MKDS-3-2-5.08, 2 pins, pitch 5.08mm, size 10.2x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-3-2-5.08 pitch 5.08mm size 10.2x11.2mm^2 drill 1.3mm pad 2.6mm")
		(property "Reference" "J10"
			(at 3.1 -2.999999 -90)
			(layer "F.SilkS")
			(uuid "8311a960-b983-4f92-9989-f6e08744c143")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 2.539999 6.36 90)
			(layer "F.Fab")
			(uuid "07806814-4ecb-43ae-86a9-33e54dc8a326")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "ef3909bb-fd54-4928-8ab3-de5991dbc5ec")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "02229ac2-305e-45ac-a8df-ad4cc67a16c1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "ad96931b-7b65-441c-b980-01c50ea7f3e8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/f251f0b5-0f8b-4418-bbfe-69d55a4bdeb8/60e4d8a3-c16e-48cd-a1fd-61f2968ecc7b")
		(sheetname "Triac Circuit9")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 7.68 -5.96)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3411d2f5-4681-45cd-bcd2-31c412f2ea69")
		)
		(fp_line
			(start -2.6 -5.96)
			(end 7.68 -5.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7ad09abb-1fad-413e-82ac-418d282f47ed")
		)
		(fp_line
			(start -2.6 -5.96)
			(end -2.6 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "af85abbf-ec94-4513-8f5e-232e00820ec9")
		)
		(fp_line
			(start -2.6 -3.9)
			(end 7.68 -3.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "40bc7c56-0b11-4959-88af-2e0231b4b357")
		)
		(fp_line
			(start 6.468 -1.654)
			(end 6.088 -1.274)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c01b3256-c7cc-445a-af2f-f629dc99196f")
		)
		(fp_line
			(start 1.388 -1.654)
			(end 1.281 -1.547)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ee50674c-d003-4724-85df-671a81d417b6")
		)
		(fp_line
			(start 6.734 -1.388)
			(end 6.339 -0.992)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d27c5060-a9ad-4ea1-b2ca-ae1eef866a41")
		)
		(fp_line
			(start 1.654 -1.388)
			(end 1.547 -1.281)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e99cd306-45e3-4353-819e-19bb298cca82")
		)
		(fp_line
			(start 3.822 0.992)
			(end 3.427 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ba32d301-ef41-468d-95aa-28f9236408b8")
		)
		(fp_line
			(start 4.073 1.274)
			(end 3.693 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b45e2ff9-8e3b-4d1a-af83-d47eefd1d4c8")
		)
		(fp_line
			(start -1.548 1.281)
			(end -1.654 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "54ea7091-4180-4016-b21f-9e41a6c9f072")
		)
		(fp_line
			(start -1.282 1.547)
			(end -1.388 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e5c79cb0-b114-405c-a60e-5b25d3296fb6")
		)
		(fp_line
			(start -2.6 2.3)
			(end 7.68 2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bd53a470-2bbd-46be-99dc-b3763dadf15a")
		)
		(fp_line
			(start -2.6 4.8)
			(end 7.68 4.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "24c2d91f-e7cb-4510-86d2-251039cabaa5")
		)
		(fp_line
			(start -2.84 4.86)
			(end -2.84 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3500bdd9-9354-4fe6-b347-c15e2d877291")
		)
		(fp_line
			(start -2.6 5.36)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1908fec7-b35f-4178-b9f2-48765f063c24")
		)
		(fp_line
			(start -2.84 5.6)
			(end -2.34 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "de6d244b-046c-4060-9c58-42c6b0d288be")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.26 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "16734bcc-9dba-4df7-8e00-2c275b3ad746")
		)
		(fp_circle
			(center 0 0)
			(end 2.18 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "8756f594-60db-4346-9b4d-8994bb086231")
		)
		(fp_line
			(start 8.13 -6.4)
			(end -3.04 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "51a470ec-a1ee-4afc-8085-54e9efb0c7bd")
		)
		(fp_line
			(start -3.04 -6.4)
			(end -3.04 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ee0e8bf9-9ced-4acd-a1e5-f66128201930")
		)
		(fp_line
			(start 8.13 5.8)
			(end 8.13 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "df5180d7-7895-4e12-aef9-9948988be7ac")
		)
		(fp_line
			(start -3.04 5.8)
			(end 8.13 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d9402465-7877-4912-92a5-1b33b4399ca4")
		)
		(fp_line
			(start 7.62 -5.9)
			(end 7.62 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "092fc09f-88c5-4627-a6ba-79bbdb59bf5d")
		)
		(fp_line
			(start -2.54 -5.9)
			(end 7.62 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "396681c6-637c-4ecd-a4d1-9838de7257c6")
		)
		(fp_line
			(start -2.54 -3.9)
			(end 7.62 -3.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "311d5c8c-8117-4f3b-ad3a-e3e0f84d0939")
		)
		(fp_line
			(start 6.353 -1.517)
			(end 3.564 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "490e28f9-73ba-4c4f-aaac-93e8cdea65f0")
		)
		(fp_line
			(start 1.273 -1.517)
			(end -1.517 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1a1b61a4-8ef1-4cd2-adda-9d4d8c39d703")
		)
		(fp_line
			(start 6.597 -1.273)
			(end 3.808 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e5a83062-59ea-4039-8ac4-024318ccd734")
		)
		(fp_line
			(start 1.517 -1.273)
			(end -1.273 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5f7cebe1-d642-43d2-aeed-b8eaaa27a99a")
		)
		(fp_line
			(start -2.54 2.3)
			(end 7.62 2.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "35374e46-6c64-4d01-b7c7-2021ab4252f9")
		)
		(fp_line
			(start -2.54 4.8)
			(end -2.54 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "de986f7e-bc2e-4f90-a91d-bb88f306200b")
		)
		(fp_line
			(start -2.54 4.8)
			(end 7.62 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "737e97c4-c666-4715-ac77-ecb7dfe8ae1d")
		)
		(fp_line
			(start 7.62 5.3)
			(end -2.04 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "336738f1-b7da-45ba-b6de-410ac76eae9d")
		)
		(fp_line
			(start -2.04 5.3)
			(end -2.54 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3c6e733d-589a-480f-b326-e0debebbfcef")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.08 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "b031c1a5-69df-447a-ac2a-f68869fb80f2")
		)
		(fp_circle
			(center 0 0)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "3b8d67cb-7f7d-4534-8f7f-5ea0190fc2a6")
		)
		(fp_text user "${REFERENCE}"
			(at 2.539999 3.1 90)
			(layer "F.Fab")
			(uuid "623b0f13-3dbc-4e04-884d-70d69f7567e8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "/Triac Circuit9/High_Voltage_L")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "2eb59b04-6142-464e-8a52-2fd24484c523")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/Triac Circuit9/High_Voltage_Out")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "ab213b2f-64a9-4132-bcdd-55ae82326659")
		)
		(model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "b88b14ed-d100-4a27-8901-8afccd03fa68")
		(at 54.005355 76.919999)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q24"
			(at 0 -2.4 180)
			(layer "F.SilkS")
			(uuid "3d7cb4cc-748b-440c-a6e2-ed7b2c945da0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BC818"
			(at 0 2.4 180)
			(layer "F.Fab")
			(uuid "3b604512-1fd3-406a-9f72-9ee3ace71cc9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c71a7938-495b-42c1-a4fb-bd179c5377e8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC818-D.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a250834b-49ee-471b-adae-67985b00f3a0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "be35ea17-70e4-454d-a32f-72a9a4bc1819")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/15d8fe7c-2a9b-438f-a777-3e4687188af1/00e550ea-8431-483d-ac3c-b4a719825546")
		(sheetname "Triac Circuit11")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -1.56)
			(end -1.675 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1e727393-7bec-4002-bd99-ffd1681ab279")
		)
		(fp_line
			(start 0 -1.56)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9e46d08f-ef3f-458f-ab67-b1dc9d8cef2f")
		)
		(fp_line
			(start 0 1.56)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "53df0cb5-e51b-48aa-a7ee-9a2048a7d868")
		)
		(fp_line
			(start 0 1.56)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1d6c69ae-ef1e-426b-9e2a-227151b858e6")
		)
		(fp_line
			(start -1.92 -1.7)
			(end -1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2f773d7f-bf3f-415e-a03f-2e6de2b0221a")
		)
		(fp_line
			(start -1.92 1.7)
			(end 1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f179eb9b-c4b1-48d3-91d9-871107e1f2d7")
		)
		(fp_line
			(start 1.92 -1.7)
			(end -1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5ccacea5-4bde-477f-8254-1e99b10e0166")
		)
		(fp_line
			(start 1.92 1.7)
			(end 1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "88050232-6c10-4c60-9a11-2b42c5f97e5c")
		)
		(fp_line
			(start -0.65 -1.125)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "63e46ad9-fd4d-40fa-a4a0-d26f656dcae5")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4ecc1561-5fc8-4a0e-a9e5-469a44e1651d")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ee006f7f-f243-47bc-bada-e745c2286be2")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cb090a2c-ce01-4058-8742-029f6d44ccb3")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1791ffd4-0319-4100-93d5-5e15c3634cb3")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
			(uuid "2a9c5ecd-5746-4c31-b63a-07c79f338ec8")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 146 "Net-(Q24-B)")
			(pinfunction "B")
			(pintype "input")
			(uuid "ecc62f80-5eee-4101-b20a-7be75ead3841")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "GND")
			(pinfunction "E")
			(pintype "passive")
			(uuid "78edd6be-af9f-4d95-b7e8-7a1d931ff13b")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 147 "Net-(Q24-C)")
			(pinfunction "C")
			(pintype "passive")
			(uuid "0f88fb67-d151-4774-a20d-6c8ed041d678")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(uuid "b8fca778-2703-46c3-ac4f-387ae873869d")
		(at 69.287855 91.3 90)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "Q25"
			(at 6.04 -2.444999 -90)
			(layer "F.SilkS")
			(uuid "82732a22-0a8e-4f94-9606-292abcc66231")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BTA16-600B"
			(at 2.539999 2.5 -90)
			(layer "F.Fab")
			(uuid "fe50ef8b-b873-4698-bb2d-71c531894424")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "0ada6992-83dd-4642-89c5-533a261f3d24")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "3f9b48b5-4faf-4066-b231-5eb364399f10")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "d8849335-db12-441e-ad9e-a58864b6ce11")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO?220*")
		(path "/fb144577-8e6f-488b-ba1b-870763a27401/d1257be0-2394-4f08-8984-f580162b15f9")
		(sheetname "Triac Circuit12")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 7.66 -3.27)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bf7ac0ef-7340-448d-b755-835b65d50fa3")
		)
		(fp_line
			(start 4.391 -3.27)
			(end 4.391 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b6606f19-fff1-487d-be61-eb2c787bb89a")
		)
		(fp_line
			(start 0.69 -3.27)
			(end 0.69 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "561b971b-8bc1-4e74-ab43-f07c4f7edcc8")
		)
		(fp_line
			(start -2.58 -3.27)
			(end 7.66 -3.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ce535ca3-0400-47bd-a602-109082cc007d")
		)
		(fp_line
			(start -2.58 -3.27)
			(end -2.58 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "44aa1c2e-0f11-4a77-a142-7ab4c3e9b648")
		)
		(fp_line
			(start -2.58 -1.76)
			(end 7.66 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ea19a654-9a2c-4bbf-b52e-eab9b3be51e6")
		)
		(fp_line
			(start -2.58 1.371)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b29a062f-8907-4549-a996-fbf4ef89b2da")
		)
		(fp_line
			(start 7.79 -3.4)
			(end -2.71 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f5edcea0-8be0-4d63-b7b9-b28aa2818277")
		)
		(fp_line
			(start -2.71 -3.4)
			(end -2.71 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "51b7a65b-9d59-466e-bf54-32eccee296ca")
		)
		(fp_line
			(start 7.79 1.51)
			(end 7.79 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b80278ca-7008-474e-bdda-a1488895674f")
		)
		(fp_line
			(start -2.71 1.51)
			(end 7.79 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "82923a94-2bab-47b8-96a7-0c7d1a390dbd")
		)
		(fp_line
			(start 7.54 -3.15)
			(end -2.46 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "44a9a675-aa33-4cd2-972f-777fb55d7ebb")
		)
		(fp_line
			(start 4.39 -3.15)
			(end 4.39 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e5e0e31c-763c-47b9-85df-548d22a434e8")
		)
		(fp_line
			(start 0.69 -3.15)
			(end 0.69 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "996d2eb6-ad27-44d6-91d3-bec69a60907a")
		)
		(fp_line
			(start -2.46 -3.15)
			(end -2.46 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5400b184-d727-40f6-a487-6c03e3bd7088")
		)
		(fp_line
			(start -2.46 -1.88)
			(end 7.54 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "39fa1d3f-d1d7-401f-bcac-3d66d8012681")
		)
		(fp_line
			(start 7.54 1.25)
			(end 7.54 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2535e55b-4f49-40dd-820f-6b4b844fb6d6")
		)
		(fp_line
			(start -2.46 1.25)
			(end 7.54 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "254d98d6-1301-41bb-8011-a06f1528c537")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 -4.27 -90)
			(layer "F.Fab")
			(uuid "aca6948f-7540-46a2-805a-0cf5f550e42e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 84 "/Triac Circuit12/High_Voltage_L")
			(pinfunction "A1")
			(pintype "passive")
			(uuid "798bc3c9-94d8-4a89-bffa-0ab56d1c6141")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/Triac Circuit12/High_Voltage_Out")
			(pinfunction "A2")
			(pintype "passive")
			(uuid "b93d7df4-8b8d-4f7c-a07f-915ccea79fb9")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 148 "Net-(Q25-G)")
			(pinfunction "G")
			(pintype "input")
			(uuid "23aa30b8-1017-473d-8103-034e65ddbb42")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(uuid "bb647afb-aec8-4db5-a1e9-52c3711f49b6")
		(at 54.35 167.09)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(uuid "546ea9fe-afeb-4471-887b-9ce6469fce8a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100n"
			(at 0 1.85 0)
			(layer "F.Fab")
			(uuid "d7bd33a8-afaa-4b92-9f03-cbdd2463b473")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1fca741e-4206-4842-9195-4b2780ac691e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "eac048cb-3f53-47a0-b02e-04fe8ee24182")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bf119c99-8722-4fe9-afb9-8952361b8aca")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/2cb99ef8-5ee2-445c-b221-0c3a60b94fcc")
		(sheetname "Główny")
		(sheetfile "16_ChannelPowerControlBoard.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.711252 -0.91)
			(end 0.711252 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7f3c30ed-579a-4ab4-832b-e4b4dd8e1e6f")
		)
		(fp_line
			(start -0.711252 0.91)
			(end 0.711252 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fcdc5afc-73c0-4aa2-a807-5bb538121c2b")
		)
		(fp_line
			(start -2.3 -1.15)
			(end 2.3 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "15a576a5-858f-43e7-aac9-1d44f9d8c537")
		)
		(fp_line
			(start -2.3 1.15)
			(end -2.3 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6bb689a4-4f43-4ffe-b395-a936e7e7b94d")
		)
		(fp_line
			(start 2.3 -1.15)
			(end 2.3 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7c7fb788-3ed9-430c-a1a2-ab21b3ef1903")
		)
		(fp_line
			(start 2.3 1.15)
			(end -2.3 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "28578847-1f3c-4def-b259-796e3b7cc00b")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dbe193e5-79dd-4f29-a82e-7f7f25917b8a")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c0a0dcf3-2c8f-4c18-a77e-a561ae97998b")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5487fd6a-811f-4dbc-87fe-8f535596a31b")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8517265b-a4ce-43bd-824f-799decf6cbec")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "e51af714-4212-43c5-959d-56d6cdde128b")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 167 "+3.3V")
			(pintype "passive")
			(uuid "28f5f967-0d25-49d6-a661-fed64b12875f")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 41 "GND")
			(pintype "passive")
			(uuid "4241906e-80b7-4532-a729-d2c2e11caef5")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "bd0d44ea-a6f2-4585-8e0a-299841f23436")
		(at 48.051787 126.28 180)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q16"
			(at 0 -2.4 0)
			(layer "F.SilkS")
			(uuid "030d3718-98a1-45ca-a7c3-29d7e25860f5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BC818"
			(at 0 2.4 0)
			(layer "F.Fab")
			(uuid "51c3d210-9f8d-456d-9abd-8e3d4cf81bc6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "306bcafd-8d91-427a-b2a8-442620f2a4c5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC818-D.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "6646fccd-9230-4a3f-aba4-c06225c11a1c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "2b592efe-46cb-4db4-8ab3-9ad3d6278e4e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/6df26bae-1f6b-42ab-99b6-42742cd98df0/00e550ea-8431-483d-ac3c-b4a719825546")
		(sheetname "Triac Circuit7")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 1.56)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "47a3a253-20ce-4629-9e53-95c28d35b2b4")
		)
		(fp_line
			(start 0 1.56)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aa3c6695-3363-4c8f-9c45-0c1847e781a0")
		)
		(fp_line
			(start 0 -1.56)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ce0b11f4-799e-4551-97a6-bc1c0e760a56")
		)
		(fp_line
			(start 0 -1.56)
			(end -1.675 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5dd4a6ef-644f-41bb-85ac-6e9f4569fb56")
		)
		(fp_line
			(start 1.92 1.7)
			(end 1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "51d3ef14-18dd-4130-8acb-4d54e2c9cc38")
		)
		(fp_line
			(start 1.92 -1.7)
			(end -1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4b16da43-98a6-4d6c-8b68-6417f0e18ae4")
		)
		(fp_line
			(start -1.92 1.7)
			(end 1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "aefc4eaf-7018-460f-8dfb-690def45d913")
		)
		(fp_line
			(start -1.92 -1.7)
			(end -1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "871e7dd2-e1b9-4e55-86aa-58b9dde60af2")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4b95ea75-03ca-468b-9d4a-1fc51c4785af")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bbdbc72a-51e7-408a-9086-e7d2a82ed296")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "723a577a-613c-40b4-90fb-2f88f7a80fa4")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cfd7e4d7-582b-4750-a356-7626c9418b53")
		)
		(fp_line
			(start -0.65 -1.125)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fb4958ab-467d-4807-971e-a9272bc4e935")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "560e533b-05be-45b4-b3ed-2e861dbcf728")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 74 "Net-(Q16-B)")
			(pinfunction "B")
			(pintype "input")
			(uuid "8e557d1c-abc7-486c-8b17-fe53eb0dab20")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "GND")
			(pinfunction "E")
			(pintype "passive")
			(uuid "81fd69af-d4e1-45fe-90e0-9713e112f8fc")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 126 "Net-(Q16-C)")
			(pinfunction "C")
			(pintype "passive")
			(uuid "7cc84b14-e51a-4945-b82c-e1c854597662")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(uuid "c187cae1-af77-44c0-832b-5d396cac2751")
		(at 69.287855 45.58 90)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "Q19"
			(at 6.04 -2.444999 -90)
			(layer "F.SilkS")
			(uuid "69cf63fc-d2c7-4699-b2e0-42d82002d4ac")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BTA16-600B"
			(at 2.539999 2.5 -90)
			(layer "F.Fab")
			(uuid "7dfa970b-6aba-40f3-b1c2-b41f56ab665c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "0629decf-59d3-439a-a44d-d0f9c5e5207d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "244dfbb5-617d-4dce-9945-f32f6c491030")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "7396ebd1-d269-44dc-9dfd-cd7fa8bdd5ec")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO?220*")
		(path "/f251f0b5-0f8b-4418-bbfe-69d55a4bdeb8/d1257be0-2394-4f08-8984-f580162b15f9")
		(sheetname "Triac Circuit9")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 7.66 -3.27)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "48de86b0-2fc7-41ae-b5b9-9652c391bbc8")
		)
		(fp_line
			(start 4.391 -3.27)
			(end 4.391 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3c376d6b-03e6-4876-ae77-20177090d7da")
		)
		(fp_line
			(start 0.69 -3.27)
			(end 0.69 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "40e26f72-ed7f-4b1e-b74a-1c16822462fc")
		)
		(fp_line
			(start -2.58 -3.27)
			(end 7.66 -3.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4c0a686f-d169-4320-9111-0c5fec089e54")
		)
		(fp_line
			(start -2.58 -3.27)
			(end -2.58 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "707a2e00-ee69-441c-8892-199ad5ad895b")
		)
		(fp_line
			(start -2.58 -1.76)
			(end 7.66 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ab56163b-1155-4802-8a6c-b254ab5b932d")
		)
		(fp_line
			(start -2.58 1.371)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8d4a9743-407b-43c8-b29d-4c196fca92d6")
		)
		(fp_line
			(start 7.79 -3.4)
			(end -2.71 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "39c9ae67-c75b-4282-bffa-38a0c72502db")
		)
		(fp_line
			(start -2.71 -3.4)
			(end -2.71 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9fc43957-c094-4ca0-b5c8-eb9e655ba710")
		)
		(fp_line
			(start 7.79 1.51)
			(end 7.79 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d8a7a645-009c-4f5a-863c-ae8f09ef11b3")
		)
		(fp_line
			(start -2.71 1.51)
			(end 7.79 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9c2a3534-0693-4c84-871a-3e36f940ca61")
		)
		(fp_line
			(start 7.54 -3.15)
			(end -2.46 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8051cd68-ebbf-4f6d-888e-5f322a4f4ddd")
		)
		(fp_line
			(start 4.39 -3.15)
			(end 4.39 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f71edb4a-04a2-4c76-b7e7-d5ec8d3688df")
		)
		(fp_line
			(start 0.69 -3.15)
			(end 0.69 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0dd0d3c9-5603-481c-a31b-387874cd7c4a")
		)
		(fp_line
			(start -2.46 -3.15)
			(end -2.46 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "46f9a056-3036-406b-a7ef-12c0b3c4e024")
		)
		(fp_line
			(start -2.46 -1.88)
			(end 7.54 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d8ee9ee3-337b-4de0-aa7b-fa3dd60c06d6")
		)
		(fp_line
			(start 7.54 1.25)
			(end 7.54 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7a8e9bfd-3bdf-405a-a908-91ee330c7b8d")
		)
		(fp_line
			(start -2.46 1.25)
			(end 7.54 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "124a3fec-0148-4fe1-a72b-7e5f9400f718")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 -4.27 -90)
			(layer "F.Fab")
			(uuid "9f6ee626-be7d-410c-a287-a3dde3d6ddd4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "/Triac Circuit9/High_Voltage_L")
			(pinfunction "A1")
			(pintype "passive")
			(uuid "32ec1454-8786-4ecc-b2d1-5f2c9f1e489d")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/Triac Circuit9/High_Voltage_Out")
			(pinfunction "A2")
			(pintype "passive")
			(uuid "e0d6354a-4dbd-42af-b384-7fbd01ef083f")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 139 "Net-(Q19-G)")
			(pinfunction "G")
			(pintype "input")
			(uuid "28400f7c-fbd6-4bbf-a4ec-81a32c4d8ac7")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "c1c00011-cb6a-44f4-b220-b795d7128643")
		(at 54.005355 137.879999)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q32"
			(at 0 -2.4 180)
			(layer "F.SilkS")
			(uuid "4e026368-4806-406a-8c5a-ddf5d394cbf6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BC818"
			(at 0 2.4 180)
			(layer "F.Fab")
			(uuid "c5a1030c-121c-4208-9eb1-21d22abe65b5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d67b6c05-af81-4b03-b79d-f6bf34949612")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC818-D.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d31d3698-62dc-4a53-81e7-875d3fe6b1be")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "bbe95eec-71e4-49bc-9e74-8d13ef2543f6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/4b0c0d83-8522-4ffe-8435-2c6bf5567543/00e550ea-8431-483d-ac3c-b4a719825546")
		(sheetname "Triac Circuit15")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -1.56)
			(end -1.675 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "08f29793-b4d4-4ed6-a1e8-6d87ea49ff32")
		)
		(fp_line
			(start 0 -1.56)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fca823b1-7edb-4ae2-8ac1-55e23bcab23d")
		)
		(fp_line
			(start 0 1.56)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0a4fbd9e-60d1-4387-9399-6f87dcbf1ccf")
		)
		(fp_line
			(start 0 1.56)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "689691df-efed-492e-8556-18d390ab6f3f")
		)
		(fp_line
			(start -1.92 -1.7)
			(end -1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "86608013-118f-47c4-9ca5-34a57f29a896")
		)
		(fp_line
			(start -1.92 1.7)
			(end 1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8e52f124-550b-4393-9abb-1311d2c6b9fe")
		)
		(fp_line
			(start 1.92 -1.7)
			(end -1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "78345805-b293-4e68-a877-6daf5f9ca36a")
		)
		(fp_line
			(start 1.92 1.7)
			(end 1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fb6bed43-7fd2-453c-818e-59c54005f3fd")
		)
		(fp_line
			(start -0.65 -1.125)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f260885f-2530-422c-9fef-d3834940107f")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9199d77e-76bc-4b94-bb22-2450b31939ed")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "79c81873-5f69-4d87-9a6d-6561ef80bc67")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b2804a6e-204b-4923-ac58-e9149a3b6265")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5f276950-1834-4dcd-813c-db1c0f48e356")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
			(uuid "a0ff6280-3a4f-4304-9523-9f8f9fa537b0")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 158 "Net-(Q32-B)")
			(pinfunction "B")
			(pintype "input")
			(uuid "e7f683d2-625b-4cae-81ec-6b155325979c")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "GND")
			(pinfunction "E")
			(pintype "passive")
			(uuid "ca5ad86e-ae93-4f75-bdb1-6f60b3cd4873")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 159 "Net-(Q32-C)")
			(pinfunction "C")
			(pintype "passive")
			(uuid "40a70d8a-6a78-4b9f-a877-e93360532ef3")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(uuid "c355a4c7-073f-4151-a5d4-acca8f042afe")
		(at 35.257142 101.54 90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R16"
			(at 3.81 -1.92 90)
			(layer "F.SilkS")
			(uuid "aee411ab-73f8-406c-a66f-2378734ba91a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "180"
			(at 3.81 1.92 90)
			(layer "F.Fab")
			(uuid "3c5ae913-93e4-4f23-a435-6cfc9c745cad")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "efdfdca6-1405-418e-9a93-d4e60170ccaa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ddbac60f-91da-4c7f-bfe4-3c78c721b490")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b258ccc4-6a53-4c5f-955f-aea16cbcf8eb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/6eb41966-4a54-4fd9-a1be-49d2f272d785/4ab64e29-964f-40b2-bf58-c546b31cd3eb")
		(sheetname "Triac Circuit5")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 5.73 -0.92)
			(end 1.89 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ca4942bb-34d0-4ab2-a88f-b815d086931f")
		)
		(fp_line
			(start 1.89 -0.92)
			(end 1.89 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "444f3302-aeaf-4f4d-aee0-8b68cfdf1dd9")
		)
		(fp_line
			(start 6.68 0)
			(end 5.73 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bdc0caea-6d01-4431-9e97-b11905f2eded")
		)
		(fp_line
			(start 0.94 0)
			(end 1.89 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9806ebc8-65d9-4dfc-9323-ba7644874d52")
		)
		(fp_line
			(start 5.73 0.92)
			(end 5.73 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f3f6e205-726e-4228-8fd3-da7992b51a35")
		)
		(fp_line
			(start 1.89 0.92)
			(end 5.73 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "964795c6-99ab-4f48-94a9-645a8925b2cb")
		)
		(fp_line
			(start 8.57 -1.05)
			(end -0.95 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "53e33fac-da6d-402f-8e5f-343bb2d0ba7f")
		)
		(fp_line
			(start -0.95 -1.05)
			(end -0.95 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bf1d9c01-85ad-4463-b9af-3b3e047e7891")
		)
		(fp_line
			(start 8.57 1.05)
			(end 8.57 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "719fabd7-ec0a-4f87-88a7-eb8ffde0b884")
		)
		(fp_line
			(start -0.95 1.05)
			(end 8.57 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a6e2fbb7-fbfb-4b40-8211-b541b6a0bef1")
		)
		(fp_line
			(start 5.61 -0.8)
			(end 2.01 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "31dfa01d-18e1-4bb7-8e8e-435a9f3bf5e1")
		)
		(fp_line
			(start 2.01 -0.8)
			(end 2.01 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1dfd5b2d-b4a9-4be5-b8b0-a1a585f3122a")
		)
		(fp_line
			(start 7.62 0)
			(end 5.61 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9d70e285-1dc5-4848-a7f0-d2b1491923e7")
		)
		(fp_line
			(start 0 0)
			(end 2.01 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e15feda6-2ee9-4783-a94b-716ad5c3a0be")
		)
		(fp_line
			(start 5.61 0.8)
			(end 5.61 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "39e2e9e3-bf5e-4af4-b3c2-6411211d5092")
		)
		(fp_line
			(start 2.01 0.8)
			(end 5.61 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ea30c39e-caf9-4119-922c-5734266b7d09")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
			(uuid "fcd9f835-d717-4fee-8331-3b20164f344b")
			(effects
				(font
					(size 0.72 0.72)
					(thickness 0.108)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(R16-Pad1)")
			(pintype "passive")
			(uuid "e16abb55-031d-4470-a964-30b0769ef9ad")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "/Triac Circuit5/High_Voltage_L")
			(pintype "passive")
			(uuid "ae247c9c-e342-4492-834d-793f36062929")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(uuid "c36c8700-1427-403e-94a3-dda529cae979")
		(at 35.8 160.06 -90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R59"
			(at 2.54 -1.92 90)
			(layer "F.SilkS")
			(uuid "5441c4a5-9585-4024-b3ef-6022068c2a08")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "220k"
			(at 2.54 1.92 90)
			(layer "F.Fab")
			(uuid "e3f5c98b-0ebe-4122-9a6f-ac4bbc1fa882")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8e6ff3e1-5106-42cb-96c7-362508901619")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1f61a022-d674-4736-be1a-27f5ca120b2b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "675744b4-164c-4ebd-a410-0a731839ab69")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/b0506013-ce11-444b-bc5e-374e3b418856/651d23d0-fccd-4821-a525-06dced80ce07")
		(sheetname "ZeroCrossDetection2")
		(sheetfile "ZeroCrossDetection.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 0.62 0.92)
			(end 4.46 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3a328ba8-05cf-4009-bbe4-ccba2cd409de")
		)
		(fp_line
			(start 0.62 -0.92)
			(end 4.46 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "269991c4-25d3-4a9c-a76c-977b49ccad2b")
		)
		(fp_line
			(start -0.95 1.05)
			(end 6.03 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c3e10aea-65c4-4f57-be0f-8285503a58f6")
		)
		(fp_line
			(start 6.03 1.05)
			(end 6.03 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "53d45ce5-0168-4acb-8f85-07a26436753f")
		)
		(fp_line
			(start -0.95 -1.05)
			(end -0.95 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9551e845-922d-44d4-80ec-33d4fe919c59")
		)
		(fp_line
			(start 6.03 -1.05)
			(end -0.95 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "943611c3-7309-4d15-80e3-1d3c70208b43")
		)
		(fp_line
			(start 0.74 0.8)
			(end 4.34 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "750aa0d6-df5d-4722-bac5-3f538d510254")
		)
		(fp_line
			(start 4.34 0.8)
			(end 4.34 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8e9ed028-d1d5-4335-bb43-ed87052aee50")
		)
		(fp_line
			(start 0 0)
			(end 0.74 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "de999fa0-80c2-4410-9132-bcadda9b75ef")
		)
		(fp_line
			(start 5.08 0)
			(end 4.34 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cf927fa9-3d6d-4bc5-8fdd-480bb931efe0")
		)
		(fp_line
			(start 0.74 -0.8)
			(end 0.74 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "efd58cd2-fa71-4400-bf05-9f55a71e20be")
		)
		(fp_line
			(start 4.34 -0.8)
			(end 0.74 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "28dc14d6-a15c-44ca-9b8c-32884ce6b51b")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 90)
			(layer "F.Fab")
			(uuid "8c2396b7-0df8-4ecd-9d3c-b3b2dfaf6c31")
			(effects
				(font
					(size 0.72 0.72)
					(thickness 0.108)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 231 "Net-(J19-Pin_1)")
			(pintype "passive")
			(uuid "599d412d-8036-4850-b679-4ce08684dc98")
		)
		(pad "2" thru_hole oval
			(at 5.08 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 236 "Net-(R59-Pad2)")
			(pintype "passive")
			(uuid "7bb6a97b-7e43-4b0f-9c32-af1e5cbe5ec1")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-6_W7.62mm"
		(layer "F.Cu")
		(uuid "c7c7fcee-00fa-4be5-92d7-372933f69035")
		(at 45.028571 85.285 180)
		(descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U6"
			(at 3.6 -2.33 0)
			(layer "F.SilkS")
			(uuid "c5a368f5-b3fc-4e41-aa47-9857a877b0e1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MOC3021M"
			(at 3.81 7.41 0)
			(layer "F.Fab")
			(uuid "187d044d-b0e0-40e7-9f32-b174cfce26d3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "35ca8ac3-4300-48be-b395-0478df11b84f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3023M-D.PDF"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "54c41158-ec71-478e-8106-8922f779f241")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "7468245d-ec05-488f-825b-dcf0921e9f21")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*")
		(path "/e56f6699-6dcd-4f6f-a67f-2156f450d5f1/0262e914-5435-478f-be04-ece49b8102cf")
		(sheetname "Triac Circuit4")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 6.46 6.41)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ac84fc73-2482-48c9-b605-8fb220a626a5")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8bcbc02c-86b5-4b5c-bcec-32acc5feea68")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1a772940-1a58-4f6f-ad33-324e7e42f7c4")
		)
		(fp_line
			(start 1.16 6.41)
			(end 6.46 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "18f06337-170c-4567-9e4e-4db52e1397aa")
		)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e2c38ef2-bae6-4798-b095-3f9b33b21d7c")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f037d58f-3c0e-41c8-92f2-1178ca5c0786")
		)
		(fp_line
			(start 8.7 6.6)
			(end 8.7 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "73a0c1d8-8427-4a86-aab4-deb7118db85f")
		)
		(fp_line
			(start 8.7 -1.55)
			(end -1.1 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d7f83495-be30-4a9f-b8b2-b316e59ecda5")
		)
		(fp_line
			(start -1.1 6.6)
			(end 8.7 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "414b3996-4a7c-434c-8a24-960b127495a7")
		)
		(fp_line
			(start -1.1 -1.55)
			(end -1.1 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e410fea6-5c01-4125-872e-41437a71af4b")
		)
		(fp_line
			(start 6.985 6.35)
			(end 0.635 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cc522953-08c7-4755-a9e8-2b91535cc293")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a3fbc01a-16a4-4634-b775-1c982ce105e6")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a7d7632d-a5d9-48b6-8bd6-1bab59f9e117")
		)
		(fp_line
			(start 0.635 6.35)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "df3032a7-5866-46b8-80da-1ed7f6644385")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d0a48f01-de40-4e3b-b2ad-b38657f2e256")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.54 0)
			(layer "F.Fab")
			(uuid "cea239e8-36d8-476b-a373-1b995f82be96")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 113 "Net-(R14-Pad1)")
			(pintype "passive")
			(uuid "4b618ee0-b258-404e-883e-932f24e6920f")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "Net-(Q10-C)")
			(pintype "passive")
			(uuid "8b79ca62-a50e-4a21-82b8-552fe4868877")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "unconnected-(U6-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "44b667e7-b807-4959-a032-288cc6ddabe7")
		)
		(pad "4" thru_hole oval
			(at 7.62 5.08 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(Q9-G)")
			(pintype "passive")
			(uuid "2350252a-831a-4a3f-b415-58ffbbf471c7")
		)
		(pad "5" thru_hole oval
			(at 7.62 2.54 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 92 "unconnected-(U6-NC-Pad5)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "25e64c29-7fa6-46fb-96c5-051fca98e40f")
		)
		(pad "6" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(R13-Pad1)")
			(pintype "passive")
			(uuid "533a19c1-b6ff-4ab7-bf84-eec1c97fbd65")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-6_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "c7e817e0-ba6d-4ae9-bfda-5f304867e3e3")
		(at 48.457145 52.88)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "7054d370-b592-4b76-9916-601c7db6771a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at -3.64 0 0)
			(layer "F.Fab")
			(uuid "0aa5d187-cd1b-434e-ac04-a4239ff779f5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "db2a06ca-e6dd-43e0-bfdf-d512878d174e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "503e4259-4122-4291-a879-f1b245b4bc4c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e44759cc-ca06-44fd-9038-d2e7e3b1667d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/fef2553d-539f-40e4-b7bd-376e44ab9a6f/ca31a324-056f-45d6-b948-82e97db62734")
		(sheetname "Triac Circuit2")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "624d2f49-55a9-4026-926e-56da40049d01")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7fdb7495-883d-4f65-8d5c-ea6abbcf2fa7")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "60ac9bbc-ab88-461c-84b2-ab062e70f4f4")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6987431d-46da-4786-8718-591cfd165b0a")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "acd18701-a4ed-492d-a44b-f46c0ff11a07")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bd58ad52-36c7-460d-b58d-1e0ca17757a0")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "855ed567-09e1-4ac3-90b0-f7e25f211a13")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c13cb299-c112-4746-b939-055f3bcd5f66")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f582a032-2f09-4662-8757-5c8bf0aa1311")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "84cf4453-2e8f-4291-a518-c15e255d2112")
		)
		(fp_text user "${REFERENCE}"
			(at 3.04 0.01 0)
			(layer "F.Fab")
			(uuid "ce8e88d7-f820-4969-922b-021b53795352")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 53 "Net-(Q6-B)")
			(pintype "passive")
			(uuid "693d4885-5c36-45ce-8a24-b4692a572558")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 24 "/Triac Circuit2/Enable")
			(pintype "passive")
			(uuid "e4d20864-fb88-4526-a011-fb7569f00b9f")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
		(layer "F.Cu")
		(uuid "c8d33ae3-b1bb-425c-9632-1a5ff0a82f74")
		(at 25.171426 81.36 -90)
		(descr "Terminal Block Phoenix MKDS-3-2-5.08, 2 pins, pitch 5.08mm, size 10.2x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-3-2-5.08 pitch 5.08mm size 10.2x11.2mm^2 drill 1.3mm pad 2.6mm")
		(property "Reference" "J5"
			(at 3.1 -3 90)
			(layer "F.SilkS")
			(uuid "9cae8b8a-1d36-492c-906e-1e3b18ed6ee4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 2.54 6.36 -90)
			(layer "F.Fab")
			(uuid "8362ee81-ff09-45c5-8ff4-a427944fe1bf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "d362f837-cf9b-4277-84c6-aa4306059954")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "350a3bd7-7dc3-4259-aa7e-ba3d95562b5c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "afcd413a-50f8-47cf-aabc-ee39a587d86d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/e56f6699-6dcd-4f6f-a67f-2156f450d5f1/60e4d8a3-c16e-48cd-a1fd-61f2968ecc7b")
		(sheetname "Triac Circuit4")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.84 5.6)
			(end -2.34 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f3311395-718c-453f-b87b-19d7c4b259ac")
		)
		(fp_line
			(start -2.6 5.36)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ae9dacba-9453-4cac-b019-f263134b4902")
		)
		(fp_line
			(start -2.84 4.86)
			(end -2.84 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3a12c42a-daa0-4395-b713-315d75953b72")
		)
		(fp_line
			(start -2.6 4.8)
			(end 7.68 4.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "724da257-a3f9-41cb-9da8-5a14b079ef19")
		)
		(fp_line
			(start -2.6 2.3)
			(end 7.68 2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "16bf5c1e-0b1d-432c-9163-f4a0e14fc019")
		)
		(fp_line
			(start -1.282 1.547)
			(end -1.388 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2459e34e-179f-4ede-9b4f-9fe624aab4a0")
		)
		(fp_line
			(start -1.548 1.281)
			(end -1.654 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "145ce915-8710-4c87-96e2-57bb165361a3")
		)
		(fp_line
			(start 4.073 1.274)
			(end 3.693 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fea3a71f-5e49-4cf0-ae05-f7abde4bc0eb")
		)
		(fp_line
			(start 3.822 0.992)
			(end 3.427 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e3f09f09-d5b9-4894-b08f-7c95d50a94b5")
		)
		(fp_line
			(start 1.654 -1.388)
			(end 1.547 -1.281)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1b6aca0f-d224-4c4f-8ebe-9f47ebd8f212")
		)
		(fp_line
			(start 6.734 -1.388)
			(end 6.339 -0.992)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "551768e8-0876-44a1-be23-8ae682391923")
		)
		(fp_line
			(start 1.388 -1.654)
			(end 1.281 -1.547)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "88142d9a-186e-48da-a4ed-3de8dee8e8c6")
		)
		(fp_line
			(start 6.468 -1.654)
			(end 6.088 -1.274)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2811e32d-1863-4ce6-81d9-51414367cc28")
		)
		(fp_line
			(start -2.6 -3.9)
			(end 7.68 -3.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e31d54f1-30da-4236-956a-9093a4708abb")
		)
		(fp_line
			(start -2.6 -5.96)
			(end -2.6 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "24ea605b-1876-4242-80a0-ab947c387de7")
		)
		(fp_line
			(start -2.6 -5.96)
			(end 7.68 -5.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8437ad65-9a8b-4a95-8d02-744cfad14ac3")
		)
		(fp_line
			(start 7.68 -5.96)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "66d2389d-05df-4d3a-ac7b-f25c3fde77f9")
		)
		(fp_circle
			(center 0 0)
			(end 2.18 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "9be0a28c-50fe-4be8-a111-a1049fdbde40")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.26 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "5ec8ea7f-d27b-4d72-8013-98dabbacfc78")
		)
		(fp_line
			(start -3.04 5.8)
			(end 8.13 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "582f7c9a-4d01-4226-be27-855c3644a9e6")
		)
		(fp_line
			(start 8.13 5.8)
			(end 8.13 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5d5e919a-a774-4fbe-8397-9db21b051106")
		)
		(fp_line
			(start -3.04 -6.4)
			(end -3.04 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bd377dce-f30d-4234-9733-eb5dc7a51040")
		)
		(fp_line
			(start 8.13 -6.4)
			(end -3.04 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e53538a6-bfad-4b8d-bfb9-57bcba514b56")
		)
		(fp_line
			(start -2.04 5.3)
			(end -2.54 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "063dac47-1771-46d7-857a-d35d5d17c328")
		)
		(fp_line
			(start 7.62 5.3)
			(end -2.04 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4e4d4f11-4184-490c-a3de-7bdd6c22c931")
		)
		(fp_line
			(start -2.54 4.8)
			(end 7.62 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a64e7aad-a13f-48a2-b8e4-18888b1cda75")
		)
		(fp_line
			(start -2.54 4.8)
			(end -2.54 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "47225f52-b965-4599-a537-2ffbfdf7be46")
		)
		(fp_line
			(start -2.54 2.3)
			(end 7.62 2.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "da07d263-d5d7-490c-ad5c-2a7515bb868d")
		)
		(fp_line
			(start 1.517 -1.273)
			(end -1.273 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f6337a4d-493e-4a52-8a29-b21bbeca080b")
		)
		(fp_line
			(start 6.597 -1.273)
			(end 3.808 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e5acce4d-21ce-4f7b-9e72-51dde80c44cf")
		)
		(fp_line
			(start 1.273 -1.517)
			(end -1.517 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5f802da9-c6f0-499c-a395-93a74dfd44ee")
		)
		(fp_line
			(start 6.353 -1.517)
			(end 3.564 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e735e70e-7353-45bf-8be3-eb632db7a667")
		)
		(fp_line
			(start -2.54 -3.9)
			(end 7.62 -3.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "de321433-2afe-4c70-a7f8-8df39e3eb5f3")
		)
		(fp_line
			(start -2.54 -5.9)
			(end 7.62 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "36c59dc6-c334-454b-bb19-6944576a3f46")
		)
		(fp_line
			(start 7.62 -5.9)
			(end 7.62 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0ab3438b-2c16-45ca-992a-5d1b0966ee20")
		)
		(fp_circle
			(center 0 0)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "845f4463-9ffa-4d67-8194-d8aff44effcc")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.08 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "5c71b8e9-b2a8-43a7-bd89-0488db354cd2")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 3.1 -90)
			(layer "F.Fab")
			(uuid "7d9cce8a-e58f-4463-9cce-e40b1134f19e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "/Triac Circuit4/High_Voltage_L")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "f72152af-9da4-475d-9288-c5f1754e7270")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/Triac Circuit4/High_Voltage_Out")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "a9e5d9b2-2082-4285-9e06-c12dc666bbc7")
		)
		(model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-6_W7.62mm"
		(layer "F.Cu")
		(uuid "cb7c4f01-c4a4-4eb2-aaaf-d77ff0930689")
		(at 44.942858 39.565 180)
		(descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U3"
			(at 3.6 -2.33 0)
			(layer "F.SilkS")
			(uuid "a721b709-1856-4473-8ce5-7d9599de3cf3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MOC3021M"
			(at 3.81 7.41 0)
			(layer "F.Fab")
			(uuid "0087987b-8453-4332-807a-7cf3e2ba2663")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "545a2096-18d5-4cab-8137-f69081014b3a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3023M-D.PDF"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "4ec1f43e-4bf8-4e48-939f-0d07a14cb58a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "01427db0-e123-4ca5-92bf-241c35b75f55")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*")
		(path "/98cc9bb7-a6bb-4cad-bced-cd34a966891d/0262e914-5435-478f-be04-ece49b8102cf")
		(sheetname "Triac Circuit1")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 6.46 6.41)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "efc85410-7839-47de-9d35-b88c4ac55285")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e25df870-3701-4c8e-a1c4-70d082e739ac")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3a6b6dc6-2c5c-4c36-972d-40102a07ec73")
		)
		(fp_line
			(start 1.16 6.41)
			(end 6.46 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "716e234a-6f26-482b-810a-adc1666c4b0d")
		)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c070e75e-c6ab-45b2-92ff-ea0f39554540")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1f0bad31-da8e-4a63-8855-a1ab62183e6a")
		)
		(fp_line
			(start 8.7 6.6)
			(end 8.7 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fc334026-44a6-43f6-b940-45eb368216f4")
		)
		(fp_line
			(start 8.7 -1.55)
			(end -1.1 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "80f02641-6966-48e5-bc17-c0ea80f0f345")
		)
		(fp_line
			(start -1.1 6.6)
			(end 8.7 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9b18da1a-233a-4040-93ea-99e36957e15c")
		)
		(fp_line
			(start -1.1 -1.55)
			(end -1.1 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bdc111bd-44f6-4134-9f4a-912e84054f8f")
		)
		(fp_line
			(start 6.985 6.35)
			(end 0.635 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "00d688f8-3d8a-46ee-b6bc-1579001a97e7")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1b4bf778-bace-4e2b-b935-4c182eb4ce45")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0eb10633-5e21-422e-8841-ce5991b720a3")
		)
		(fp_line
			(start 0.635 6.35)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c1d87e09-3668-4baf-b348-febd1d92899e")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4f5596e8-859a-4629-a076-6f85b156e482")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.54 0)
			(layer "F.Fab")
			(uuid "26cd6a17-ae2a-4a9b-8e4a-035348d6a44c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 110 "Net-(R5-Pad1)")
			(pintype "passive")
			(uuid "25d59ed3-2482-4794-b188-35667bbdb20a")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "Net-(Q4-C)")
			(pintype "passive")
			(uuid "3d3651a6-0373-4398-acbb-2568834c87b0")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 162 "unconnected-(U3-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "bf5f36cb-03c7-46e5-954c-8da83dd988b7")
		)
		(pad "4" thru_hole oval
			(at 7.62 5.08 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(Q3-G)")
			(pintype "passive")
			(uuid "f11235da-4039-4266-9dce-a8e371333f44")
		)
		(pad "5" thru_hole oval
			(at 7.62 2.54 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 163 "unconnected-(U3-NC-Pad5)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "ae7063b8-eec0-49a4-bc2f-915e1b998536")
		)
		(pad "6" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "Net-(R4-Pad1)")
			(pintype "passive")
			(uuid "f5627f6f-120b-4f92-89ff-be42a61ccf8c")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-6_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-6_W7.62mm"
		(layer "F.Cu")
		(uuid "ce5f6d68-d9f1-43b0-bb9d-a7b7d6dbc250")
		(at 45.057142 100.525 180)
		(descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U7"
			(at 3.6 -2.33 0)
			(layer "F.SilkS")
			(uuid "9494476f-ef6a-4f0b-b51d-e1eae7190ea3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MOC3021M"
			(at 3.81 7.41 0)
			(layer "F.Fab")
			(uuid "08166c13-7fb3-49ec-aaf2-3881a5857ea2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "69a48ed1-488a-4b80-94ed-51592439a383")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3023M-D.PDF"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "dcf154dd-dfee-45fb-b357-9d0199904bdb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "cbdb2513-2e0f-4d3c-b8d1-5250f1c737d1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*")
		(path "/6eb41966-4a54-4fd9-a1be-49d2f272d785/0262e914-5435-478f-be04-ece49b8102cf")
		(sheetname "Triac Circuit5")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 6.46 6.41)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "937535ce-0201-4aed-b07d-78f529c2872e")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "15f24ea2-d8ae-4c1b-8ec0-e9e4fd3aa1ae")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "12909d15-e747-4a63-9f4c-b362d8b09568")
		)
		(fp_line
			(start 1.16 6.41)
			(end 6.46 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b56e6375-c37e-41ab-92d1-6627aaa07ef6")
		)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fd412168-ce5a-4a4b-be09-34e80acfa045")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9fe8431e-d250-4029-ad1b-24b8f306128d")
		)
		(fp_line
			(start 8.7 6.6)
			(end 8.7 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1b3e23e5-6de6-47b8-8956-a6a9835f3355")
		)
		(fp_line
			(start 8.7 -1.55)
			(end -1.1 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "46c57134-4e03-4851-ae33-7d4af37d2658")
		)
		(fp_line
			(start -1.1 6.6)
			(end 8.7 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c0ee35eb-ccea-4a68-815b-fc87f69fb1bd")
		)
		(fp_line
			(start -1.1 -1.55)
			(end -1.1 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "86dde827-d20d-47e1-9715-1951af6d91e6")
		)
		(fp_line
			(start 6.985 6.35)
			(end 0.635 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "42549741-457e-4c5c-940b-1df417cc7db5")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "06dd281b-c98f-4a79-8b6d-9812daaf4bb4")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "162f3d5a-e440-41df-9a54-07a5132a2fe9")
		)
		(fp_line
			(start 0.635 6.35)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "49ad5333-565c-4d85-8935-14ae27a9a7d4")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8a3ef9f4-2635-459d-992f-dbb10e5bea98")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.54 0)
			(layer "F.Fab")
			(uuid "52665618-69b8-4115-8634-596be0242eb6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 114 "Net-(R17-Pad1)")
			(pintype "passive")
			(uuid "f3e37532-d809-4ce9-886b-f3b3c7e142ca")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "Net-(Q12-C)")
			(pintype "passive")
			(uuid "d66e243d-00a2-48c7-b93e-2d14ac3b878b")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 93 "unconnected-(U7-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "54e633da-4c43-44f5-a8c5-1f9de4de305f")
		)
		(pad "4" thru_hole oval
			(at 7.62 5.08 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(Q11-G)")
			(pintype "passive")
			(uuid "17ac530a-e9bd-48fb-8d4d-df22437b80ce")
		)
		(pad "5" thru_hole oval
			(at 7.62 2.54 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 94 "unconnected-(U7-NC-Pad5)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "ac0e390c-0796-4103-aa46-af823693d69d")
		)
		(pad "6" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(R16-Pad1)")
			(pintype "passive")
			(uuid "e8de2f47-1b91-40a3-bc82-0b79e42c00cd")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-6_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "cec5840d-5f9d-4c21-a378-31c674a78777")
		(at 53.542855 119.84 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R45"
			(at 0 -1.82 180)
			(layer "F.SilkS")
			(uuid "f883ef12-cecb-4b68-aeff-3c3494780251")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at -3.64 0 180)
			(layer "F.Fab")
			(uuid "5885058b-912d-41af-8379-0178908b40eb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "0c6f15cb-5514-4d44-819c-5605985ff4dc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "18e42298-1242-4b69-99e1-520e37aaf82d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "07d65a67-ee92-4cc5-92b7-ac684fb7f976")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/683a6cfc-1cb6-4c63-ae1f-c9d1fdc220d0/ca31a324-056f-45d6-b948-82e97db62734")
		(sheetname "Triac Circuit14")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e9ade4da-d6d0-4cff-9a78-03aa3592e3ca")
		)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ae8c28a5-5f9e-40b5-ad38-f4958dc61f60")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9eb0bc53-3fbf-4d5e-b5d1-bd3b2353b1f6")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "de2c2935-fe4b-4150-ad07-8abee5ab120b")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8f8a3e78-6b2f-4357-9844-41fccc16fe73")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e5df9794-1398-4e27-b9c8-1dc510df67e5")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "49f16bed-aace-45fd-adf1-2b297c0e8522")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "74f4d084-c239-4771-bb9d-8eb894bc66ca")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "07dd5f62-e587-4daf-8b9a-23fca2828468")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "23123e42-75d0-43b0-9621-e0f69246e803")
		)
		(fp_text user "${REFERENCE}"
			(at 3.04 0.01 180)
			(layer "F.Fab")
			(uuid "a1be515e-a7bb-43c1-b1bb-0aba8f0efd17")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 155 "Net-(Q30-B)")
			(pintype "passive")
			(uuid "63d50fba-15e0-4ef3-a56c-3c64c078a7cc")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 137 "/Triac Circuit14/Enable")
			(pintype "passive")
			(uuid "394eb892-83c7-42b8-9b9c-326149318b9b")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(uuid "d22b8d01-66ef-4ca9-8988-028258f78956")
		(at 69.287855 30.34 90)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "Q17"
			(at 6.04 -2.444999 -90)
			(layer "F.SilkS")
			(uuid "804159b7-f70f-47e5-8a2a-8fd3f9844955")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BTA16-600B"
			(at 2.539999 2.5 -90)
			(layer "F.Fab")
			(uuid "5959e092-1011-4185-a206-97c3a82e8231")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "ee95eb14-5dd7-4c6d-878a-6295321d1857")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "a46eff5b-65fb-4d6a-a161-5f7746132c5e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "42fb0664-d771-4b71-aafb-f82a8717b971")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO?220*")
		(path "/a837c47c-5707-46fe-8eca-0b07e116b13e/d1257be0-2394-4f08-8984-f580162b15f9")
		(sheetname "Triac Circuit8")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 7.66 -3.27)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "60a93900-c55e-47c1-977c-7aa5d9c58bf1")
		)
		(fp_line
			(start 4.391 -3.27)
			(end 4.391 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "63ae098c-ce4c-4cfe-b7bb-80c90873dba3")
		)
		(fp_line
			(start 0.69 -3.27)
			(end 0.69 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "13f182c4-a8d2-40cf-a6d6-818308e5f679")
		)
		(fp_line
			(start -2.58 -3.27)
			(end 7.66 -3.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d0c54da3-bc00-41ea-baf2-13bbbfeb7c82")
		)
		(fp_line
			(start -2.58 -3.27)
			(end -2.58 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9af58f22-13de-470b-8f62-1ded378bdd8e")
		)
		(fp_line
			(start -2.58 -1.76)
			(end 7.66 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "73d7df82-407e-4953-b571-1a6fcf0604cf")
		)
		(fp_line
			(start -2.58 1.371)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f4dd20a2-ec75-4154-b0ad-fc369f6a3857")
		)
		(fp_line
			(start 7.79 -3.4)
			(end -2.71 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0a2c0e57-f2be-450b-a9ce-11ba5ecde648")
		)
		(fp_line
			(start -2.71 -3.4)
			(end -2.71 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "77630801-24ae-488f-98b6-930a2b643613")
		)
		(fp_line
			(start 7.79 1.51)
			(end 7.79 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9a1f7322-af0d-4c2d-be9c-59dbd302ef09")
		)
		(fp_line
			(start -2.71 1.51)
			(end 7.79 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b85506e0-2df3-474c-8bd4-02e5e581d092")
		)
		(fp_line
			(start 7.54 -3.15)
			(end -2.46 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1e15c1fc-f6c2-4a98-b3a4-f9726cc56b47")
		)
		(fp_line
			(start 4.39 -3.15)
			(end 4.39 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5d79de79-85ff-4f2c-9f12-26d4575de7ba")
		)
		(fp_line
			(start 0.69 -3.15)
			(end 0.69 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f5ed9d74-47fc-4d15-9f94-112f2a8a9c97")
		)
		(fp_line
			(start -2.46 -3.15)
			(end -2.46 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c07ea0c8-1486-4cf4-af90-4ddc8d1b2ef6")
		)
		(fp_line
			(start -2.46 -1.88)
			(end 7.54 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3b26a2e7-6212-4e3c-9f42-02d8b6364fd4")
		)
		(fp_line
			(start 7.54 1.25)
			(end 7.54 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "17e5d0e3-1317-4b8b-9c8f-7fa1ba87b639")
		)
		(fp_line
			(start -2.46 1.25)
			(end 7.54 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "29104d22-d136-48b4-8ce3-f54a4019898e")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 -4.27 -90)
			(layer "F.Fab")
			(uuid "fad59245-a073-4da6-b592-4c1c12ef55cd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "/Triac Circuit8/High_Voltage_L")
			(pinfunction "A1")
			(pintype "passive")
			(uuid "041a2602-61fd-4559-89cf-bc1e27eb966e")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/Triac Circuit8/High_Voltage_Out")
			(pinfunction "A2")
			(pintype "passive")
			(uuid "b214c8e3-eaaa-4d21-b62c-f5fed5c5b92e")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "Net-(Q17-G)")
			(pinfunction "G")
			(pintype "input")
			(uuid "ee0b28e4-3e63-4007-8dda-7d0332697dca")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(uuid "d5f7dfce-1639-4838-98b9-48a4e04a7873")
		(at 32.740716 66.18 -90)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "Q7"
			(at 6.04 -2.445 90)
			(layer "F.SilkS")
			(uuid "3efe32bf-2d23-4258-a01b-a1bb3a516255")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BTA16-600B"
			(at 2.54 2.5 90)
			(layer "F.Fab")
			(uuid "2d9d7d1d-a71c-4b67-a5db-886c7979b0a1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "e49b1304-18a3-4687-8951-ef16ecca480d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "40a73079-634c-4c3b-8641-fa77f3ba4fa0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "743933ad-ce5c-428a-a7c7-f6b3c867879f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO?220*")
		(path "/1abc9394-30bb-4ef5-a1be-aa230dbd1566/d1257be0-2394-4f08-8984-f580162b15f9")
		(sheetname "Triac Circuit3")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.58 1.371)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9063183f-a9c3-4696-8e41-9e27249f1248")
		)
		(fp_line
			(start -2.58 -1.76)
			(end 7.66 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "330f5668-3a61-492e-b66e-e9b12abcf279")
		)
		(fp_line
			(start -2.58 -3.27)
			(end -2.58 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3086f9a3-4763-4eba-9b61-98e72a6fe629")
		)
		(fp_line
			(start -2.58 -3.27)
			(end 7.66 -3.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6c9ab917-4f42-4074-a359-3d7c4e215232")
		)
		(fp_line
			(start 0.69 -3.27)
			(end 0.69 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "48884012-37fd-4034-a45e-810d293d9fdb")
		)
		(fp_line
			(start 4.391 -3.27)
			(end 4.391 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bb12f75b-5b6b-467d-b830-3b7f39470587")
		)
		(fp_line
			(start 7.66 -3.27)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "05df196c-1c1c-4abc-abaa-a52661112066")
		)
		(fp_line
			(start -2.71 1.51)
			(end 7.79 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c3771ea1-fecd-49b8-9e9e-4325b363f1dc")
		)
		(fp_line
			(start 7.79 1.51)
			(end 7.79 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ba58d609-743f-4014-aa37-0a25c2bc3210")
		)
		(fp_line
			(start -2.71 -3.4)
			(end -2.71 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f9c6b2a9-a9a5-497e-8ce7-09b3b3f614ea")
		)
		(fp_line
			(start 7.79 -3.4)
			(end -2.71 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "213814a9-dda5-4ff8-9dba-748a6f0f6778")
		)
		(fp_line
			(start -2.46 1.25)
			(end 7.54 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f922a164-59d1-4e46-a103-9a7851c251f1")
		)
		(fp_line
			(start 7.54 1.25)
			(end 7.54 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fadde9ca-1834-4bf8-9c28-e756964a2185")
		)
		(fp_line
			(start -2.46 -1.88)
			(end 7.54 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "59917391-c759-4a55-beb6-9e0f8b51b2e0")
		)
		(fp_line
			(start -2.46 -3.15)
			(end -2.46 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "08b2439f-c050-44d0-b23f-1f51a531518d")
		)
		(fp_line
			(start 0.69 -3.15)
			(end 0.69 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2dab835b-069b-4c75-b972-266689e939f9")
		)
		(fp_line
			(start 4.39 -3.15)
			(end 4.39 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a924a564-bfe6-49ac-b4ca-dc55bcd1c977")
		)
		(fp_line
			(start 7.54 -3.15)
			(end -2.46 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b36327a3-ab4d-45c9-a38d-d07e0f402376")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 -4.27 90)
			(layer "F.Fab")
			(uuid "6dc4b622-41da-413a-8734-f5dade4bce22")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/Triac Circuit3/High_Voltage_L")
			(pinfunction "A1")
			(pintype "passive")
			(uuid "7239e381-8cc1-4867-94d8-c1c695326720")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/Triac Circuit3/High_Voltage_Out")
			(pinfunction "A2")
			(pintype "passive")
			(uuid "5ee423a9-a2ad-4c56-bdab-6de28326d4f6")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(Q7-G)")
			(pinfunction "G")
			(pintype "input")
			(uuid "c98745c4-2e90-4796-85a9-a3b7080fc53e")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
		(layer "F.Cu")
		(uuid "d659d3a7-68d6-4a8c-b71a-e214c23f49e4")
		(at 25.8 162.08 -90)
		(descr "Terminal Block Phoenix MKDS-3-2-5.08, 2 pins, pitch 5.08mm, size 10.2x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-3-2-5.08 pitch 5.08mm size 10.2x11.2mm^2 drill 1.3mm pad 2.6mm")
		(property "Reference" "J19"
			(at 2.54 -6.96 90)
			(layer "F.SilkS")
			(uuid "cf7b5752-c162-48c3-a5eb-4858d498e1ab")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 2.54 6.36 90)
			(layer "F.Fab")
			(uuid "07274831-ba66-43d6-89ab-a266d1c6c8d8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1369fe89-9403-40de-b6e0-89f620fabfd8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2772912d-0b2e-432e-8987-8295c23dffd9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "128ec35c-1149-4c19-907b-391506d2b121")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/b0506013-ce11-444b-bc5e-374e3b418856/8337496e-1761-4ed3-ac07-07d584382a3f")
		(sheetname "ZeroCrossDetection2")
		(sheetfile "ZeroCrossDetection.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.84 5.6)
			(end -2.34 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "44c7f418-7ebe-4dec-b729-def6b2539aff")
		)
		(fp_line
			(start -2.6 5.36)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e6320906-3f4b-4d10-8453-b4ca72919a46")
		)
		(fp_line
			(start -2.84 4.86)
			(end -2.84 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b8ad8774-4daf-41e5-bd6e-35e6510c9728")
		)
		(fp_line
			(start -2.6 4.8)
			(end 7.68 4.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e53d041a-1a6f-4341-83fe-84494067fa11")
		)
		(fp_line
			(start -2.6 2.3)
			(end 7.68 2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4b3a311c-5c2e-4c2a-89bb-f3f25217d40a")
		)
		(fp_line
			(start -1.282 1.547)
			(end -1.388 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "57b5f1ff-121c-4934-98a6-882a297f24e2")
		)
		(fp_line
			(start -1.548 1.281)
			(end -1.654 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fcbdfa7b-736a-4b41-8ab4-54b455cacb82")
		)
		(fp_line
			(start 4.073 1.274)
			(end 3.693 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bd716985-5f68-450e-b875-48b84ab031bc")
		)
		(fp_line
			(start 3.822 0.992)
			(end 3.427 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c12e2c82-e0b2-45b2-a82e-4cf3735061dc")
		)
		(fp_line
			(start 1.654 -1.388)
			(end 1.547 -1.281)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "326accc1-56ea-4374-a848-c0bef44abbd6")
		)
		(fp_line
			(start 6.734 -1.388)
			(end 6.339 -0.992)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "333d657d-79fe-4574-b8c2-d0a4a7214d3c")
		)
		(fp_line
			(start 1.388 -1.654)
			(end 1.281 -1.547)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9948ae7d-26f9-496a-927f-151a866e0190")
		)
		(fp_line
			(start 6.468 -1.654)
			(end 6.088 -1.274)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e9238162-07c9-4f87-9f06-30a49a6086f7")
		)
		(fp_line
			(start -2.6 -3.9)
			(end 7.68 -3.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1e2658ad-7b14-4561-b558-2bac6783beb5")
		)
		(fp_line
			(start -2.6 -5.96)
			(end -2.6 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5672b27c-cece-4ed8-bc78-576be92a17b2")
		)
		(fp_line
			(start -2.6 -5.96)
			(end 7.68 -5.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1ee8d360-51f1-4a05-9506-ae0da6a68260")
		)
		(fp_line
			(start 7.68 -5.96)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d4875acc-db54-4d52-b2b0-95e2427c32d4")
		)
		(fp_circle
			(center 0 0)
			(end 2.18 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "23f68f69-64e8-4253-9165-e4d2b988ec69")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.26 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "8e46f511-2d2c-49ad-8a8e-e21faed3dbc3")
		)
		(fp_line
			(start -3.04 5.8)
			(end 8.13 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "deead7a8-f651-4907-9779-54bb9b017bb7")
		)
		(fp_line
			(start 8.13 5.8)
			(end 8.13 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "aea2e6f6-6a24-464e-82f7-3a0adb5ed88f")
		)
		(fp_line
			(start -3.04 -6.4)
			(end -3.04 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "51712bc8-4921-48fa-b984-3b3307510ffb")
		)
		(fp_line
			(start 8.13 -6.4)
			(end -3.04 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0e75ebeb-d8ad-40ab-a376-0e20f9e0b18c")
		)
		(fp_line
			(start -2.04 5.3)
			(end -2.54 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "46bc8c95-36bb-4b73-b835-6ab20e442ff6")
		)
		(fp_line
			(start 7.62 5.3)
			(end -2.04 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f1e2f984-ae3e-4853-a017-e5fbb1ebba70")
		)
		(fp_line
			(start -2.54 4.8)
			(end 7.62 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "856a7f42-cc9d-478a-b7af-a2be0c23c006")
		)
		(fp_line
			(start -2.54 4.8)
			(end -2.54 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "25e12de3-71f1-42a1-be9e-f9dea6f0a035")
		)
		(fp_line
			(start -2.54 2.3)
			(end 7.62 2.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3776d8d9-2571-4f6b-b859-15a540006790")
		)
		(fp_line
			(start 1.517 -1.273)
			(end -1.273 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9aba082e-885b-4444-9483-763aedecc718")
		)
		(fp_line
			(start 6.597 -1.273)
			(end 3.808 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c92ac535-d959-4240-a841-2fb519c6e626")
		)
		(fp_line
			(start 1.273 -1.517)
			(end -1.517 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ae104d1e-b784-45ba-af66-e6a4ecd57fd4")
		)
		(fp_line
			(start 6.353 -1.517)
			(end 3.564 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cbe3c15e-125a-4d16-8677-7787f29d0cd7")
		)
		(fp_line
			(start -2.54 -3.9)
			(end 7.62 -3.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "916587fa-0ac0-462f-b3c6-1ed5edeb4586")
		)
		(fp_line
			(start -2.54 -5.9)
			(end 7.62 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6c280655-1bfc-4c82-b1ba-4cde710db236")
		)
		(fp_line
			(start 7.62 -5.9)
			(end 7.62 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "64cb43f9-c8df-4777-a601-5d799450fea4")
		)
		(fp_circle
			(center 0 0)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "0498cef5-8514-488d-a5d8-240daa3811cd")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.08 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "52b3e976-7a39-4ec5-964f-fd899bcefd7b")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 3.1 90)
			(layer "F.Fab")
			(uuid "9a74edb6-2ff1-42e6-ac81-efa8d68783d6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 231 "Net-(J19-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "e2b72e52-c602-405b-b359-74ca8f5a722f")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 230 "Net-(J19-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "48e2413f-04e4-493c-9e00-9c8bddecb5e5")
		)
		(model "${KICAD8_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "d699a45c-2fb0-4e5b-bf1d-a8ed04c4e1fa")
		(at 48.394645 55.08)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "a50d2ffd-7af5-46af-a152-9819eb3c4189")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at 0 1.82 0)
			(layer "F.Fab")
			(uuid "c8b39ef8-bc55-4f9b-86f3-829420891322")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "83f41170-e256-4319-b3cd-93cd71b5aa77")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "581d8cb0-7b85-48e1-a5ab-733cc69f216e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a46ee560-6ec0-4f9e-8ccb-143a4b1938d7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/fef2553d-539f-40e4-b7bd-376e44ab9a6f/de24ad75-a874-4d54-a682-b1d6f2079d30")
		(sheetname "Triac Circuit2")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4bab77fe-29b3-45fa-bcdc-c7ebb327b984")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7151842f-9600-4600-b9e9-7b1677ca25ba")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d2983f52-d421-4d6d-bc29-2fa3f1469e63")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d555f850-3cdd-495a-a347-bd676b69aba1")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "21e68989-c4f9-44ac-bcd9-0923202f944b")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d56065c2-1c1d-4a45-98df-6e075d49cb32")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0672b054-e8a6-45be-b5a1-aa03d7a86bf3")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "925ba804-23bf-44de-8e0f-a8c74776aa67")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6704c99b-2316-45fd-b5be-61557a34d710")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "633cbcbf-8ba6-4d9a-a3ec-426f35407fa8")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "108f7c64-aac8-4e8e-8f9a-79e4e497cd2c")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 111 "Net-(R8-Pad1)")
			(pintype "passive")
			(uuid "2b91012a-1ee4-4af4-934d-d7fc70e30596")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 37 "+3V3")
			(pintype "passive")
			(uuid "b34c8b5c-b56d-49d3-8030-b24e7f78be86")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(uuid "d7678225-9962-4b6c-8ac6-79810f77c6a5")
		(at 32.883571 81.42 -90)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "Q9"
			(at 6.04 -2.445 90)
			(layer "F.SilkS")
			(uuid "a03a87c5-fae6-4a2e-b61b-688f41adf684")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BTA16-600B"
			(at 2.54 2.5 90)
			(layer "F.Fab")
			(uuid "b33f0753-6c98-4df9-a860-9fccd75ff0b2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "6b174e8a-79b0-4f8d-b1e1-1dca6c58c4c5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "e905b471-e0ea-4d07-afe2-086bd0570bc7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "1415b729-39b4-4a22-97e7-a39031d78d34")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO?220*")
		(path "/e56f6699-6dcd-4f6f-a67f-2156f450d5f1/d1257be0-2394-4f08-8984-f580162b15f9")
		(sheetname "Triac Circuit4")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.58 1.371)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dfecbd48-3232-4a4b-8481-100ace7794ea")
		)
		(fp_line
			(start -2.58 -1.76)
			(end 7.66 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "74abc338-f05b-4c27-b650-0fed270237b4")
		)
		(fp_line
			(start -2.58 -3.27)
			(end -2.58 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "67512dc1-28b1-4683-9ac9-6a859ba5605d")
		)
		(fp_line
			(start -2.58 -3.27)
			(end 7.66 -3.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1c43e95b-9fdb-48b4-8a86-2a3e552c7501")
		)
		(fp_line
			(start 0.69 -3.27)
			(end 0.69 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e1a5f853-83e8-4d06-af8f-5056f77ba735")
		)
		(fp_line
			(start 4.391 -3.27)
			(end 4.391 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c5ab5abd-c9e2-48ee-ab55-02cb543a6fff")
		)
		(fp_line
			(start 7.66 -3.27)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4d9690db-d2c6-4271-8f1b-7bc3edfc5568")
		)
		(fp_line
			(start -2.71 1.51)
			(end 7.79 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7ed5117f-ff41-483a-8df4-a4fff30fd6bd")
		)
		(fp_line
			(start 7.79 1.51)
			(end 7.79 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5f798f68-b385-4b23-ab4d-55d338f2a108")
		)
		(fp_line
			(start -2.71 -3.4)
			(end -2.71 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8ed52c73-2e1d-492c-a561-2dc72698f2b8")
		)
		(fp_line
			(start 7.79 -3.4)
			(end -2.71 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "70c54293-5231-42a0-b982-14bd83124b22")
		)
		(fp_line
			(start -2.46 1.25)
			(end 7.54 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aae07686-d1a5-46bc-a32a-e38717bfa8fa")
		)
		(fp_line
			(start 7.54 1.25)
			(end 7.54 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "14836f66-4dce-4087-9165-b6d3fea420b6")
		)
		(fp_line
			(start -2.46 -1.88)
			(end 7.54 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f6d88642-32d3-4652-8a0e-357c672d6a20")
		)
		(fp_line
			(start -2.46 -3.15)
			(end -2.46 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "53a9850e-3e5a-4215-8b33-84218f6ac3cf")
		)
		(fp_line
			(start 0.69 -3.15)
			(end 0.69 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0fca4594-aee9-4958-8d91-720e734db9ee")
		)
		(fp_line
			(start 4.39 -3.15)
			(end 4.39 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "af1e1b20-7031-4c1d-8a52-a96690884109")
		)
		(fp_line
			(start 7.54 -3.15)
			(end -2.46 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f77f7d0b-2d39-489b-a818-beb4ff8ae413")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 -4.27 90)
			(layer "F.Fab")
			(uuid "18f74a08-4a03-4166-921c-cac27fed1c2c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "/Triac Circuit4/High_Voltage_L")
			(pinfunction "A1")
			(pintype "passive")
			(uuid "8c8d1693-517d-4cdf-8bcb-0efcb292f4f4")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/Triac Circuit4/High_Voltage_Out")
			(pinfunction "A2")
			(pintype "passive")
			(uuid "b1a4bd22-d686-41cb-bedc-c17ee16cdad2")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(Q9-G)")
			(pinfunction "G")
			(pintype "input")
			(uuid "968a1b9f-c1ee-414d-bb9c-e362827fe5cd")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
		(layer "F.Cu")
		(uuid "d7f4957b-3cf9-4d0e-abb1-240d1bcf48c6")
		(at 25.8 151.48 -90)
		(descr "Terminal Block Phoenix MKDS-3-2-5.08, 2 pins, pitch 5.08mm, size 10.2x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-3-2-5.08 pitch 5.08mm size 10.2x11.2mm^2 drill 1.3mm pad 2.6mm")
		(property "Reference" "J18"
			(at 2.54 -6.96 90)
			(layer "F.SilkS")
			(uuid "b1ff69d9-3fa9-45fe-983b-4f1a8b6ccab8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 2.54 6.36 90)
			(layer "F.Fab")
			(uuid "1a5265eb-9820-4774-b028-d9bf1ee4a291")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "02a8c725-cde4-43cd-ac80-54354140c0d9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "642c82a3-644c-4587-bfb2-a870692110e0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "907e4d8a-3710-482c-9f0d-f9c84ad2961d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/e9267efd-e7bf-4ed4-9938-23d638b0f804/8337496e-1761-4ed3-ac07-07d584382a3f")
		(sheetname "ZeroCrossDetection1")
		(sheetfile "ZeroCrossDetection.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.84 5.6)
			(end -2.34 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "36bf1a48-2155-4af6-ac3e-88542152349d")
		)
		(fp_line
			(start -2.6 5.36)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "78eadf93-1e7b-4968-8d41-d2ca0a4c56f2")
		)
		(fp_line
			(start -2.84 4.86)
			(end -2.84 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e0b3e11d-8089-4e81-9494-46a7f695b94e")
		)
		(fp_line
			(start -2.6 4.8)
			(end 7.68 4.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "122da52a-a361-4711-ab8c-279e552f3787")
		)
		(fp_line
			(start -2.6 2.3)
			(end 7.68 2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cc088b30-5864-47bb-ba2e-b300a18f4763")
		)
		(fp_line
			(start -1.282 1.547)
			(end -1.388 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f0c8ed60-0c2d-41a3-9626-023d76dbc245")
		)
		(fp_line
			(start -1.548 1.281)
			(end -1.654 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "16c7518a-d503-4218-a59d-8847145cd3e9")
		)
		(fp_line
			(start 4.073 1.274)
			(end 3.693 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8481263c-8781-4b96-90fc-801258a73ac7")
		)
		(fp_line
			(start 3.822 0.992)
			(end 3.427 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1891c01d-8e41-4537-9fa3-3931741b97e0")
		)
		(fp_line
			(start 1.654 -1.388)
			(end 1.547 -1.281)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ac93b880-b81d-4b6b-8eba-ee58a3896ec2")
		)
		(fp_line
			(start 6.734 -1.388)
			(end 6.339 -0.992)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a91c2a28-cb85-458e-9360-998151e9b90f")
		)
		(fp_line
			(start 1.388 -1.654)
			(end 1.281 -1.547)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d2b48bb5-2a52-498e-814b-d70a6072f186")
		)
		(fp_line
			(start 6.468 -1.654)
			(end 6.088 -1.274)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f45321ed-f875-4ea9-820f-9dd3344ab115")
		)
		(fp_line
			(start -2.6 -3.9)
			(end 7.68 -3.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9e16ed31-9543-4ee9-a514-e37f1f364664")
		)
		(fp_line
			(start -2.6 -5.96)
			(end -2.6 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fb2b52e8-3057-4b48-b192-283159ab9efa")
		)
		(fp_line
			(start -2.6 -5.96)
			(end 7.68 -5.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "60d02f02-9bd5-473e-9b6b-1cb53ecc7a55")
		)
		(fp_line
			(start 7.68 -5.96)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0a492d62-fdfc-4b12-82f9-0dc3be576d80")
		)
		(fp_circle
			(center 0 0)
			(end 2.18 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "a1f4eee4-dd2b-4a1a-984c-a37a9187ab17")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.26 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "5e5909cf-70c9-4e21-a5be-ecb47c5bd58f")
		)
		(fp_line
			(start -3.04 5.8)
			(end 8.13 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6048b20b-d2a1-4f55-8b00-6772ecffa706")
		)
		(fp_line
			(start 8.13 5.8)
			(end 8.13 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8ac8f9d8-71b3-4b85-8ba4-64fa7b7f1ad8")
		)
		(fp_line
			(start -3.04 -6.4)
			(end -3.04 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8563a68a-6826-4d77-b80d-fdafc7a4a0d8")
		)
		(fp_line
			(start 8.13 -6.4)
			(end -3.04 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ee67caee-a6b0-4405-80ae-29671e015861")
		)
		(fp_line
			(start -2.04 5.3)
			(end -2.54 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "85ef9310-f260-409a-a943-0eb6eaa121ba")
		)
		(fp_line
			(start 7.62 5.3)
			(end -2.04 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cf60bac8-6c46-4712-8ad7-c75909654233")
		)
		(fp_line
			(start -2.54 4.8)
			(end 7.62 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ad8ce5d1-d222-412a-8581-b5fa9169d04a")
		)
		(fp_line
			(start -2.54 4.8)
			(end -2.54 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e0424187-f159-4dd7-b1c7-79956a296c4a")
		)
		(fp_line
			(start -2.54 2.3)
			(end 7.62 2.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7cfcc68f-8eba-45ec-a4e9-a5204ede7c4e")
		)
		(fp_line
			(start 1.517 -1.273)
			(end -1.273 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c1e81180-98c0-416e-8cfb-d14aa250652d")
		)
		(fp_line
			(start 6.597 -1.273)
			(end 3.808 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dd252515-161c-4f24-9aa2-7a9e3cc98da8")
		)
		(fp_line
			(start 1.273 -1.517)
			(end -1.517 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0754b5ab-f7f7-4598-b818-ce9bc41f99fa")
		)
		(fp_line
			(start 6.353 -1.517)
			(end 3.564 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7eb16a4f-2339-43bf-a095-e5449b4f4117")
		)
		(fp_line
			(start -2.54 -3.9)
			(end 7.62 -3.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f8fb7f82-38c4-479f-a355-4fa19a4dea43")
		)
		(fp_line
			(start -2.54 -5.9)
			(end 7.62 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d59e9c3b-827b-4905-a3fa-4bcd9a97c3ef")
		)
		(fp_line
			(start 7.62 -5.9)
			(end 7.62 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eadbb438-3979-4fd4-9534-f723ad512c97")
		)
		(fp_circle
			(center 0 0)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "174d726e-d579-417f-91f4-0c079a627dca")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.08 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "e9c0ebde-f012-444e-b63f-069ac66d546d")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 3.1 90)
			(layer "F.Fab")
			(uuid "7de7462c-0d80-4199-a1cc-95658ce00612")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 228 "Net-(J18-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "32de63b8-3558-4dc7-8c0c-afd4036ac82f")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 229 "Net-(J18-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "fe21e252-faca-4c25-b7ff-b28c06496d3d")
		)
		(model "${KICAD8_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(uuid "d7f66e4e-92f9-4fe8-bfaf-1a1aeb699183")
		(at 66.942855 116.9 -90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R43"
			(at 3.809999 -1.92 -90)
			(layer "F.SilkS")
			(uuid "2bd09dcd-9918-4994-81aa-7e689fa81914")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "180"
			(at 3.81 1.919999 -90)
			(layer "F.Fab")
			(uuid "703f6d65-525c-4a34-b425-387a9beddfd7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "c664e6e3-e852-4fff-8422-051ffe498e82")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b57ad8b1-ccd2-401f-a85d-f19b8448646e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bdf1e74a-509c-4360-8fe6-8bb0b92fa51f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/683a6cfc-1cb6-4c63-ae1f-c9d1fdc220d0/4ab64e29-964f-40b2-bf58-c546b31cd3eb")
		(sheetname "Triac Circuit14")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.89 0.92)
			(end 5.73 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7b2b51b4-be55-4610-8659-8198e775b19c")
		)
		(fp_line
			(start 5.73 0.92)
			(end 5.73 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ff0e25ea-945a-4e0b-b760-fd75bc9682ea")
		)
		(fp_line
			(start 0.94 0)
			(end 1.89 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a05bd2b3-18d2-4d5d-befb-8c5581473312")
		)
		(fp_line
			(start 6.68 0)
			(end 5.73 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "caa30575-484a-4eda-a6c5-ae4e6a8a32a9")
		)
		(fp_line
			(start 1.89 -0.92)
			(end 1.89 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9dc70be4-8e6e-4d61-b7f8-ab319f9339e6")
		)
		(fp_line
			(start 5.73 -0.92)
			(end 1.89 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d15f6b84-08ea-4ef3-a9dc-91ed2a285622")
		)
		(fp_line
			(start -0.95 1.05)
			(end 8.57 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "05e158b5-6a26-444b-b49e-ee6acff9302a")
		)
		(fp_line
			(start 8.57 1.05)
			(end 8.57 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "591c64b7-098e-4f3d-a8a1-54ed6ee1861f")
		)
		(fp_line
			(start -0.95 -1.05)
			(end -0.95 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e996654e-93e1-4677-9d71-cd05f5c45ad7")
		)
		(fp_line
			(start 8.57 -1.05)
			(end -0.95 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "587ce3b2-4880-415d-b1e0-c34fc4360261")
		)
		(fp_line
			(start 2.01 0.8)
			(end 5.61 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ca0f82fa-bc42-4e1d-b66f-dbf833195d5b")
		)
		(fp_line
			(start 5.61 0.8)
			(end 5.61 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "632f49fb-d87b-4417-ad94-e3623430779f")
		)
		(fp_line
			(start 0 0)
			(end 2.01 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4d4ede1c-2a8c-44c3-a19f-6d2075274b3c")
		)
		(fp_line
			(start 7.62 0)
			(end 5.61 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0810718f-7c90-49fd-a572-f8c11643ea88")
		)
		(fp_line
			(start 2.01 -0.8)
			(end 2.01 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a8705d22-0346-4e00-bd33-6e18594bc102")
		)
		(fp_line
			(start 5.61 -0.8)
			(end 2.01 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "82f0716f-622c-49d0-89de-f3f6b94566fd")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 -90)
			(layer "F.Fab")
			(uuid "abb770ca-5f48-4a3b-8df3-9280513131ee")
			(effects
				(font
					(size 0.72 0.72)
					(thickness 0.108)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "Net-(R43-Pad1)")
			(pintype "passive")
			(uuid "20851cd9-4cac-49de-b88a-94e68b335445")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 86 "/Triac Circuit14/High_Voltage_L")
			(pintype "passive")
			(uuid "4204965c-1ff8-4248-bc87-7f55fc53dffc")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(uuid "d857daf2-c3f0-459a-a6d6-cbdff2b677ec")
		(at 54.35 163.74)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(uuid "e3634470-6335-4ff3-8974-f25835bf07f8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "22p"
			(at 0 1.85 0)
			(layer "F.Fab")
			(uuid "29a18e2b-1e7f-4282-b483-516d447fb691")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "31e33401-1b83-4efa-ad2c-287e7c33ef8f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6bb2a3fb-c846-4c0b-b6ed-f1cd997094e4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f5b4ad78-195c-4c30-9f70-acb4fafe9132")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/0d57006e-540d-4b18-8bb4-b2565af9f056")
		(sheetname "Główny")
		(sheetfile "16_ChannelPowerControlBoard.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.711252 -0.91)
			(end 0.711252 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "788eef49-5814-4f76-878c-80cd3e28d46e")
		)
		(fp_line
			(start -0.711252 0.91)
			(end 0.711252 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6d9ca1b6-7c47-4cad-8ff4-1076c1d01d59")
		)
		(fp_line
			(start -2.3 -1.15)
			(end 2.3 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f412a551-4288-4b03-906a-1fd932cd17d5")
		)
		(fp_line
			(start -2.3 1.15)
			(end -2.3 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3dca4ce2-35d7-4d3b-a93e-a73d0392403d")
		)
		(fp_line
			(start 2.3 -1.15)
			(end 2.3 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5d44d7fe-0c22-421e-a3b7-2f9d3e8b26ba")
		)
		(fp_line
			(start 2.3 1.15)
			(end -2.3 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b2184961-46ef-4587-8497-2e63acf397ab")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "85af151a-8b9e-4ae1-9de3-6989263cffda")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4499fd14-817d-4a2f-9f97-98d605109d80")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0d909452-abf3-4d3f-bba7-377cb92ea281")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "141a14ec-fb65-46d4-be8e-ad3c42e61a16")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "dfe2332f-8ee2-4051-84b3-4d211a15e8e9")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 165 "Net-(U19-OSC2)")
			(pintype "passive")
			(uuid "5579f009-c800-47b1-9d00-c6fb10f0eb95")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 41 "GND")
			(pintype "passive")
			(uuid "c47a8de9-b531-4756-bfb9-5e5fdb59e867")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "df485b94-0569-4ae2-9b1f-7e08d191584c")
		(at 53.542855 28.4 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R27"
			(at 0 -1.82 180)
			(layer "F.SilkS")
			(uuid "888ff86d-eeb6-42bb-a8b9-8bba5d300088")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at -3.64 0 180)
			(layer "F.Fab")
			(uuid "d54c0731-b8c4-4021-8804-6c3c01de8f2f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "38074117-d68b-441c-b314-32c24121fb83")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "6b1e2ef8-d32a-44cd-b936-98a6a5003cc9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "291ebf39-0b3f-4de6-9f3d-948f6b7bb4c8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/a837c47c-5707-46fe-8eca-0b07e116b13e/ca31a324-056f-45d6-b948-82e97db62734")
		(sheetname "Triac Circuit8")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d67c72c0-c93b-4cc5-b15d-acaf44e08394")
		)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aa771205-6292-4441-84a3-ac3c95aaf4e1")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "76011d54-0bab-4ab5-b2f3-dd59c9efa598")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8f40cd30-616e-41e2-bee9-266c3138b0af")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8eb9444f-6643-489b-8c83-9ba20cc4fb10")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c3a18306-5bae-458e-939c-7063afc78e86")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "776a4655-1925-4e3a-ae94-97f74e898314")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "52b8a34d-faa1-4525-80a1-ec50299c2f1b")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3f3ddb2b-f15c-4cf9-a6b6-e71a653bfedb")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "862d2709-fd43-46fd-ad9e-c1425f03ecae")
		)
		(fp_text user "${REFERENCE}"
			(at 3.04 0.01 180)
			(layer "F.Fab")
			(uuid "0c71b5d8-a695-40fb-820d-59a5cec04f71")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 129 "Net-(Q18-B)")
			(pintype "passive")
			(uuid "2a27ce45-9d61-48fd-991f-04c116cd65f4")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 131 "/Triac Circuit8/Enable")
			(pintype "passive")
			(uuid "ebef5fc7-1829-43ef-a0a9-1cafd4377214")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_5x5.4"
		(layer "F.Cu")
		(uuid "df5bfe44-b514-47d3-bd0c-30b9c8932919")
		(at 61.4 180.2)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 5.0x5.4mm")
		(tags "capacitor electrolyic nonpolar")
		(property "Reference" "C1"
			(at 0 -3.7 0)
			(layer "F.SilkS")
			(uuid "7c3c1be5-b4f6-4e2d-afce-b00437412a27")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4u7"
			(at 0 3.7 0)
			(layer "F.Fab")
			(uuid "07d2a06b-6ed3-4256-90d2-f1198cfc254d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_Elec_5x5.4"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d6339c1e-b024-4cb1-8860-4a7c955ae61d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8c1bf14e-141d-4246-96eb-c3efbf04d7f1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bb98f3a2-d0e0-4e46-b80c-511b53f22668")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/a12f1fa5-fd32-4068-a9c6-9b0e33387c3f")
		(sheetname "Główny")
		(sheetfile "16_ChannelPowerControlBoard.kicad_sch")
		(attr smd)
		(fp_line
			(start -2.76 -1.695563)
			(end -2.76 -1.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0b19afd5-2908-4ea3-8f4d-bf37163f9ef0")
		)
		(fp_line
			(start -2.76 -1.695563)
			(end -1.695563 -2.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1b94780d-a2a1-47f3-a8d3-efa75f8b7035")
		)
		(fp_line
			(start -2.76 1.695563)
			(end -2.76 1.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "346d7c27-10e3-4a6e-9674-efe8d91c3992")
		)
		(fp_line
			(start -2.76 1.695563)
			(end -1.695563 2.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f004b871-ef0c-41e4-8644-7a82212e6da9")
		)
		(fp_line
			(start -1.695563 -2.76)
			(end 2.76 -2.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "47c666c6-c08d-4b5a-af31-fdd29dbbae15")
		)
		(fp_line
			(start -1.695563 2.76)
			(end 2.76 2.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "66a0f651-8bfc-445f-bf50-552f95566313")
		)
		(fp_line
			(start 2.76 -2.76)
			(end 2.76 -1.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c152acb6-0053-419d-99a8-ea8537e6f785")
		)
		(fp_line
			(start 2.76 2.76)
			(end 2.76 1.06)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a62a1151-c569-4760-9199-eec97bd09d35")
		)
		(fp_line
			(start -3.7 -1.05)
			(end -3.7 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1664b045-6db2-4d17-b91d-6ba109d7635d")
		)
		(fp_line
			(start -3.7 1.05)
			(end -2.9 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3b20e43d-7b28-41e2-9a28-051caaa974fc")
		)
		(fp_line
			(start -2.9 -1.75)
			(end -2.9 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5962327b-66cf-4fc0-98bc-a59c299a4366")
		)
		(fp_line
			(start -2.9 -1.75)
			(end -1.75 -2.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "620b2f54-ac28-4a64-b270-02238de63971")
		)
		(fp_line
			(start -2.9 -1.05)
			(end -3.7 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6cd48c2a-2dfa-4c85-ba13-c0ef083e202b")
		)
		(fp_line
			(start -2.9 1.05)
			(end -2.9 1.75)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e2f1f0ae-bb56-4cb2-897c-c709f313bc84")
		)
		(fp_line
			(start -2.9 1.75)
			(end -1.75 2.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0cf2d469-f906-4454-80ee-c4bb8d2a5dea")
		)
		(fp_line
			(start -1.75 -2.9)
			(end 2.9 -2.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "07747cdb-0f99-4d0b-884d-4b84a4f7ecd1")
		)
		(fp_line
			(start -1.75 2.9)
			(end 2.9 2.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0be74501-42ed-43ef-8790-ab78152b5e1d")
		)
		(fp_line
			(start 2.9 -2.9)
			(end 2.9 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ab4666ef-d6bf-4c1d-b69b-8cbe7dde60f9")
		)
		(fp_line
			(start 2.9 -1.05)
			(end 3.7 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "93c39525-fd62-4472-a654-dca05b3f3177")
		)
		(fp_line
			(start 2.9 1.05)
			(end 2.9 2.9)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f0584e60-7af5-4024-a87d-89424b8040e0")
		)
		(fp_line
			(start 3.7 -1.05)
			(end 3.7 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1c97147d-a924-4da2-ba4d-494e3ab9e633")
		)
		(fp_line
			(start 3.7 1.05)
			(end 2.9 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f889e930-4c09-4a79-b803-bed5dbfe36bf")
		)
		(fp_line
			(start -2.65 -1.65)
			(end -2.65 1.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b20bef1a-7e5b-46e3-980a-d11d2a61dd7f")
		)
		(fp_line
			(start -2.65 -1.65)
			(end -1.65 -2.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c094777d-b421-4ef5-9e35-ef283e0c15e4")
		)
		(fp_line
			(start -2.65 1.65)
			(end -1.65 2.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d2f88ea7-4f9d-4edd-8668-1f68015e33ed")
		)
		(fp_line
			(start -1.65 -2.65)
			(end 2.65 -2.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8d865ab1-aff0-480a-813c-4e842efa9e5e")
		)
		(fp_line
			(start -1.65 2.65)
			(end 2.65 2.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8f269fab-5b9d-4a29-ac26-66eee3ba3f08")
		)
		(fp_line
			(start 2.65 -2.65)
			(end 2.65 2.65)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "96de1376-7c58-4fb8-90b1-b97dc568e45f")
		)
		(fp_circle
			(center 0 0)
			(end 2.5 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "862bbe45-57a6-43eb-8d41-ac9ea18188c9")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "21f0f128-e221-435d-b0a3-e30b4602d5f1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -2.0625 0)
			(size 2.775 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.15625)
			(net 164 "Net-(C1-Pad1)")
			(pintype "passive")
			(uuid "bec225f9-b64f-4e13-8ac8-bb0aad967e3f")
		)
		(pad "2" smd roundrect
			(at 2.0625 0)
			(size 2.775 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.15625)
			(net 41 "GND")
			(pintype "passive")
			(uuid "d3615c92-4359-4ed6-97e2-0d906a6b7eca")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_5x5.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-6_W7.62mm"
		(layer "F.Cu")
		(uuid "e09109ab-9f47-498b-bd26-c793d4c66845")
		(at 57.142855 102.675)
		(descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U15"
			(at 3.599999 -2.33 180)
			(layer "F.SilkS")
			(uuid "11e6b770-37dc-4f1b-a5c5-37ec1a98e69b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MOC3021M"
			(at 3.81 7.409999 180)
			(layer "F.Fab")
			(uuid "e3b89e67-0b1e-455c-a98d-082b72b5a1ed")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d3036363-4e7e-4179-aa65-91ad4c13e71d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3023M-D.PDF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "28b2104d-3e9e-4407-9ec6-e18b16a19e06")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "adcdf48a-5b3b-41d9-a0a9-256954c883f6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*")
		(path "/4a948621-4b4c-41c9-b07f-b928eecc9e1e/0262e914-5435-478f-be04-ece49b8102cf")
		(sheetname "Triac Circuit13")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "49bb2501-7fe9-4342-b1c6-f5068b79a330")
		)
		(fp_line
			(start 1.16 6.41)
			(end 6.46 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c3a8aaec-fbd1-4b9b-8822-88c11c8e7dea")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5e40763f-7306-4959-8138-88717bfb384f")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b555e6de-029f-4d46-bc22-c3faf02e3900")
		)
		(fp_line
			(start 6.46 6.41)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9448e99a-1856-4ea4-9170-3c75b8dc5736")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3746a0e7-f211-4e5e-a656-1a0493a185c9")
		)
		(fp_line
			(start -1.1 -1.55)
			(end -1.1 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3cc6f04e-4b6c-4a5a-88ad-37588b7de3dc")
		)
		(fp_line
			(start -1.1 6.6)
			(end 8.7 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e285c10f-6b97-4698-9419-73267f3ae838")
		)
		(fp_line
			(start 8.7 -1.55)
			(end -1.1 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f6793a68-782a-4c1d-926c-8c6b548f1899")
		)
		(fp_line
			(start 8.7 6.6)
			(end 8.7 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "88375d7b-4e28-46be-ac66-346dd7457762")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ce6390b4-2c35-46ec-a9c6-af5d1352cf27")
		)
		(fp_line
			(start 0.635 6.35)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fcd1e5c7-c2ab-4707-b887-0a4b46b05d82")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3327a4e5-7e85-4ca0-b67f-738d88cb67cb")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8eca91fb-fe46-4b8c-82df-c841c8365958")
		)
		(fp_line
			(start 6.985 6.35)
			(end 0.635 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "66e4a897-2c0d-4147-bbe0-4d7bd8855bff")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.539999 180)
			(layer "F.Fab")
			(uuid "c6ca94ce-64a2-4c48-8177-137ac9aa566b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 122 "Net-(R41-Pad1)")
			(pintype "passive")
			(uuid "073c1d8b-131f-48fb-9183-7424ec64319f")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 153 "Net-(Q28-C)")
			(pintype "passive")
			(uuid "992e47b6-e00e-47c4-b325-8966479d5e11")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 105 "unconnected-(U15-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "d0e9bf00-2efc-44b6-b347-7da143a90cf1")
		)
		(pad "4" thru_hole oval
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 151 "Net-(Q27-G)")
			(pintype "passive")
			(uuid "42ee0e59-705a-412a-99a8-af005acff488")
		)
		(pad "5" thru_hole oval
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 106 "unconnected-(U15-NC-Pad5)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "80c0611d-7092-4315-8a56-3a975f2240f5")
		)
		(pad "6" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(R40-Pad1)")
			(pintype "passive")
			(uuid "2139ef9a-86e9-4cc4-abe9-1b1233e75dfb")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-6_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "e0a77db5-7a7e-4b20-8549-10e7153d60c5")
		(at 54.005355 46.439999)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q20"
			(at 0 -2.4 180)
			(layer "F.SilkS")
			(uuid "23a0ff8b-ca73-4427-aa04-35c1a127b904")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BC818"
			(at 0 2.4 180)
			(layer "F.Fab")
			(uuid "ffe1b28e-00e4-4ddd-85dd-3e6ea1968ba2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0a46c927-dac1-4348-ac7f-fa19a59ac9a9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC818-D.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "190b164a-02a2-49a2-a686-f1f1ba828198")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "12572580-769f-467d-98c2-4fb28a825b92")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/f251f0b5-0f8b-4418-bbfe-69d55a4bdeb8/00e550ea-8431-483d-ac3c-b4a719825546")
		(sheetname "Triac Circuit9")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -1.56)
			(end -1.675 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "94319a88-923a-4d99-8b57-154de394f643")
		)
		(fp_line
			(start 0 -1.56)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0890ea5d-e901-497f-86ad-7af6591e80c3")
		)
		(fp_line
			(start 0 1.56)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "310f846e-d8b6-4866-8152-00e853ccc0b4")
		)
		(fp_line
			(start 0 1.56)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "70c5ad50-5bde-4cef-80bf-67024933e482")
		)
		(fp_line
			(start -1.92 -1.7)
			(end -1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2d875921-5143-4b21-8ac1-00238c1259a8")
		)
		(fp_line
			(start -1.92 1.7)
			(end 1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "72ca40b0-e75e-4020-92ee-685594688209")
		)
		(fp_line
			(start 1.92 -1.7)
			(end -1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7b7bc3da-f368-4faa-827c-f8887cc65ac2")
		)
		(fp_line
			(start 1.92 1.7)
			(end 1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ae2eee9b-1f63-4930-b9bb-41e292414933")
		)
		(fp_line
			(start -0.65 -1.125)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9e8c6cea-5264-4ff4-ba57-63529f97cbda")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "67047aad-0cc3-42a2-885c-48fe7d22a1e9")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f6d41dfb-9758-4830-90ba-ce03bb3f6b38")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7d24197a-3ce7-4a7a-80a1-3f11f1a6dbe4")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "413f7b38-3d48-449a-8df4-e1210845af11")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
			(uuid "e87c71dd-946f-48b3-98b8-726a9c60e561")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 140 "Net-(Q20-B)")
			(pinfunction "B")
			(pintype "input")
			(uuid "0fcf4e4c-96bc-4b6f-9f9d-50d1738f2ccf")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "GND")
			(pinfunction "E")
			(pintype "passive")
			(uuid "58bc27be-4c8a-4def-a2b6-c788c1ff828d")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 141 "Net-(Q20-C)")
			(pinfunction "C")
			(pintype "passive")
			(uuid "1da39f7e-54da-4b8f-bd83-c7a4a0a0068d")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "e0a8b868-04f9-41a2-87df-b67f5cabb2a9")
		(at 54.005355 31.199999)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q18"
			(at 0 -2.4 180)
			(layer "F.SilkS")
			(uuid "8bcaf0a1-cda1-4948-9c92-3762191431f9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BC818"
			(at 0 2.4 180)
			(layer "F.Fab")
			(uuid "3c7f528d-2bb5-47df-b09e-5f545f47690e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "37b7263c-c54f-43e4-a991-22bf8ea1bd6b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC818-D.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "5202117f-783b-4ccb-835a-9d6683912c16")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3f0cbe01-7ab3-4b7b-9a48-e4572ea4bfbb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/a837c47c-5707-46fe-8eca-0b07e116b13e/00e550ea-8431-483d-ac3c-b4a719825546")
		(sheetname "Triac Circuit8")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -1.56)
			(end -1.675 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ac66d511-ebde-4442-9c17-babbed2a1eee")
		)
		(fp_line
			(start 0 -1.56)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "36b1f03d-21f2-4968-b2ab-01aa1c366518")
		)
		(fp_line
			(start 0 1.56)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e7f08087-541a-482b-a373-5300769db331")
		)
		(fp_line
			(start 0 1.56)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "98ec1dbe-e0cf-4b8d-97ea-617a334a0fb0")
		)
		(fp_line
			(start -1.92 -1.7)
			(end -1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0079fbe1-9fdf-419b-b955-d19a470c72cc")
		)
		(fp_line
			(start -1.92 1.7)
			(end 1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d70d2020-b814-4b38-a1ca-02ae4567a64d")
		)
		(fp_line
			(start 1.92 -1.7)
			(end -1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7cdede7c-0458-4849-9852-ef88aac17cf8")
		)
		(fp_line
			(start 1.92 1.7)
			(end 1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "87e2b69c-52a4-474e-bc79-509a0a469f78")
		)
		(fp_line
			(start -0.65 -1.125)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a9fae80a-630b-49f7-a883-a7b6d466a75c")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "775310ce-f5eb-46d5-8f3e-aa2b2ca58bc9")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b466d49c-e05b-41f9-b52f-d81e901b45ec")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e5ca7ecd-9293-4db2-adcf-720b5cb58f9f")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e3fb19a4-9cf4-45fa-b2e1-2051a789339c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
			(uuid "7479789b-3ff3-4334-92f8-f67b8b4fe175")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 129 "Net-(Q18-B)")
			(pinfunction "B")
			(pintype "input")
			(uuid "548a622d-c9ac-47b8-9270-8510b2c0c556")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "GND")
			(pinfunction "E")
			(pintype "passive")
			(uuid "e627479c-acf7-4f6e-b68a-b79b52d40e62")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 130 "Net-(Q18-C)")
			(pinfunction "C")
			(pintype "passive")
			(uuid "93a0bbac-f02e-4d64-861d-df8e31c1194b")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "e1528d0f-0f77-44c4-b398-b7c0c9b96ba1")
		(at 48.6 22.4)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 0 -1.82 0)
			(layer "F.SilkS")
			(uuid "3a4a57e1-b585-4938-941e-dbf75ba575c5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at -3.64 0 0)
			(layer "F.Fab")
			(uuid "fb12a6eb-e197-436e-985f-2b5a0d2b2711")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4c1c6674-d28e-4ee3-a955-f8611a309159")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "fa25b402-dd9e-482b-8a27-1440390057c2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "572f6c4a-67f4-4f4c-8713-f9ab1b21cd19")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/84e52baa-d126-4c4f-b1c5-63bb27b07c2b/ca31a324-056f-45d6-b948-82e97db62734")
		(sheetname "Triac Circuit")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dd5cdbd6-24c5-4d5f-b80c-0acd8b118746")
		)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d26f4dea-9296-4c15-8b70-9dbb87d14c0a")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6b4210fa-f56a-4846-a548-53177f968c63")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7f8d920c-fb22-451c-af13-528b17e1b3d3")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8ca966d4-c762-440a-a950-a1472c06f5d9")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9b68291b-e950-44a4-b88f-08b7ab23909d")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "edbf6a98-4343-4cbf-907c-65ad17bc4805")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "53657ecb-eb18-424c-957c-7a8a38b84780")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8d5fad35-6dbd-450d-9dd9-c74c0d9caf4f")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "81fbc598-7e3b-4e0f-81b9-a850c73127f2")
		)
		(fp_text user "${REFERENCE}"
			(at 3.04 0.01 0)
			(layer "F.Fab")
			(uuid "2205a110-6b4b-482e-ad7f-75af88962d7c")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 40 "Net-(Q2-B)")
			(pintype "passive")
			(uuid "68fc3e81-6550-470a-a28e-402e5fd6ffa7")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 21 "/Triac Circuit/Enable")
			(pintype "passive")
			(uuid "5dcd6905-8e33-4fac-807c-f1f8a417fc2f")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-6_W7.62mm"
		(layer "F.Cu")
		(uuid "e26fcc93-f267-469e-ad2a-fa384ea75693")
		(at 45 24.325 180)
		(descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U2"
			(at 3.6 -2.33 0)
			(layer "F.SilkS")
			(uuid "e8745404-6d57-45c0-ad8e-b3d83255480b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MOC3021M"
			(at 3.81 7.41 0)
			(layer "F.Fab")
			(uuid "f9dfe2d0-4266-494c-b296-019b0dba1709")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "1e891595-cc6e-4535-a22a-036c044feb59")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3023M-D.PDF"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "20cc586d-febd-46b9-a85c-adabe8a30f79")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "d8a8bd7d-3354-46fd-89a0-8684fe9e77cf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*")
		(path "/84e52baa-d126-4c4f-b1c5-63bb27b07c2b/0262e914-5435-478f-be04-ece49b8102cf")
		(sheetname "Triac Circuit")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 6.46 6.41)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "593f0939-e434-4de7-8554-6f59c83b0bda")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d086ee3b-ae15-4821-9900-6622268ec9b4")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "004652fe-ae6a-411d-8c59-99650bab3f8a")
		)
		(fp_line
			(start 1.16 6.41)
			(end 6.46 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4f989f15-0638-4d26-bc1a-7a95007d08d9")
		)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bc38806c-db60-4664-a4fa-2364cdcdc930")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2b1009bc-6160-4b4f-a9bd-40b12ff9eae1")
		)
		(fp_line
			(start 8.7 6.6)
			(end 8.7 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c6e45e07-860a-4f35-9e38-a30611c1c788")
		)
		(fp_line
			(start 8.7 -1.55)
			(end -1.1 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bc2111b6-de99-4a5d-ab2d-2d012eeabb79")
		)
		(fp_line
			(start -1.1 6.6)
			(end 8.7 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4d85b3b7-1fca-42dd-b670-a262c85c6026")
		)
		(fp_line
			(start -1.1 -1.55)
			(end -1.1 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "133cb912-9de8-4bbe-9d16-d023db801c51")
		)
		(fp_line
			(start 6.985 6.35)
			(end 0.635 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4d788c08-ae96-4cbf-8fda-355760b5ba40")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d5744457-afaa-4d31-a254-418dff31c1a2")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c4546ef7-baa9-4097-b824-be6b9d72d3e5")
		)
		(fp_line
			(start 0.635 6.35)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7b0e4897-2ff7-452f-b121-a18a8dea7a66")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a166ebb5-6d39-4b05-9c6b-041193746756")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.54 0)
			(layer "F.Fab")
			(uuid "4fbd7ffb-18f1-4ac0-984b-43481f5211aa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 109 "Net-(R2-Pad1)")
			(pintype "passive")
			(uuid "44839f18-e28f-44cf-b7a2-c6eabb1b1e0c")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "Net-(Q2-C)")
			(pintype "passive")
			(uuid "c51edc9b-e151-4256-a05c-be2d62748b6d")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 160 "unconnected-(U2-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "72385e00-dc03-4bba-8065-a8eefd352a7b")
		)
		(pad "4" thru_hole oval
			(at 7.62 5.08 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(Q1-G)")
			(pintype "passive")
			(uuid "8e4ca4c4-c421-4fca-ae60-915b93512841")
		)
		(pad "5" thru_hole oval
			(at 7.62 2.54 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 161 "unconnected-(U2-NC-Pad5)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "aef2c305-955c-4d42-9ced-528cb3fbfeb3")
		)
		(pad "6" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(R1-Pad1)")
			(pintype "passive")
			(uuid "3c350070-dbf7-4256-9e8e-65e9e04af515")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-6_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(uuid "e2bf3c5a-b014-4f85-8305-86de33fb2476")
		(at 66.942855 25.46 -90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R25"
			(at 3.809999 -1.92 -90)
			(layer "F.SilkS")
			(uuid "18a25413-1823-4ea9-a525-e4574179d1ab")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "180"
			(at 3.81 1.919999 -90)
			(layer "F.Fab")
			(uuid "de0ec271-086e-4a19-a0ce-8499ea69e119")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "39d570c0-10fe-4d31-9905-1d9c46f29799")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "413449e7-3f23-40b6-9798-7f45bf61ce83")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ab78efbd-a0d2-4ac1-ba33-ed1413738feb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/a837c47c-5707-46fe-8eca-0b07e116b13e/4ab64e29-964f-40b2-bf58-c546b31cd3eb")
		(sheetname "Triac Circuit8")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.89 0.92)
			(end 5.73 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2c797284-a12d-4d23-94b7-ddeff3769dce")
		)
		(fp_line
			(start 5.73 0.92)
			(end 5.73 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "51593e4a-f924-4ccb-a2cf-5199a3638881")
		)
		(fp_line
			(start 0.94 0)
			(end 1.89 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "93bc05d4-ac91-4cb1-a2d0-18674434a311")
		)
		(fp_line
			(start 6.68 0)
			(end 5.73 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "377736a9-47f3-4d16-a523-b1beee5c652c")
		)
		(fp_line
			(start 1.89 -0.92)
			(end 1.89 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2b4edf0a-d66a-43c2-aac7-0c53c83bc12a")
		)
		(fp_line
			(start 5.73 -0.92)
			(end 1.89 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d8c22c71-ceb5-4242-92ad-038bc543ff8a")
		)
		(fp_line
			(start -0.95 1.05)
			(end 8.57 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9deef750-9288-4bda-9593-de3f6d8e8b15")
		)
		(fp_line
			(start 8.57 1.05)
			(end 8.57 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a92ba9c6-2231-482d-9499-05e4505f8619")
		)
		(fp_line
			(start -0.95 -1.05)
			(end -0.95 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f80893ee-0d05-4620-806d-8ffcfe36f739")
		)
		(fp_line
			(start 8.57 -1.05)
			(end -0.95 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9559f5ba-e18f-4f0d-9efd-e6975475a142")
		)
		(fp_line
			(start 2.01 0.8)
			(end 5.61 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6c4e1951-3f43-445e-817d-51b545509a43")
		)
		(fp_line
			(start 5.61 0.8)
			(end 5.61 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a0322042-1dba-4a92-a0dc-9337d9878f5b")
		)
		(fp_line
			(start 0 0)
			(end 2.01 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "768d31dd-1ea9-4847-b216-bd2ca91eb9c9")
		)
		(fp_line
			(start 7.62 0)
			(end 5.61 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a006e997-77f3-4959-8bbb-118d25a9142a")
		)
		(fp_line
			(start 2.01 -0.8)
			(end 2.01 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e8f8a816-1a1f-4592-bd03-21536a2a626e")
		)
		(fp_line
			(start 5.61 -0.8)
			(end 2.01 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1d86759c-8a5d-4d63-a51f-48cf098bed0e")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 -90)
			(layer "F.Fab")
			(uuid "72613a71-524b-45d0-96e4-d25d48999d25")
			(effects
				(font
					(size 0.72 0.72)
					(thickness 0.108)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "Net-(R25-Pad1)")
			(pintype "passive")
			(uuid "dfac00e3-d6d4-4e30-a9dd-480c59da5fdb")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "/Triac Circuit8/High_Voltage_L")
			(pintype "passive")
			(uuid "8be79102-b903-45c0-9e6e-cd45608edfe6")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "e57d657f-7386-4800-aab0-1fe88d56e29f")
		(at 48.108929 111.04 180)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q14"
			(at 0 -2.4 0)
			(layer "F.SilkS")
			(uuid "e0f3573c-e4ab-4bf7-b672-5d4597ef0cd2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BC818"
			(at 0 2.4 0)
			(layer "F.Fab")
			(uuid "b364ab24-5d54-477d-ab04-e43973f4bf7a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "1fd65d7b-7086-4f0b-a3b8-2d877d0bd4a0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC818-D.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "2f501cc4-acb1-4e5f-8221-c292f92453b8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "e2f61e7d-f713-423a-9452-af156bd1cb56")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/4a841339-199f-4bc7-a6bd-fe2a9936827c/00e550ea-8431-483d-ac3c-b4a719825546")
		(sheetname "Triac Circuit6")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 1.56)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2e6baa9d-7e64-4abb-b09d-f3d05d644f0d")
		)
		(fp_line
			(start 0 1.56)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3ae00f5a-3e6d-475a-aa42-3090ada2303b")
		)
		(fp_line
			(start 0 -1.56)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3da17cc9-2e6c-4a5c-8538-0d8b2d1302cc")
		)
		(fp_line
			(start 0 -1.56)
			(end -1.675 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fd34ca2c-fd01-4f92-9ccf-240a8596327b")
		)
		(fp_line
			(start 1.92 1.7)
			(end 1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "921c2a8d-c8bf-490b-9de5-ed0d9ba959fa")
		)
		(fp_line
			(start 1.92 -1.7)
			(end -1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d70f770b-2b7a-44a5-b60b-579dd599fdae")
		)
		(fp_line
			(start -1.92 1.7)
			(end 1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "05ebc919-e3b7-4db7-b768-106fe6e32924")
		)
		(fp_line
			(start -1.92 -1.7)
			(end -1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "02556892-8721-45dc-b3d6-eb4a8752a716")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "24957a67-f019-4086-955e-f5400c2caa41")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dc6b5f87-411f-4cbb-ae16-4b0ede2069d7")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5bedf2dd-1394-4d30-9a3f-4d06d3192766")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4262e04f-4c02-4a79-a8bd-753a44e46374")
		)
		(fp_line
			(start -0.65 -1.125)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6e7dc1bb-d8e1-4307-a0e4-b77581f8c436")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "79bea974-0d8c-456a-94ce-bf673132f6e1")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 72 "Net-(Q14-B)")
			(pinfunction "B")
			(pintype "input")
			(uuid "a37cf733-5197-4350-b6dd-fe9c01712e4f")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "GND")
			(pinfunction "E")
			(pintype "passive")
			(uuid "ef87483c-babb-4554-a4b5-f0da24ffd5b0")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 73 "Net-(Q14-C)")
			(pinfunction "C")
			(pintype "passive")
			(uuid "39c9983c-f333-4701-8efa-a80096925540")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(uuid "e8c9d580-5b02-4f91-885d-dc249dc28e51")
		(at 32.912142 96.66 -90)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "Q11"
			(at 6.04 -2.445 90)
			(layer "F.SilkS")
			(uuid "32e03c7f-606e-4712-bc85-eaeca56ab6cb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BTA16-600B"
			(at 2.54 2.5 90)
			(layer "F.Fab")
			(uuid "16452c0b-7329-4332-91dc-0f4d9afe7738")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "5c7f1f9c-d7ff-4bcf-bf65-0d0abd1f4f2a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "fa9e26f7-f8c7-46f8-b6ed-7623c46ba4f9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "0df76df1-7de2-4e8f-987c-d4a781abf97a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO?220*")
		(path "/6eb41966-4a54-4fd9-a1be-49d2f272d785/d1257be0-2394-4f08-8984-f580162b15f9")
		(sheetname "Triac Circuit5")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.58 1.371)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "30791b66-2999-4051-8f55-98ec7c7346a0")
		)
		(fp_line
			(start -2.58 -1.76)
			(end 7.66 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c5406643-5669-4522-b142-5aa56ce8b05b")
		)
		(fp_line
			(start -2.58 -3.27)
			(end -2.58 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "50e57ef0-224b-40a8-a19c-38a1970010c5")
		)
		(fp_line
			(start -2.58 -3.27)
			(end 7.66 -3.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "575d5eef-2900-4419-8457-84ed814e3a30")
		)
		(fp_line
			(start 0.69 -3.27)
			(end 0.69 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a7a019bb-0f90-44af-b158-f12190435218")
		)
		(fp_line
			(start 4.391 -3.27)
			(end 4.391 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9ae40892-9691-446d-989b-d7a405ab30a2")
		)
		(fp_line
			(start 7.66 -3.27)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "39511ec4-0db4-44b1-9541-4f42fe386f7a")
		)
		(fp_line
			(start -2.71 1.51)
			(end 7.79 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9d0a494f-0954-46a1-8f23-4695014e9931")
		)
		(fp_line
			(start 7.79 1.51)
			(end 7.79 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6eaba10c-9f8c-4544-a5fa-ff2254603db8")
		)
		(fp_line
			(start -2.71 -3.4)
			(end -2.71 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8f7bbe52-eb3f-4616-869b-f70fae63269b")
		)
		(fp_line
			(start 7.79 -3.4)
			(end -2.71 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "92f93c74-e256-4f72-a890-4064e8daade6")
		)
		(fp_line
			(start -2.46 1.25)
			(end 7.54 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "672c0675-656c-4f7a-bab0-4e1ab82301ca")
		)
		(fp_line
			(start 7.54 1.25)
			(end 7.54 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "eda6a64e-ba63-448d-a6a7-a89a1a9d5f1c")
		)
		(fp_line
			(start -2.46 -1.88)
			(end 7.54 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6346fbb0-7ab8-4a4b-8f8f-d6a804247ac3")
		)
		(fp_line
			(start -2.46 -3.15)
			(end -2.46 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ab0c5903-64c5-4f5a-be92-a600d38194cd")
		)
		(fp_line
			(start 0.69 -3.15)
			(end 0.69 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5e5bacb0-6348-45ab-a8e2-5f532855db97")
		)
		(fp_line
			(start 4.39 -3.15)
			(end 4.39 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5ec311ea-526b-4f84-9636-28f474997210")
		)
		(fp_line
			(start 7.54 -3.15)
			(end -2.46 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c7f0d3cb-bc60-4761-92c1-5a2c25db0488")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 -4.27 90)
			(layer "F.Fab")
			(uuid "bc7c7513-98d3-4276-b25f-f8d454942ca4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "/Triac Circuit5/High_Voltage_L")
			(pinfunction "A1")
			(pintype "passive")
			(uuid "893badcf-6114-4af5-bf57-152088db5ba8")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/Triac Circuit5/High_Voltage_Out")
			(pinfunction "A2")
			(pintype "passive")
			(uuid "7d173ed1-b67d-4755-8867-1cd2b99901c7")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(Q11-G)")
			(pinfunction "G")
			(pintype "input")
			(uuid "bebe059c-ddc4-40f0-bb93-36afb85d8ccc")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(uuid "e9cb025b-e8eb-497a-aeaa-2295c65ac5c0")
		(at 69.287855 76.06 90)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "Q23"
			(at 6.04 -2.444999 -90)
			(layer "F.SilkS")
			(uuid "b1b4c7dd-3c9a-4baa-9b1e-6cd650623f2f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BTA16-600B"
			(at 2.539999 2.5 -90)
			(layer "F.Fab")
			(uuid "a82b626e-4366-4502-8467-e8ebf12d1bcc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "479a465a-c3da-4cca-b622-b9ee4404fbf5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "ec670e08-9fd2-4b08-bd63-3b08990bc24b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "7920d200-2f51-47db-83fa-8b559e1d5307")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO?220*")
		(path "/15d8fe7c-2a9b-438f-a777-3e4687188af1/d1257be0-2394-4f08-8984-f580162b15f9")
		(sheetname "Triac Circuit11")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 7.66 -3.27)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "382e9a5f-99f7-4a58-b371-eac7cc8f00af")
		)
		(fp_line
			(start 4.391 -3.27)
			(end 4.391 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7c4eb56c-9fd0-4022-9f2f-6bc52d303e04")
		)
		(fp_line
			(start 0.69 -3.27)
			(end 0.69 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d096c4ce-c94b-4e0c-86fb-c5528610dcbd")
		)
		(fp_line
			(start -2.58 -3.27)
			(end 7.66 -3.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fb79bde6-cafe-451b-b521-f95e37182cb7")
		)
		(fp_line
			(start -2.58 -3.27)
			(end -2.58 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ee0cf3e9-b57f-4482-9082-7fe6c7b797ae")
		)
		(fp_line
			(start -2.58 -1.76)
			(end 7.66 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ec741cae-1c24-41cc-aa9c-167146fe6daf")
		)
		(fp_line
			(start -2.58 1.371)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5efda937-2a61-4f0c-9a43-f79cf84aa9bd")
		)
		(fp_line
			(start 7.79 -3.4)
			(end -2.71 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4c7fc861-dc2f-460e-b114-d0291d7ba85d")
		)
		(fp_line
			(start -2.71 -3.4)
			(end -2.71 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b4b01467-2a47-4ae3-9d91-0f0aad518908")
		)
		(fp_line
			(start 7.79 1.51)
			(end 7.79 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7d7c990d-3e3b-43b8-be9f-5abf00eb63f5")
		)
		(fp_line
			(start -2.71 1.51)
			(end 7.79 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "83543d61-17e4-4f62-974e-6d1446e7d418")
		)
		(fp_line
			(start 7.54 -3.15)
			(end -2.46 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b8d9e9dd-fe0d-45f0-bf36-0148288d64d2")
		)
		(fp_line
			(start 4.39 -3.15)
			(end 4.39 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c34bcd75-cc9f-4655-9dd3-50aedc7e01a6")
		)
		(fp_line
			(start 0.69 -3.15)
			(end 0.69 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4975905b-c964-48e6-9f6b-3847a40ba5a7")
		)
		(fp_line
			(start -2.46 -3.15)
			(end -2.46 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "325cf626-0d10-4e72-ac30-914a1ff958ed")
		)
		(fp_line
			(start -2.46 -1.88)
			(end 7.54 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b052be60-4bd1-45ca-9536-c6966953ff45")
		)
		(fp_line
			(start 7.54 1.25)
			(end 7.54 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ebc2a8d6-c1c3-42b3-953d-b32ef3f618fd")
		)
		(fp_line
			(start -2.46 1.25)
			(end 7.54 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6ef35c91-ad04-4e36-bb2e-1377a3f5b53b")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 -4.27 -90)
			(layer "F.Fab")
			(uuid "c6338c2e-f287-46de-a31d-78a71a901a68")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 83 "/Triac Circuit11/High_Voltage_L")
			(pinfunction "A1")
			(pintype "passive")
			(uuid "aae25fe4-b766-4e69-8a37-3f6d607b86fc")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/Triac Circuit11/High_Voltage_Out")
			(pinfunction "A2")
			(pintype "passive")
			(uuid "83fec880-9260-4194-b7a7-d4b3c1bf9a7e")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 145 "Net-(Q23-G)")
			(pinfunction "G")
			(pintype "input")
			(uuid "b345db57-659d-4fd4-8988-ffa2d362bdf9")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
		(layer "F.Cu")
		(uuid "ea28b0b6-85f9-44a4-9a9d-13615241f1cc")
		(at 77 60.88 90)
		(descr "Terminal Block Phoenix MKDS-3-2-5.08, 2 pins, pitch 5.08mm, size 10.2x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-3-2-5.08 pitch 5.08mm size 10.2x11.2mm^2 drill 1.3mm pad 2.6mm")
		(property "Reference" "J11"
			(at 3.1 -2.999999 -90)
			(layer "F.SilkS")
			(uuid "d0d3b5fc-c952-41a2-bbed-c47c5cd34f96")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 2.539999 6.36 90)
			(layer "F.Fab")
			(uuid "43d61a1d-9894-4cc0-a957-6b7514acb403")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "09801cc3-5c0e-4c29-a890-588510374ead")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "db3a4b61-2a9a-41b2-b27c-cf20a9f6c7d3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "99228989-d3b2-47e0-8c80-0d4b23fd9948")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/d20c900a-3d9a-4460-9d5d-3ed4d11c2b93/60e4d8a3-c16e-48cd-a1fd-61f2968ecc7b")
		(sheetname "Triac Circuit10")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 7.68 -5.96)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b04736f4-2209-40f6-b963-34e0b28440eb")
		)
		(fp_line
			(start -2.6 -5.96)
			(end 7.68 -5.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "207f7509-c1d0-45e6-b199-72803c97ea48")
		)
		(fp_line
			(start -2.6 -5.96)
			(end -2.6 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6f242c63-f1e8-4574-830c-49cce57d0d56")
		)
		(fp_line
			(start -2.6 -3.9)
			(end 7.68 -3.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9022dca0-73d3-486c-bfd3-48a90d8babce")
		)
		(fp_line
			(start 6.468 -1.654)
			(end 6.088 -1.274)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bf403f70-c7c7-4113-9c1c-5411bb3a1b4e")
		)
		(fp_line
			(start 1.388 -1.654)
			(end 1.281 -1.547)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cc1a63fa-4870-4c77-9383-c00a046bfd9c")
		)
		(fp_line
			(start 6.734 -1.388)
			(end 6.339 -0.992)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "89066e35-30a6-4b18-a3a0-b1da596e6a74")
		)
		(fp_line
			(start 1.654 -1.388)
			(end 1.547 -1.281)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "22194320-0933-46ae-8404-04a5e4da5a31")
		)
		(fp_line
			(start 3.822 0.992)
			(end 3.427 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "01ee235e-3dc3-4a87-9a47-701bc93a5236")
		)
		(fp_line
			(start 4.073 1.274)
			(end 3.693 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "17cb733f-ebf8-4dcc-b608-d60d1bb9731b")
		)
		(fp_line
			(start -1.548 1.281)
			(end -1.654 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1ea8572b-c712-4b24-bfaa-141f781b1625")
		)
		(fp_line
			(start -1.282 1.547)
			(end -1.388 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ee7d76aa-285d-44df-875f-a61ac1ae3e28")
		)
		(fp_line
			(start -2.6 2.3)
			(end 7.68 2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b058c3f9-7dd0-4bf0-8ded-e4314f9b0339")
		)
		(fp_line
			(start -2.6 4.8)
			(end 7.68 4.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e4245503-9e00-42fb-b848-9591454475b2")
		)
		(fp_line
			(start -2.84 4.86)
			(end -2.84 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "91846e14-cd09-4302-8e40-fff827d68ae0")
		)
		(fp_line
			(start -2.6 5.36)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9170f79a-7fb9-4e53-80a4-80f057dfe9c8")
		)
		(fp_line
			(start -2.84 5.6)
			(end -2.34 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d59b5122-b9f0-48af-a755-a2b4f7de1940")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.26 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "b39b06c5-881b-451c-ae6b-4a73b5713108")
		)
		(fp_circle
			(center 0 0)
			(end 2.18 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "a6438584-e710-426a-893e-522257c3cf07")
		)
		(fp_line
			(start 8.13 -6.4)
			(end -3.04 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "39db51f5-5f3c-42e3-9ee6-6cc420c3223b")
		)
		(fp_line
			(start -3.04 -6.4)
			(end -3.04 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0254b839-fc1a-4b93-865d-4449b20f6831")
		)
		(fp_line
			(start 8.13 5.8)
			(end 8.13 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5ccd6962-51e1-4aca-b132-01e115ec71fb")
		)
		(fp_line
			(start -3.04 5.8)
			(end 8.13 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "75977b4d-bc05-445e-9d33-fbc6ba6d88c8")
		)
		(fp_line
			(start 7.62 -5.9)
			(end 7.62 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9687d4a7-b836-4487-8e8f-c4b89c8cafee")
		)
		(fp_line
			(start -2.54 -5.9)
			(end 7.62 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "498f04c4-0cbe-48bf-bc25-8153978054be")
		)
		(fp_line
			(start -2.54 -3.9)
			(end 7.62 -3.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "add3fc6a-53f6-4765-876d-5a7dae133865")
		)
		(fp_line
			(start 6.353 -1.517)
			(end 3.564 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "29cf7493-267b-4d13-8463-6c60fa5d503c")
		)
		(fp_line
			(start 1.273 -1.517)
			(end -1.517 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "11c93031-a299-4bf0-8988-78f48704471e")
		)
		(fp_line
			(start 6.597 -1.273)
			(end 3.808 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bd636c5f-b528-4a86-b46e-0364c66af9f9")
		)
		(fp_line
			(start 1.517 -1.273)
			(end -1.273 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7f502a6b-0289-48ec-84df-b3366f2c053f")
		)
		(fp_line
			(start -2.54 2.3)
			(end 7.62 2.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "dd1ed6fc-f6be-4b17-91e4-109886b3b6c9")
		)
		(fp_line
			(start -2.54 4.8)
			(end -2.54 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d683a22c-d83e-4a06-8d35-08c9bc2f29b7")
		)
		(fp_line
			(start -2.54 4.8)
			(end 7.62 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d1fdee48-6c23-47c6-8843-ee109b9c8b66")
		)
		(fp_line
			(start 7.62 5.3)
			(end -2.04 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8c21aa0b-051f-45ed-acb8-651a344843a0")
		)
		(fp_line
			(start -2.04 5.3)
			(end -2.54 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a70741bb-6827-4566-94b0-56b140e5d00c")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.08 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "c25eff8c-18cc-4b80-8007-8ed77aeb9ece")
		)
		(fp_circle
			(center 0 0)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "5fc75319-42c6-4a19-9d65-6a5c2161e82a")
		)
		(fp_text user "${REFERENCE}"
			(at 2.539999 3.1 90)
			(layer "F.Fab")
			(uuid "457addf1-1f71-43cc-b67c-7d48df97c1a0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "/Triac Circuit10/High_Voltage_L")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "db65a582-8d39-46bb-9aca-6d4300a3b406")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/Triac Circuit10/High_Voltage_Out")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "3babf14e-af5e-4234-aae0-cedca381f989")
		)
		(model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(uuid "ead511cf-663a-4357-938d-081298c43105")
		(at 32.769287 127.14 -90)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "Q15"
			(at 6.04 -2.445 90)
			(layer "F.SilkS")
			(uuid "62c66d7a-cd37-4452-b176-09c9df083d4e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BTA16-600B"
			(at 2.54 2.5 90)
			(layer "F.Fab")
			(uuid "aa63a88e-736f-4eed-890b-b69d706b5c71")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "2b140164-d336-4efd-b4aa-8fbee3674b1f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "8c02a419-9687-4afa-8293-fa182ed89306")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "0aaee92c-a09b-4cc0-bd61-08838ac2d848")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO?220*")
		(path "/6df26bae-1f6b-42ab-99b6-42742cd98df0/d1257be0-2394-4f08-8984-f580162b15f9")
		(sheetname "Triac Circuit7")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.58 1.371)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c369699c-2724-4547-8cfe-a374451c7265")
		)
		(fp_line
			(start -2.58 -1.76)
			(end 7.66 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "98fe9d90-ffc1-4b79-bdf8-4c7979cb9826")
		)
		(fp_line
			(start -2.58 -3.27)
			(end -2.58 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e670c687-d5bd-4a82-b2cc-ce8fbeb72e21")
		)
		(fp_line
			(start -2.58 -3.27)
			(end 7.66 -3.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bd8eaf09-b16c-4ec4-9080-3709230b8091")
		)
		(fp_line
			(start 0.69 -3.27)
			(end 0.69 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dcda889d-fa12-43da-aaa0-7e6f75f726c5")
		)
		(fp_line
			(start 4.391 -3.27)
			(end 4.391 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0bec4b71-fb26-4b02-95d1-8b558f3dc43f")
		)
		(fp_line
			(start 7.66 -3.27)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "42f2b2d5-d09c-4908-b8f0-6b85dc617ef3")
		)
		(fp_line
			(start -2.71 1.51)
			(end 7.79 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f78913ca-cb55-479a-b87e-6a6918ac92c8")
		)
		(fp_line
			(start 7.79 1.51)
			(end 7.79 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ffe3d91d-11f7-4bd8-9400-bcad2cafeaad")
		)
		(fp_line
			(start -2.71 -3.4)
			(end -2.71 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1b37e26c-5f4d-484f-b784-c2b403fe94a9")
		)
		(fp_line
			(start 7.79 -3.4)
			(end -2.71 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cca35dfc-92ff-401c-ada7-273c9f698bdb")
		)
		(fp_line
			(start -2.46 1.25)
			(end 7.54 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d69d86c2-8a68-4bf3-b236-8abc068c7e79")
		)
		(fp_line
			(start 7.54 1.25)
			(end 7.54 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "80e55e92-06ae-49f5-8196-2b7028fb3a13")
		)
		(fp_line
			(start -2.46 -1.88)
			(end 7.54 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0aa6a9a4-cf86-4f8f-8ebc-0678dfb6032c")
		)
		(fp_line
			(start -2.46 -3.15)
			(end -2.46 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "848438a7-9090-4eda-836a-c58d42c53ca2")
		)
		(fp_line
			(start 0.69 -3.15)
			(end 0.69 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8578c8d5-bf4f-48d7-bacb-b2056f449786")
		)
		(fp_line
			(start 4.39 -3.15)
			(end 4.39 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "47ec0c08-e9c4-46a2-bb66-d3469de754c1")
		)
		(fp_line
			(start 7.54 -3.15)
			(end -2.46 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2064b033-551c-4dc7-9f3e-60f05c874204")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 -4.27 90)
			(layer "F.Fab")
			(uuid "860b13bc-ada6-4df7-8c0d-e7420a8f768d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "/Triac Circuit7/High_Voltage_L")
			(pinfunction "A1")
			(pintype "passive")
			(uuid "9d896699-f43d-4797-9921-06611ee93964")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/Triac Circuit7/High_Voltage_Out")
			(pinfunction "A2")
			(pintype "passive")
			(uuid "329bf472-1eeb-48ab-bdf5-0979b3c2080a")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 270)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(Q15-G)")
			(pinfunction "G")
			(pintype "input")
			(uuid "0856e51c-b542-40cd-9590-53aad606a577")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-6_W7.62mm"
		(layer "F.Cu")
		(uuid "ecadb762-1de9-405e-9c05-e241200da82d")
		(at 57.142855 87.435)
		(descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U14"
			(at 3.599999 -2.33 180)
			(layer "F.SilkS")
			(uuid "3024f6ed-987a-49c5-bdd7-fb9bcdca2b92")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MOC3021M"
			(at 3.81 7.409999 180)
			(layer "F.Fab")
			(uuid "de73219a-d959-438d-940f-36672cb2a403")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "470c2dec-2ff0-4f35-b27f-bcc0cf8eab75")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3023M-D.PDF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "5c97c897-285e-4fe5-8aae-791054ae7d6e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "db6f41e5-4815-4503-9a4f-fae3eebe402c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*")
		(path "/fb144577-8e6f-488b-ba1b-870763a27401/0262e914-5435-478f-be04-ece49b8102cf")
		(sheetname "Triac Circuit12")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6b207349-d532-49c9-b3a9-4ea9ee8834c9")
		)
		(fp_line
			(start 1.16 6.41)
			(end 6.46 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b1853622-8872-4b42-8558-1cda11e2c463")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bf4c5f82-6e12-4662-895f-738beb07a45e")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4b54d26d-a652-49ff-88b0-8c92f9e3bd63")
		)
		(fp_line
			(start 6.46 6.41)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7e1175bb-bdc6-41b8-b6a9-73f759f5f2ac")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cb666f5e-1dfa-4544-bf76-8b19db6a1575")
		)
		(fp_line
			(start -1.1 -1.55)
			(end -1.1 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eb038e08-18b5-476e-be76-5029bc8edb1c")
		)
		(fp_line
			(start -1.1 6.6)
			(end 8.7 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ce7bd7e3-1936-4460-91e3-84694c5ce828")
		)
		(fp_line
			(start 8.7 -1.55)
			(end -1.1 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9f582a74-9738-4f87-bb77-24a0a9b540ca")
		)
		(fp_line
			(start 8.7 6.6)
			(end 8.7 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e1ae8815-277d-497b-86a3-c9ac7ceec167")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8c31e0a6-dcaf-4f53-8f90-c43ed4befc35")
		)
		(fp_line
			(start 0.635 6.35)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ecfb7398-5b4a-4c29-9119-f74858ff852d")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d3e2a634-9483-4b53-9884-3d02580b5eb1")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b594557a-3945-498c-b89a-ff9a4339bf6a")
		)
		(fp_line
			(start 6.985 6.35)
			(end 0.635 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "14cc925f-b714-47bd-889d-59fa85230fe2")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.539999 180)
			(layer "F.Fab")
			(uuid "8b0990bf-011e-45f8-9cee-e12ca4942674")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 121 "Net-(R38-Pad1)")
			(pintype "passive")
			(uuid "fd013f26-96b1-4107-bca4-0549d8cd5c91")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 150 "Net-(Q26-C)")
			(pintype "passive")
			(uuid "210dc676-8b98-45c7-a4ce-48c7a25e1105")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "unconnected-(U14-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "ed918334-085d-4f78-bd3f-a6322d18e954")
		)
		(pad "4" thru_hole oval
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 148 "Net-(Q25-G)")
			(pintype "passive")
			(uuid "75f14c80-ed41-470a-aab2-1b66a2e936b5")
		)
		(pad "5" thru_hole oval
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 104 "unconnected-(U14-NC-Pad5)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "a31ca18e-49ec-4535-b06e-aa0629e0bcce")
		)
		(pad "6" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(R37-Pad1)")
			(pintype "passive")
			(uuid "3deb70c0-879c-4ed8-ba84-45563ef88465")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-6_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "ed0afd21-8cc0-427b-ba9d-856c20fb47af")
		(at 53.605355 132.88 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R47"
			(at 0 -1.82 180)
			(layer "F.SilkS")
			(uuid "0fa7dbe2-228f-41e3-a1bd-dd4713fcf3a9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at 0 1.82 180)
			(layer "F.Fab")
			(uuid "ece55141-1bc8-41ce-9518-9c74657b9a9a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "07f1a8ee-1c1d-4ff4-8593-14a105457fd1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "259b1fc0-ad44-4bcc-8c85-6df4ce266349")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "6e21c315-9235-4fb9-8f71-b6cb202e518e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/4b0c0d83-8522-4ffe-8435-2c6bf5567543/de24ad75-a874-4d54-a682-b1d6f2079d30")
		(sheetname "Triac Circuit15")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a4fcb475-62b3-4f2a-888a-98588c19bbde")
		)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c36f877e-9aa3-4923-af1f-27398d840474")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c5f6db6d-0832-4920-b6ed-b228306bd500")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fce9ddf1-0e5b-4681-a501-9f9c8ac04866")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9acf5337-357e-44e1-b082-247edd8fbee8")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5237584e-049c-4e9f-9546-cdcf3f955ebf")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "777ea3c3-19ed-40c4-b0b8-a3ff5f322610")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e6cc6bfe-17c7-45c1-9411-d46740e569ff")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a9f0123e-e184-4788-9b72-f28eaa7c667a")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "af85df47-4607-4fc4-9a86-cc0b85e00397")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
			(uuid "76970c34-3a58-4a79-a192-61644c5fdd39")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 128 "Net-(R47-Pad1)")
			(pintype "passive")
			(uuid "38946500-fa17-479f-ab2e-c59ad84935fd")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 37 "+3V3")
			(pintype "passive")
			(uuid "3f9e17f2-7287-4fc9-bd58-df4b0af7cb42")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
		(layer "F.Cu")
		(uuid "ee82b68e-edcf-4d9a-8c83-5f8c4dfcb9b7")
		(at 25 50.88 -90)
		(descr "Terminal Block Phoenix MKDS-3-2-5.08, 2 pins, pitch 5.08mm, size 10.2x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-3-2-5.08 pitch 5.08mm size 10.2x11.2mm^2 drill 1.3mm pad 2.6mm")
		(property "Reference" "J3"
			(at 3.1 -3 90)
			(layer "F.SilkS")
			(uuid "f7a87aaa-21a9-4eab-9cd0-4ffd282e4011")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 2.54 6.36 -90)
			(layer "F.Fab")
			(uuid "dfd65f3d-d41c-4cab-8dbd-9330fe4211f8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "4cef54ef-835f-431c-b60f-2729da0883ce")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "4b6cb961-cf80-461d-bd3a-aecbea607a91")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "ec3afc40-2c74-4d7f-b4ce-5c0b7e13ca2b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/fef2553d-539f-40e4-b7bd-376e44ab9a6f/60e4d8a3-c16e-48cd-a1fd-61f2968ecc7b")
		(sheetname "Triac Circuit2")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.84 5.6)
			(end -2.34 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0aa9690e-f42b-4e9e-8ffa-10329b39b792")
		)
		(fp_line
			(start -2.6 5.36)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9a371736-ed7a-4c95-9782-0faf88e908ed")
		)
		(fp_line
			(start -2.84 4.86)
			(end -2.84 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ea0a3888-96d1-4bac-b04d-72b89234bdf5")
		)
		(fp_line
			(start -2.6 4.8)
			(end 7.68 4.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e589fa13-7135-4fbf-acce-477538873208")
		)
		(fp_line
			(start -2.6 2.3)
			(end 7.68 2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a66bf97f-a3cf-4a0c-9e8f-0e7c8fe30531")
		)
		(fp_line
			(start -1.282 1.547)
			(end -1.388 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fc5fcb10-fc4c-411c-8b4e-6565b6b5e69f")
		)
		(fp_line
			(start -1.548 1.281)
			(end -1.654 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "55dc44db-8e5e-4435-9557-f28f14378db0")
		)
		(fp_line
			(start 4.073 1.274)
			(end 3.693 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b06c3e2f-a039-48c4-b53a-02d7ce734e2e")
		)
		(fp_line
			(start 3.822 0.992)
			(end 3.427 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "61d1b8c8-02c2-46ce-a3c9-6c96e24e5b33")
		)
		(fp_line
			(start 1.654 -1.388)
			(end 1.547 -1.281)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1565d560-a74f-4c62-9205-e8f25b3cd229")
		)
		(fp_line
			(start 6.734 -1.388)
			(end 6.339 -0.992)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7fe814ea-c91b-45ff-aa28-4e45718c668d")
		)
		(fp_line
			(start 1.388 -1.654)
			(end 1.281 -1.547)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "107cec99-adcd-4c83-b7ac-f831f1a6d962")
		)
		(fp_line
			(start 6.468 -1.654)
			(end 6.088 -1.274)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "686a8305-6ade-46bd-bcdb-31a040c151b5")
		)
		(fp_line
			(start -2.6 -3.9)
			(end 7.68 -3.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5fa12169-2ff0-47e6-bc47-da1cc800686b")
		)
		(fp_line
			(start -2.6 -5.96)
			(end -2.6 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d467e223-8088-4b61-831c-c791b70905a5")
		)
		(fp_line
			(start -2.6 -5.96)
			(end 7.68 -5.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6237d639-336a-4c5c-b1ec-018f5710f598")
		)
		(fp_line
			(start 7.68 -5.96)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "029da5b0-767c-4d8c-8e8c-62b95025e9e3")
		)
		(fp_circle
			(center 0 0)
			(end 2.18 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "26989004-ec75-4fcb-b4c1-ab83786a604b")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.26 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "df76a87d-c132-48f5-832e-234ff5bfac2d")
		)
		(fp_line
			(start -3.04 5.8)
			(end 8.13 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9f6ee423-910a-40f4-9445-3dabd1d6d243")
		)
		(fp_line
			(start 8.13 5.8)
			(end 8.13 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "98715645-0582-4f7b-9bf0-554723e3c78e")
		)
		(fp_line
			(start -3.04 -6.4)
			(end -3.04 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8894e1f3-7cd0-41a8-b045-b33beb560dd7")
		)
		(fp_line
			(start 8.13 -6.4)
			(end -3.04 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "00239e8a-8b33-4289-a95e-cee35f630879")
		)
		(fp_line
			(start -2.04 5.3)
			(end -2.54 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c2311bfb-88a3-497c-bafd-010ddfc38a2f")
		)
		(fp_line
			(start 7.62 5.3)
			(end -2.04 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ab293560-76ac-4d7f-b529-59ea72eb0293")
		)
		(fp_line
			(start -2.54 4.8)
			(end 7.62 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b3f0d683-fb5a-4819-b3c9-a199a34a57fc")
		)
		(fp_line
			(start -2.54 4.8)
			(end -2.54 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7c285f9e-f8c4-488d-9f44-766edceba585")
		)
		(fp_line
			(start -2.54 2.3)
			(end 7.62 2.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f1659d38-3ac4-4651-bd3c-5a38c767a0f8")
		)
		(fp_line
			(start 1.517 -1.273)
			(end -1.273 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "08c57bb2-8061-4fdb-8720-7bb295cae10d")
		)
		(fp_line
			(start 6.597 -1.273)
			(end 3.808 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0d80f2a3-def3-4ca9-a6de-b5c2afd834ad")
		)
		(fp_line
			(start 1.273 -1.517)
			(end -1.517 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "14e70b38-e21a-43cf-a151-cf6e830106dc")
		)
		(fp_line
			(start 6.353 -1.517)
			(end 3.564 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0095a16f-cba9-4c23-b855-8f4724034cd5")
		)
		(fp_line
			(start -2.54 -3.9)
			(end 7.62 -3.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b2e97c5f-308b-4665-8450-c873e3b4c8bd")
		)
		(fp_line
			(start -2.54 -5.9)
			(end 7.62 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4a152f57-8699-4185-88cc-a62a791a995e")
		)
		(fp_line
			(start 7.62 -5.9)
			(end 7.62 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4fae76bc-1cb2-451b-b8ce-16127310ce7f")
		)
		(fp_circle
			(center 0 0)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "b913d6e7-1c1b-456d-a512-db4a7a606e4c")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.08 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "a3a56eee-75fe-42c2-9aa9-d48f22189c21")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 3.1 -90)
			(layer "F.Fab")
			(uuid "31f383d6-f9e9-4d0c-851e-ab7b41a0ed7e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/Triac Circuit2/High_Voltage_L")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "77262df0-c04a-415b-ab6f-1c74422eb3c0")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/Triac Circuit2/High_Voltage_Out")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "5b1809b8-c5f8-4dd5-b571-cbb172e59ccd")
		)
		(model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "f023838e-ef66-4870-b884-43153dcf0de2")
		(at 53.605355 71.92 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R35"
			(at 0 -1.82 180)
			(layer "F.SilkS")
			(uuid "9ba610cf-d889-4ba7-9165-6836fb6b695a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at 0 1.82 180)
			(layer "F.Fab")
			(uuid "c2af4624-0145-407b-8445-8ce478cd0477")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "a2b6b9da-4566-4ace-b556-e42d99c2fb40")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "7be88ae3-dfad-4294-84e7-88dfe5dc6f70")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "c0947b11-d1a1-4cbe-b876-b270f0bc371a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/15d8fe7c-2a9b-438f-a777-3e4687188af1/de24ad75-a874-4d54-a682-b1d6f2079d30")
		(sheetname "Triac Circuit11")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b280821b-f7ea-4b20-a2fb-6254a3962db9")
		)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "21ca1801-fb23-4706-8ed1-3617fe9c370b")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c3c686d4-f1bb-4349-9323-d31d6bab4b32")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a0421147-47f6-4651-a727-5222ab480c90")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c87a5dca-2325-41a2-a137-a057b69a742f")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8bced043-2cb1-4bb5-841a-68bc8262c1ec")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "813724b8-974c-4b1c-8461-c1edd95fd5b7")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "624ae07f-d1b0-4e58-a0a5-3ab71678565c")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e55c1ac4-f911-47a1-915e-43ed83f71671")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c908e877-6f38-4663-9be8-e8eaa7fe076f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
			(uuid "8ba50d26-4ac6-439a-949c-742039bdc13e")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 120 "Net-(R35-Pad1)")
			(pintype "passive")
			(uuid "be3d5443-913b-455b-bc77-6eabd4969830")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 37 "+3V3")
			(pintype "passive")
			(uuid "ada3f7c5-99ce-45e7-b57f-26d46b32e123")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
		(layer "F.Cu")
		(uuid "f0c15bb4-4b6d-4194-8150-d6cef8956486")
		(at 77 30.4 90)
		(descr "Terminal Block Phoenix MKDS-3-2-5.08, 2 pins, pitch 5.08mm, size 10.2x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-3-2-5.08 pitch 5.08mm size 10.2x11.2mm^2 drill 1.3mm pad 2.6mm")
		(property "Reference" "J9"
			(at 3.1 -2.999999 -90)
			(layer "F.SilkS")
			(uuid "4e44aa62-79bb-4fcb-8295-044326e395a2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 2.539999 6.36 90)
			(layer "F.Fab")
			(uuid "072135d4-7838-43e4-9c38-39a35099f6f5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "eda4a113-c278-413c-adea-1acee9cc84df")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "55eb9d34-1794-4fe6-9f2d-619844e54f5c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "ea8096c7-5a61-4188-9fb3-39615cf36f2c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/a837c47c-5707-46fe-8eca-0b07e116b13e/60e4d8a3-c16e-48cd-a1fd-61f2968ecc7b")
		(sheetname "Triac Circuit8")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 7.68 -5.96)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8293c948-0d9a-4841-8445-06ae3b4cdcde")
		)
		(fp_line
			(start -2.6 -5.96)
			(end 7.68 -5.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bdb0630a-7896-402e-bf17-948de203ade6")
		)
		(fp_line
			(start -2.6 -5.96)
			(end -2.6 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "30a7ebb7-0d82-4cb2-9211-7fdb0f69753a")
		)
		(fp_line
			(start -2.6 -3.9)
			(end 7.68 -3.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "02821a67-782f-459b-b51f-17ba7e64a4ff")
		)
		(fp_line
			(start 6.468 -1.654)
			(end 6.088 -1.274)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f74f960c-f35f-449d-b96a-c3e4d09e3605")
		)
		(fp_line
			(start 1.388 -1.654)
			(end 1.281 -1.547)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1ec1d6ea-b187-41b7-b605-ace1589e11f4")
		)
		(fp_line
			(start 6.734 -1.388)
			(end 6.339 -0.992)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "631ce88a-6662-4b3a-b10f-02ba664c12ee")
		)
		(fp_line
			(start 1.654 -1.388)
			(end 1.547 -1.281)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "15fe99a6-f9b9-4cd6-9430-374fcbd7da9a")
		)
		(fp_line
			(start 3.822 0.992)
			(end 3.427 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "aa6ee74a-f6ef-4ef3-8ba8-9f4ca66b9173")
		)
		(fp_line
			(start 4.073 1.274)
			(end 3.693 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8f72f9b8-ba2e-4a90-9ace-6e3c3f21c9e9")
		)
		(fp_line
			(start -1.548 1.281)
			(end -1.654 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3be56f70-4965-4952-b72e-461b5f8a522d")
		)
		(fp_line
			(start -1.282 1.547)
			(end -1.388 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7a1c9c82-e91c-42d0-bf35-e1e90bc5c8e7")
		)
		(fp_line
			(start -2.6 2.3)
			(end 7.68 2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "23d120a0-fcc4-4b3e-8e7d-c65026d356e0")
		)
		(fp_line
			(start -2.6 4.8)
			(end 7.68 4.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "953e56f1-66e0-463b-9daf-4e0f7b9021b5")
		)
		(fp_line
			(start -2.84 4.86)
			(end -2.84 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "99930998-4976-486c-9052-281f09fc7396")
		)
		(fp_line
			(start -2.6 5.36)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a3eeae87-d430-414e-bc24-f95ba35a5743")
		)
		(fp_line
			(start -2.84 5.6)
			(end -2.34 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "70be7dd6-50f5-43bb-aa7e-9e74a0aaabb0")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.26 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "5f37fccc-a956-41e8-ad22-8604ec3400ba")
		)
		(fp_circle
			(center 0 0)
			(end 2.18 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "3d4f3d48-24cb-4e09-9f77-e514c34c8654")
		)
		(fp_line
			(start 8.13 -6.4)
			(end -3.04 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5d37d0fe-4f94-4b83-b07f-3b49f9051020")
		)
		(fp_line
			(start -3.04 -6.4)
			(end -3.04 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7ec668fd-831a-4264-babf-0f16b5a35e64")
		)
		(fp_line
			(start 8.13 5.8)
			(end 8.13 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e6240e77-766b-4b15-b24f-2e0bf9fff68d")
		)
		(fp_line
			(start -3.04 5.8)
			(end 8.13 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "723b1dfe-8e0d-4de4-be77-5a82d845342e")
		)
		(fp_line
			(start 7.62 -5.9)
			(end 7.62 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4eb69814-5c42-4746-88c1-8f580c249895")
		)
		(fp_line
			(start -2.54 -5.9)
			(end 7.62 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "78e021c1-33a5-4ced-84ed-77a968c7ac77")
		)
		(fp_line
			(start -2.54 -3.9)
			(end 7.62 -3.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e8fe66c1-6917-4130-b922-f27b29a285c8")
		)
		(fp_line
			(start 6.353 -1.517)
			(end 3.564 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "739ee961-eb25-4b3f-9bb5-66b893b1db30")
		)
		(fp_line
			(start 1.273 -1.517)
			(end -1.517 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "16d65895-eca4-4230-b423-f5942884cb85")
		)
		(fp_line
			(start 6.597 -1.273)
			(end 3.808 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fbfd85f1-e84e-4ef9-8678-e6bc443fc122")
		)
		(fp_line
			(start 1.517 -1.273)
			(end -1.273 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3c90d225-07de-4d8a-9323-1bb8f482ff98")
		)
		(fp_line
			(start -2.54 2.3)
			(end 7.62 2.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "74e44b1d-aa8c-4144-9d5a-b8575db07540")
		)
		(fp_line
			(start -2.54 4.8)
			(end -2.54 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f0e94e9c-8d3f-47a2-8994-3fd387fe4cfa")
		)
		(fp_line
			(start -2.54 4.8)
			(end 7.62 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3803875a-8d75-427f-8946-3789e8550c85")
		)
		(fp_line
			(start 7.62 5.3)
			(end -2.04 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3570732e-1bc7-4ada-82a0-1865f42bf1b4")
		)
		(fp_line
			(start -2.04 5.3)
			(end -2.54 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0f68ad0f-d939-44b2-bcc5-86ae30013758")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.08 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "82e6bed5-c61f-4572-9c42-f3ec4623391b")
		)
		(fp_circle
			(center 0 0)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "85e6db00-3e5c-4f85-b4ad-053e949627db")
		)
		(fp_text user "${REFERENCE}"
			(at 2.539999 3.1 90)
			(layer "F.Fab")
			(uuid "e35d991f-6b97-457e-9833-d24a78715d9a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "/Triac Circuit8/High_Voltage_L")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "f842e5ac-b364-4253-b169-baca5566d77a")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/Triac Circuit8/High_Voltage_Out")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "ca6ac2dd-2441-4579-84a3-c426f5aa4a94")
		)
		(model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "f1de17b2-77f9-4731-89b1-0e00eaea67cd")
		(at 53.542855 43.64 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R30"
			(at 0 -1.82 180)
			(layer "F.SilkS")
			(uuid "5fd2b760-c016-4b2d-b398-e9b65921961f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at -3.64 0 180)
			(layer "F.Fab")
			(uuid "8a6d0e9f-35fd-49b4-bcfd-bf4c1393d045")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "45fcf520-3379-4b03-a299-71a4f9df49f3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "8a73ac10-d748-4e39-8917-3c1379f63b97")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "6407dfc7-f20b-4bd5-8859-7e7ab232b70a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/f251f0b5-0f8b-4418-bbfe-69d55a4bdeb8/ca31a324-056f-45d6-b948-82e97db62734")
		(sheetname "Triac Circuit9")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "423c70a5-efcb-4550-a031-a19504279ae1")
		)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b844e201-b8ae-4f29-a5c5-b71aa7365157")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2a9921d8-2e97-4bc0-bd9d-9526e7d0051e")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ec989f6a-bd30-4fe2-a39d-26b0c2f9967b")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cf6a2fb6-301e-47f3-a4a0-9ef674598de9")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c601191d-f582-4c40-8ad8-05855d17c540")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4a5b4456-9bfa-4ab6-b9b8-d82d95ac2986")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3d532bb5-150e-451b-823b-48e360f864e1")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0c7f3068-d7bd-4edc-bafd-a387dbfe8fb4")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ae2d78ff-28fa-4915-bc4e-446da5c863a6")
		)
		(fp_text user "${REFERENCE}"
			(at 3.04 0.01 180)
			(layer "F.Fab")
			(uuid "ad4b4db0-56fe-4cd1-a5ce-265d1900b152")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 140 "Net-(Q20-B)")
			(pintype "passive")
			(uuid "23a4c97c-3f20-4dd7-9098-c93ee6d78d1b")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 132 "/Triac Circuit9/Enable")
			(pintype "passive")
			(uuid "77f6b099-fdbd-45a8-8eb2-08a3503ba2ff")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "f1e61bee-c45e-4abf-b99e-f3058790e04a")
		(at 48.023216 65.32 180)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q8"
			(at 0 -2.4 0)
			(layer "F.SilkS")
			(uuid "b55492fd-a78d-4250-a58b-0123d48a2337")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BC818"
			(at 0 2.4 0)
			(layer "F.Fab")
			(uuid "e6121f45-5f4b-4ea1-b942-7d37780dbe78")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "975addf9-3e46-4de3-88a7-41139eb6caa5")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BC818-D.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "001afa2d-3808-4482-b4aa-a8f72940a6a3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "fa20215a-b8e0-470a-9ad7-f014cb8b29ee")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/1abc9394-30bb-4ef5-a1be-aa230dbd1566/00e550ea-8431-483d-ac3c-b4a719825546")
		(sheetname "Triac Circuit3")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 1.56)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2f880e71-9b56-4b54-8857-6ab7304113d7")
		)
		(fp_line
			(start 0 1.56)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f209874f-6774-4502-b813-c6545af309e1")
		)
		(fp_line
			(start 0 -1.56)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "28c2fb03-6c08-4239-a627-9737da7f832c")
		)
		(fp_line
			(start 0 -1.56)
			(end -1.675 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a5d4b751-0fff-4acd-a95f-37668803ef99")
		)
		(fp_line
			(start 1.92 1.7)
			(end 1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7f2e385f-29da-4889-b829-c6911d163636")
		)
		(fp_line
			(start 1.92 -1.7)
			(end -1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "41df7f18-947d-4dce-aeb9-dfe77362ef7e")
		)
		(fp_line
			(start -1.92 1.7)
			(end 1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a59715e4-7f7a-4d29-b113-6b370d55b1a6")
		)
		(fp_line
			(start -1.92 -1.7)
			(end -1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3e633c4f-1b42-4bcb-8315-0687264710b6")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bb6f3b3d-e217-4a22-b8bd-d9d4099c6b6c")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8a30ae3a-55fa-4492-b47a-3034a0c87631")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8c410051-7d26-4d94-a288-f834bd09b89c")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b6f9bcf8-7384-48c5-a460-c5445d0c2b7c")
		)
		(fp_line
			(start -0.65 -1.125)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c0569eb6-a758-4076-9b03-71b698b91048")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "43436b04-285a-45c9-8c96-f1903f8dce52")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 59 "Net-(Q8-B)")
			(pinfunction "B")
			(pintype "input")
			(uuid "0ea9fa4b-0393-462f-8be8-44b1221543f0")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "GND")
			(pinfunction "E")
			(pintype "passive")
			(uuid "45bde967-5b37-45e0-bb2c-ca6f112783c9")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 60 "Net-(Q8-C)")
			(pinfunction "C")
			(pintype "passive")
			(uuid "9177b2bf-a099-4cf3-a154-79511bcd3c0c")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(uuid "f2c0adf9-f296-4b4b-9d0e-44203f4f0aeb")
		(at 54.35 177.14)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 0 -1.85 0)
			(layer "F.SilkS")
			(uuid "995efcae-77ec-4096-a597-7fbb21cfc037")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100n"
			(at 0 1.85 0)
			(layer "F.Fab")
			(uuid "cecb95a9-d198-437f-a0ee-07012c559c2b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Capacitor_SMD:C_1206_3216Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2e6b7c92-0a17-42a1-9380-a454fe224db1")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ab95d700-4828-46e9-b0ea-36972e77bbf2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "dd2fba8b-7e93-45f5-9747-8c8012a7be4c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/020d656a-0586-4bb4-baa7-ce6155a59031")
		(sheetname "Główny")
		(sheetfile "16_ChannelPowerControlBoard.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.711252 -0.91)
			(end 0.711252 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "19e920fd-64a0-47be-9481-8ef91ec4719f")
		)
		(fp_line
			(start -0.711252 0.91)
			(end 0.711252 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "168a4cb4-5d38-4a34-8b74-0c2331d15551")
		)
		(fp_line
			(start -2.3 -1.15)
			(end 2.3 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a98ef38b-7012-49d8-b6c5-f3bb361be86b")
		)
		(fp_line
			(start -2.3 1.15)
			(end -2.3 -1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0b77a97c-2a6a-489e-8f0d-9e9c8696fbe3")
		)
		(fp_line
			(start 2.3 -1.15)
			(end 2.3 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d11cdab3-beb6-4e6a-8e61-fe4541f55dad")
		)
		(fp_line
			(start 2.3 1.15)
			(end -2.3 1.15)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "757cf085-4eea-447c-b05c-dc6b4c3105a3")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2e96a36f-1307-4a8e-81f6-dee9a7cc3aa3")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e8f975c2-23d4-4600-b7f4-779cd4062c25")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3ed6741f-728d-445e-a747-ef38db6d5355")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d3c1eb0c-2fae-4904-9202-7e5396b4fd32")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c8d893b2-e443-4d35-a0bf-15902c7731df")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 164 "Net-(C1-Pad1)")
			(pintype "passive")
			(uuid "0959323f-65f7-465d-9a75-1549da0d8f22")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 41 "GND")
			(pintype "passive")
			(uuid "84ea3e5a-5cdc-4020-a3c9-45afef3556e3")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-6_W7.62mm"
		(layer "F.Cu")
		(uuid "f3f61655-d9b4-4def-a069-b9be2462e4f3")
		(at 44.857145 54.805 180)
		(descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U4"
			(at 3.6 -2.33 0)
			(layer "F.SilkS")
			(uuid "2fe70c8c-44ea-405f-b0dc-e74e40fdaaa8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MOC3021M"
			(at 3.81 7.41 0)
			(layer "F.Fab")
			(uuid "1664cf01-3218-4471-8355-4ceced9aa55b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "b544c1d2-d361-4b27-a696-7dd46b70b777")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3023M-D.PDF"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "1609ec76-f314-4e63-8cec-e461977578ba")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "330b66b9-f95c-4570-8126-3207b431e245")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*")
		(path "/fef2553d-539f-40e4-b7bd-376e44ab9a6f/0262e914-5435-478f-be04-ece49b8102cf")
		(sheetname "Triac Circuit2")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 6.46 6.41)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f6611b82-a956-44d1-8122-2256caffabde")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d3195a67-39fa-4560-9d57-103d3a4c9fc7")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e191c26f-3a2c-4f14-b964-bef87052caf7")
		)
		(fp_line
			(start 1.16 6.41)
			(end 6.46 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6d5f4f74-a60a-432e-a1e4-1c90bc0265ca")
		)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "68a7ea97-cbca-45cb-acc9-5e23d9e8ac23")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b9bb2262-8b1e-4bc0-bef2-5bd45bf2f9dc")
		)
		(fp_line
			(start 8.7 6.6)
			(end 8.7 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fbd49e55-e7f6-49e2-a99c-d7f69b12a3b7")
		)
		(fp_line
			(start 8.7 -1.55)
			(end -1.1 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e4c4481a-b70c-4bf1-b2c0-701950b2de21")
		)
		(fp_line
			(start -1.1 6.6)
			(end 8.7 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c9f73e1e-5bb3-477e-a071-36bec76b483e")
		)
		(fp_line
			(start -1.1 -1.55)
			(end -1.1 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a788f619-509e-4603-99c0-517d5d1d0fe9")
		)
		(fp_line
			(start 6.985 6.35)
			(end 0.635 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "53921d56-322b-4d13-a7ec-4f4fd59b182f")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "19105a99-da3f-4f6f-a20b-5fc27ac4b5b5")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e9f831ed-13ce-43ea-975b-ad5aaa5fe789")
		)
		(fp_line
			(start 0.635 6.35)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "45cc4905-34b8-477f-8533-ea398fae0305")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "97e2a509-9fd3-4286-bace-43c71d85b9ef")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.54 0)
			(layer "F.Fab")
			(uuid "f9fcf5fe-f156-455b-b379-cb38f0dc03ad")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 111 "Net-(R8-Pad1)")
			(pintype "passive")
			(uuid "cb3e4f92-e6cb-4ced-ab43-9c61f2456133")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "Net-(Q6-C)")
			(pintype "passive")
			(uuid "d053df20-55d5-4b22-a2f8-b519be931dbb")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "unconnected-(U4-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "f0e4a3f6-d1c3-482c-838b-67c13d9243d8")
		)
		(pad "4" thru_hole oval
			(at 7.62 5.08 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(Q5-G)")
			(pintype "passive")
			(uuid "e9129ee8-1030-42b8-a517-82b47dc5cf4b")
		)
		(pad "5" thru_hole oval
			(at 7.62 2.54 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 89 "unconnected-(U4-NC-Pad5)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "93a7b73f-6986-44d0-90e0-082a627e411d")
		)
		(pad "6" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "Net-(R7-Pad1)")
			(pintype "passive")
			(uuid "feca7d9a-bcab-4a81-9fb5-32bc2dcb0138")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-6_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(uuid "f4416046-a967-434d-8aed-9d522251cd5f")
		(at 69.2625 174.975)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "D1"
			(at 0 -2.4 0)
			(layer "F.SilkS")
			(uuid "104091be-ae2b-4703-be8f-4a063d265e3a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MMBZxx"
			(at 0 2.4 0)
			(layer "F.Fab")
			(uuid "26a01a88-f3f3-408a-8903-9a961387aa86")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "54b7b265-8bf2-43b4-895c-eb019774efb4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/MMBZ5V6ALT1-D.PDF"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "f85fb74c-0ee9-4f8f-a55b-83837a23afad")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Double Zener Diode, Common Anode, 225mW, SOT-23"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a603e3a3-fd5a-4356-a3cf-3caa1e11df8a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "SOT?23*")
		(path "/a7def4dc-d2ed-4c31-8eed-330fd2a6cd98")
		(sheetname "Główny")
		(sheetfile "16_ChannelPowerControlBoard.kicad_sch")
		(attr smd)
		(fp_line
			(start 0 -1.56)
			(end -0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8f41758e-3b9d-428a-94a4-fb50bd2ef80d")
		)
		(fp_line
			(start 0 -1.56)
			(end 0.65 -1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "25f64dd5-d456-45e9-a230-d1b153baa485")
		)
		(fp_line
			(start 0 1.56)
			(end -0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5ba837e7-9384-4985-b94f-3b8e23185ada")
		)
		(fp_line
			(start 0 1.56)
			(end 0.65 1.56)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cbe8f6bc-d2a7-49e1-97af-778fa0845b8b")
		)
		(fp_poly
			(pts
				(xy -1.1625 -1.51) (xy -1.4025 -1.84) (xy -0.9225 -1.84) (xy -1.1625 -1.51)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill solid)
			(layer "F.SilkS")
			(uuid "e6d0a713-92a7-40ad-9ca6-b75f8c3651c3")
		)
		(fp_line
			(start -1.92 -1.7)
			(end -1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5e6e7364-d634-4882-b9c8-6df7993f1069")
		)
		(fp_line
			(start -1.92 1.7)
			(end 1.92 1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0a913a0b-7efd-4b71-baab-4590a75a08be")
		)
		(fp_line
			(start 1.92 -1.7)
			(end -1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "010ac95c-63a1-45bd-9219-401551d9d952")
		)
		(fp_line
			(start 1.92 1.7)
			(end 1.92 -1.7)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2668e777-f012-482a-8415-3a7cdfe3874b")
		)
		(fp_line
			(start -0.65 -1.125)
			(end -0.325 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2497949f-4b71-4173-9c12-8992a65b3462")
		)
		(fp_line
			(start -0.65 1.45)
			(end -0.65 -1.125)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f1d94b6c-68c1-4c15-a4a5-cbfcca491203")
		)
		(fp_line
			(start -0.325 -1.45)
			(end 0.65 -1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8c65463f-dcfd-403b-a7bf-896bcdaf4b94")
		)
		(fp_line
			(start 0.65 -1.45)
			(end 0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "17098623-7c09-4664-a755-83207390e135")
		)
		(fp_line
			(start 0.65 1.45)
			(end -0.65 1.45)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3da7f27f-2239-4b36-9437-9a46a10be44d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "2e329769-f198-408f-9b62-991f479cee64")
			(effects
				(font
					(size 0.32 0.32)
					(thickness 0.05)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 181 "Net-(U1-CANL)")
			(pinfunction "K")
			(pintype "passive")
			(uuid "a69b31d6-5637-45ed-b47f-03a162a7bc0d")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "GND")
			(pinfunction "K")
			(pintype "passive")
			(uuid "a19b5bd1-7096-4eaf-8742-64727347a403")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 178 "unconnected-(D1-A-Pad3)")
			(pinfunction "A")
			(pintype "passive")
			(uuid "34eb63ca-c025-474e-a8d2-b2397d8b66df")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(uuid "f59e4d08-aa5c-4b5b-af2f-761d7e29dd09")
		(at 33.4 168.6 90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R60"
			(at 2.54 -1.92 90)
			(layer "F.SilkS")
			(uuid "06ad6eee-84d7-42df-8cc8-59f00fdf1adb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "220k"
			(at 2.54 1.92 90)
			(layer "F.Fab")
			(uuid "174b2a20-23b1-4660-8749-e1b2d35b40ba")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9caec2c6-316a-47f4-88a4-a53949ba27a7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7a3152ed-9465-410f-99da-f46e28fd7a03")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cc2959d5-9ae1-4c06-916b-fe7c0bf74cfa")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/b0506013-ce11-444b-bc5e-374e3b418856/a8ed06bc-ef8c-4560-b835-f2ef8ce81949")
		(sheetname "ZeroCrossDetection2")
		(sheetfile "ZeroCrossDetection.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 0.62 -0.92)
			(end 4.46 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e900fe79-7c46-4644-aae0-30b843d468e8")
		)
		(fp_line
			(start 0.62 0.92)
			(end 4.46 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "61e00f3a-2588-4195-8553-c46f98aaa098")
		)
		(fp_line
			(start 6.03 -1.05)
			(end -0.95 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "aeb32fac-c455-4ab6-b0d4-04c871a8e8cc")
		)
		(fp_line
			(start -0.95 -1.05)
			(end -0.95 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "31d3179e-a928-4572-9ab6-c01bbec90ca9")
		)
		(fp_line
			(start 6.03 1.05)
			(end 6.03 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "73c4fdc6-16f6-46b3-8e69-f8f9bc93112d")
		)
		(fp_line
			(start -0.95 1.05)
			(end 6.03 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "eb3c7e59-ab44-43dc-aee3-0507a5dd0e7c")
		)
		(fp_line
			(start 4.34 -0.8)
			(end 0.74 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "24c9e9c3-5037-4451-82f0-30825e8c6bec")
		)
		(fp_line
			(start 0.74 -0.8)
			(end 0.74 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "35837d03-4bea-4db7-bf58-a5ebcbf6780a")
		)
		(fp_line
			(start 5.08 0)
			(end 4.34 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7bea5a64-d3d4-4abc-87ad-e121b173baa7")
		)
		(fp_line
			(start 0 0)
			(end 0.74 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "56687310-9d2a-44b6-ae5a-7626ae178d80")
		)
		(fp_line
			(start 4.34 0.8)
			(end 4.34 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c3002ee5-75d0-4834-8af7-4b0e760183bf")
		)
		(fp_line
			(start 0.74 0.8)
			(end 4.34 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7b0dc90e-947b-4751-90b6-f06a4411169e")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 90)
			(layer "F.Fab")
			(uuid "f5b0ba1a-a92b-4ac8-8d05-9769ee55a66c")
			(effects
				(font
					(size 0.72 0.72)
					(thickness 0.108)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 230 "Net-(J19-Pin_2)")
			(pintype "passive")
			(uuid "0ef8cfd5-e625-44a5-967e-d994d9517df2")
		)
		(pad "2" thru_hole oval
			(at 5.08 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 237 "Net-(R60-Pad2)")
			(pintype "passive")
			(uuid "cd1a8e0b-8e1f-4d91-a5cc-56f89ddc5a77")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(uuid "f8649181-d40c-4568-b90f-60413e40c4cc")
		(at 35.085716 71.06 90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R10"
			(at 3.81 -1.92 90)
			(layer "F.SilkS")
			(uuid "ab2fe588-c0be-4851-a89e-dc583f422e94")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "180"
			(at 3.81 1.92 90)
			(layer "F.Fab")
			(uuid "e2e83bf4-6cec-492b-aa51-70acbf4bc6e6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0e83678d-0fb8-47fb-8ed3-01c27a316c94")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a22e1782-57ae-4892-8e7c-2f9930dadd9f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a2634370-9eba-4ec3-9d13-46d573ef8c03")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1abc9394-30bb-4ef5-a1be-aa230dbd1566/4ab64e29-964f-40b2-bf58-c546b31cd3eb")
		(sheetname "Triac Circuit3")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 5.73 -0.92)
			(end 1.89 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "58965638-70a0-4ee3-a3c6-50f4deffb6a4")
		)
		(fp_line
			(start 1.89 -0.92)
			(end 1.89 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9566c07d-b023-49db-933e-ee0fae402610")
		)
		(fp_line
			(start 6.68 0)
			(end 5.73 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6876bae9-788d-4d7c-a715-15808870b407")
		)
		(fp_line
			(start 0.94 0)
			(end 1.89 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6f0af180-8983-45a5-8a47-3f583fc690de")
		)
		(fp_line
			(start 5.73 0.92)
			(end 5.73 -0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f87ee124-2065-4b07-bed6-3a4e776e19a0")
		)
		(fp_line
			(start 1.89 0.92)
			(end 5.73 0.92)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f699acce-e553-4e2a-885e-c128a8630e9f")
		)
		(fp_line
			(start 8.57 -1.05)
			(end -0.95 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a7e942c2-51c0-4dcc-b490-7bd39674ce28")
		)
		(fp_line
			(start -0.95 -1.05)
			(end -0.95 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "25b9ed17-08bc-4d30-9292-523c96076d7b")
		)
		(fp_line
			(start 8.57 1.05)
			(end 8.57 -1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "245dbb66-7143-4c09-8494-0078a924cce2")
		)
		(fp_line
			(start -0.95 1.05)
			(end 8.57 1.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a5cab57c-62fb-4887-a8c6-d33ecf6b7186")
		)
		(fp_line
			(start 5.61 -0.8)
			(end 2.01 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d3805d19-3664-4389-bd01-ea3b0b04fa21")
		)
		(fp_line
			(start 2.01 -0.8)
			(end 2.01 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1b92e7ff-9814-4d55-93e3-17687d721a4e")
		)
		(fp_line
			(start 7.62 0)
			(end 5.61 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e09970d2-6f19-4e3b-a4ab-db9d4f8ffe27")
		)
		(fp_line
			(start 0 0)
			(end 2.01 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "54862045-f9fd-4de1-899f-03719f5472ff")
		)
		(fp_line
			(start 5.61 0.8)
			(end 5.61 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "88635295-fab0-497a-88ba-7a11d587f328")
		)
		(fp_line
			(start 2.01 0.8)
			(end 5.61 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f4546aa4-2262-4431-92d6-b744fcdbb67d")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
			(uuid "fd5c0dd3-39be-4162-b3c4-8097ab8a06c6")
			(effects
				(font
					(size 0.72 0.72)
					(thickness 0.108)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "Net-(R10-Pad1)")
			(pintype "passive")
			(uuid "9c55b37d-16ed-4aef-82eb-c79ddea0ebcf")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/Triac Circuit3/High_Voltage_L")
			(pintype "passive")
			(uuid "b349e2ff-d1f2-4a73-8cd1-d5518a5c9157")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(uuid "f90928ba-280e-4c52-a4bc-ebea0c78af8b")
		(at 69.287855 137.02 90)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "Q31"
			(at 6.04 -2.444999 -90)
			(layer "F.SilkS")
			(uuid "d893d529-22ee-4b7f-8eda-c05c3bdd3c8b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "BTA16-600B"
			(at 2.539999 2.5 -90)
			(layer "F.Fab")
			(uuid "6362e97c-b2bf-48e5-9dac-9e1200938bf8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "fdea113b-445c-43b0-a554-a0cd863bdd33")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/bta16.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "c7741bf3-9be9-4918-b3d8-fcf290f754f4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
			(uuid "73d139fc-a071-47c8-9839-d1ad0b7d6a14")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TO?220*")
		(path "/4b0c0d83-8522-4ffe-8435-2c6bf5567543/d1257be0-2394-4f08-8984-f580162b15f9")
		(sheetname "Triac Circuit15")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 7.66 -3.27)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3dbe3e93-48a1-4d9e-b7d8-7a89666bef3a")
		)
		(fp_line
			(start 4.391 -3.27)
			(end 4.391 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "29bde6bf-f8e0-4af6-bb79-b7319f9da635")
		)
		(fp_line
			(start 0.69 -3.27)
			(end 0.69 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "20f3295f-b3c4-4716-a59b-4344ddba487e")
		)
		(fp_line
			(start -2.58 -3.27)
			(end 7.66 -3.27)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "af63ff1f-3589-4637-8cec-7ddcf22f26b8")
		)
		(fp_line
			(start -2.58 -3.27)
			(end -2.58 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b099d3a1-bd76-486f-ad1c-f047e58c3473")
		)
		(fp_line
			(start -2.58 -1.76)
			(end 7.66 -1.76)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "16297cdc-1562-4b7b-bac1-659e30d5f67a")
		)
		(fp_line
			(start -2.58 1.371)
			(end 7.66 1.371)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a55fd5f4-be31-4bd7-a352-656690b58012")
		)
		(fp_line
			(start 7.79 -3.4)
			(end -2.71 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d8d70f75-16cf-4ca3-9c60-7ff22999ca1a")
		)
		(fp_line
			(start -2.71 -3.4)
			(end -2.71 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a14a4769-de81-4479-a9ab-3189ae73a81d")
		)
		(fp_line
			(start 7.79 1.51)
			(end 7.79 -3.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4e58c62a-ef17-44e5-966b-648e6657b4f5")
		)
		(fp_line
			(start -2.71 1.51)
			(end 7.79 1.51)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fb9352e8-8c95-4e86-8be1-6de71b842f31")
		)
		(fp_line
			(start 7.54 -3.15)
			(end -2.46 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "44fe43a3-943a-4861-90a4-39d8b4dc5e3c")
		)
		(fp_line
			(start 4.39 -3.15)
			(end 4.39 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4b1b3ded-d3e6-479d-bbf3-a66e243a39ab")
		)
		(fp_line
			(start 0.69 -3.15)
			(end 0.69 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aa26b527-442c-41cf-bbd6-f92f11111273")
		)
		(fp_line
			(start -2.46 -3.15)
			(end -2.46 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a873208d-e64a-4fbe-806b-21ac2c39a0c2")
		)
		(fp_line
			(start -2.46 -1.88)
			(end 7.54 -1.88)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "caca27c8-2761-4007-b498-d146c7820456")
		)
		(fp_line
			(start 7.54 1.25)
			(end 7.54 -3.15)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "98902c69-e441-4b69-af2b-8c72dd23a845")
		)
		(fp_line
			(start -2.46 1.25)
			(end 7.54 1.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "03bbea32-6c82-4999-b5ed-dd54cafb33d2")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 -4.27 -90)
			(layer "F.Fab")
			(uuid "590559dc-22bb-4c28-ba53-9c282105f05b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 87 "/Triac Circuit15/High_Voltage_L")
			(pinfunction "A1")
			(pintype "passive")
			(uuid "698188e1-419a-4be8-8e79-d534c4c15f5d")
		)
		(pad "2" thru_hole oval
			(at 2.54 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/Triac Circuit15/High_Voltage_Out")
			(pinfunction "A2")
			(pintype "passive")
			(uuid "05d2b6f7-f8a8-4eab-9ed3-237bb3c6905b")
		)
		(pad "3" thru_hole oval
			(at 5.08 0 90)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 157 "Net-(Q31-G)")
			(pinfunction "G")
			(pintype "input")
			(uuid "39b2bf50-dade-4267-90e5-32f0bf345502")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(uuid "f98e912c-d5cd-4cb8-bbbb-aea9dd43e96a")
		(at 53.605355 102.4 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R41"
			(at 0 -1.82 180)
			(layer "F.SilkS")
			(uuid "fe684078-0715-4231-a01a-669c8493a6df")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4k7"
			(at 0 1.82 180)
			(layer "F.Fab")
			(uuid "6b9b785d-2f3e-4009-90df-22a4d31f7b21")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Resistor_SMD:R_1206_3216Metric"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "008d394b-612b-48ee-aeaf-d0da05acc777")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "7453b5d2-dd20-4a98-9c1c-60d25fe572d0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "117b0213-8fae-4908-9d25-6ce3de16f1bb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/4a948621-4b4c-41c9-b07f-b928eecc9e1e/de24ad75-a874-4d54-a682-b1d6f2079d30")
		(sheetname "Triac Circuit13")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr smd)
		(fp_line
			(start -0.727064 0.91)
			(end 0.727064 0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2af4d4b5-145c-4343-8c12-d91570737bfe")
		)
		(fp_line
			(start -0.727064 -0.91)
			(end 0.727064 -0.91)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3fc88c56-1781-41c5-8649-b618d0884992")
		)
		(fp_line
			(start 2.28 1.12)
			(end -2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "67a1e3a8-1522-4520-a9ee-9a9664f93bc8")
		)
		(fp_line
			(start 2.28 -1.12)
			(end 2.28 1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9b7961c6-f339-4721-ba04-7205fd8dcfe6")
		)
		(fp_line
			(start -2.28 1.12)
			(end -2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "155ac474-4573-448a-9f25-6e9f39998427")
		)
		(fp_line
			(start -2.28 -1.12)
			(end 2.28 -1.12)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3a3ffdf2-f7e1-4f52-a46a-3651eb37ca9a")
		)
		(fp_line
			(start 1.6 0.8)
			(end -1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5179c551-1662-42ac-bcad-139552fcce44")
		)
		(fp_line
			(start 1.6 -0.8)
			(end 1.6 0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e9d77c26-7e2d-4a04-8759-e1e32b9ed760")
		)
		(fp_line
			(start -1.6 0.8)
			(end -1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "21ad5046-81fd-40c2-b2b7-6642d5a0e326")
		)
		(fp_line
			(start -1.6 -0.8)
			(end 1.6 -0.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "559f6dd5-8dd8-4936-90e4-1a0a70e9815c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
			(uuid "1381d02c-6bdc-4b73-9a58-eb4473dad138")
			(effects
				(font
					(size 0.8 0.8)
					(thickness 0.12)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 122 "Net-(R41-Pad1)")
			(pintype "passive")
			(uuid "a109c3cf-c56c-4973-aaf0-9eddd03db6b4")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 180)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.222222)
			(net 37 "+3V3")
			(pintype "passive")
			(uuid "c68c0e63-371e-47ef-a76f-3d6c445d202d")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-6_W7.62mm"
		(layer "F.Cu")
		(uuid "fcbcc3ab-32c3-4226-bdf5-1075f3e66141")
		(at 44.885716 70.045 180)
		(descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "U5"
			(at 3.6 -2.33 0)
			(layer "F.SilkS")
			(uuid "5eb06ac2-38bc-4daa-88f7-293ca2f6da17")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MOC3021M"
			(at 3.81 7.41 0)
			(layer "F.Fab")
			(uuid "43f5956d-9a65-448b-9a00-0cb16f4e5d15")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "6d8a6149-b7fd-411a-8729-2605d3c19585")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MOC3023M-D.PDF"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "0e8dc2a8-0a33-42e9-82f0-74151c723b42")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "24c66f2e-cc28-4aa3-b583-e78598db916e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "DIP*W7.62mm* SMDIP*W9.53mm* DIP*W10.16mm*")
		(path "/1abc9394-30bb-4ef5-a1be-aa230dbd1566/0262e914-5435-478f-be04-ece49b8102cf")
		(sheetname "Triac Circuit3")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start 6.46 6.41)
			(end 6.46 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a8aec148-d6ea-44f0-b4a0-bb1ff17c0394")
		)
		(fp_line
			(start 6.46 -1.33)
			(end 4.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "31837a37-1552-428a-bbeb-bae8e854f411")
		)
		(fp_line
			(start 2.81 -1.33)
			(end 1.16 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f0291c0b-0817-48b9-8add-9d626885110e")
		)
		(fp_line
			(start 1.16 6.41)
			(end 6.46 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d29329a1-1d01-424b-98da-cf81af8ac33e")
		)
		(fp_line
			(start 1.16 -1.33)
			(end 1.16 6.41)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a3569639-05f0-4b27-8fad-bf516bac56a7")
		)
		(fp_arc
			(start 4.81 -1.33)
			(mid 3.81 -0.33)
			(end 2.81 -1.33)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "272529c4-0f0b-4f13-a5f3-52e5c2a75aee")
		)
		(fp_line
			(start 8.7 6.6)
			(end 8.7 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4718556c-22e4-47f6-b532-0688e4e36ce6")
		)
		(fp_line
			(start 8.7 -1.55)
			(end -1.1 -1.55)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e9db3c60-9695-4b32-b70e-adf08b195e0e")
		)
		(fp_line
			(start -1.1 6.6)
			(end 8.7 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a6699cfb-c952-4410-bac1-292ef6a54460")
		)
		(fp_line
			(start -1.1 -1.55)
			(end -1.1 6.6)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "113bfd08-a027-442f-ada3-0c647d3a9370")
		)
		(fp_line
			(start 6.985 6.35)
			(end 0.635 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f95e5c8b-adae-4c89-ae3c-49d9c42bcf67")
		)
		(fp_line
			(start 6.985 -1.27)
			(end 6.985 6.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2bac8ac4-cbed-403e-9b5d-992411bc6fee")
		)
		(fp_line
			(start 1.635 -1.27)
			(end 6.985 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f04ba2e5-f6b2-4f72-8c60-de2e0890a55e")
		)
		(fp_line
			(start 0.635 6.35)
			(end 0.635 -0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "24fc9754-5e95-4710-b966-b2eba70e05d6")
		)
		(fp_line
			(start 0.635 -0.27)
			(end 1.635 -1.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a9694d5e-f1bc-4a00-abfd-36d99b64d3f2")
		)
		(fp_text user "${REFERENCE}"
			(at 3.81 2.54 0)
			(layer "F.Fab")
			(uuid "276fbe00-ffc0-4e29-9411-43529641fb40")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 112 "Net-(R11-Pad1)")
			(pintype "passive")
			(uuid "5542a5ed-25c0-4282-8683-d94fd2cac1af")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "Net-(Q8-C)")
			(pintype "passive")
			(uuid "fd02da09-45d8-4f2a-92c3-8780224cb519")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 90 "unconnected-(U5-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "05018434-a69d-4803-a9e7-edbff7a44e2d")
		)
		(pad "4" thru_hole oval
			(at 7.62 5.08 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(Q7-G)")
			(pintype "passive")
			(uuid "dc65c38e-556b-4239-a50d-d7bc46b1624a")
		)
		(pad "5" thru_hole oval
			(at 7.62 2.54 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "unconnected-(U5-NC-Pad5)")
			(pinfunction "NC")
			(pintype "no_connect")
			(uuid "32fce07e-1ae5-4cbe-baef-788139f616e9")
		)
		(pad "6" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "Net-(R10-Pad1)")
			(pintype "passive")
			(uuid "ad6bdfe4-3229-4109-a230-0a630385cdb8")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-6_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
		(layer "F.Cu")
		(uuid "fcc139da-dbba-455d-848b-3880779809de")
		(at 25.199997 96.6 -90)
		(descr "Terminal Block Phoenix MKDS-3-2-5.08, 2 pins, pitch 5.08mm, size 10.2x11.2mm^2, drill diamater 1.3mm, pad diameter 2.6mm, see http://www.farnell.com/datasheets/2138224.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-3-2-5.08 pitch 5.08mm size 10.2x11.2mm^2 drill 1.3mm pad 2.6mm")
		(property "Reference" "J6"
			(at 3.1 -3 90)
			(layer "F.SilkS")
			(uuid "8f63a9d2-45b9-49fd-a84f-0ce81346a061")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 2.54 6.36 -90)
			(layer "F.Fab")
			(uuid "320735bc-3edd-4f16-ad3c-e3fa3e4802b7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Footprint" "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "a2612f0e-5ffd-424e-b35c-c21bb3c899f8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "c7c39374-6c02-4b0b-9270-0ff023508f1b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
			(uuid "e2d06a19-972c-480e-a3d5-6fbc1311efeb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(path "/6eb41966-4a54-4fd9-a1be-49d2f272d785/60e4d8a3-c16e-48cd-a1fd-61f2968ecc7b")
		(sheetname "Triac Circuit5")
		(sheetfile "TriacCircuit.kicad_sch")
		(attr through_hole)
		(fp_line
			(start -2.84 5.6)
			(end -2.34 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b3e781c3-08ed-4385-b582-c2b97d93ec98")
		)
		(fp_line
			(start -2.6 5.36)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d2c2c931-5373-4e6e-b53b-dc3746007064")
		)
		(fp_line
			(start -2.84 4.86)
			(end -2.84 5.6)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9e3bc5fc-81c2-4f0c-98db-e85a9abc5d91")
		)
		(fp_line
			(start -2.6 4.8)
			(end 7.68 4.8)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a6cd7a82-a725-4ce1-8b51-5092ad9edc55")
		)
		(fp_line
			(start -2.6 2.3)
			(end 7.68 2.3)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c5edc348-71a2-459e-94d9-e9a971fa74b3")
		)
		(fp_line
			(start -1.282 1.547)
			(end -1.388 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "354297db-4eea-4f14-ad6c-3f6d44ddf0f8")
		)
		(fp_line
			(start -1.548 1.281)
			(end -1.654 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d21128e4-70c3-4ea9-bc21-c93ece76a2fb")
		)
		(fp_line
			(start 4.073 1.274)
			(end 3.693 1.654)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "962282e6-1499-4044-a749-7cf600ae7891")
		)
		(fp_line
			(start 3.822 0.992)
			(end 3.427 1.388)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "71996176-9c25-4b09-b4d3-7c4fe3a9c3f0")
		)
		(fp_line
			(start 1.654 -1.388)
			(end 1.547 -1.281)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8d2d3871-0beb-4d8e-befc-9d2746a7cf8e")
		)
		(fp_line
			(start 6.734 -1.388)
			(end 6.339 -0.992)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "246a1beb-2fae-4e97-896f-53a649d664da")
		)
		(fp_line
			(start 1.388 -1.654)
			(end 1.281 -1.547)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "30b26b02-ece5-47dd-9f41-a5af138697fe")
		)
		(fp_line
			(start 6.468 -1.654)
			(end 6.088 -1.274)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4a58bbd2-a61a-46c6-b342-ae4e3566e1a6")
		)
		(fp_line
			(start -2.6 -3.9)
			(end 7.68 -3.9)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "177093b8-6f94-4b8e-a5aa-3d06bc476d62")
		)
		(fp_line
			(start -2.6 -5.96)
			(end -2.6 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "64dda953-2058-4552-bb0a-819be2f91d1b")
		)
		(fp_line
			(start -2.6 -5.96)
			(end 7.68 -5.96)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2acad453-2228-4b41-8050-9c498eecc67c")
		)
		(fp_line
			(start 7.68 -5.96)
			(end 7.68 5.36)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6fb92d3c-929b-449a-bb49-feda4c0315d0")
		)
		(fp_circle
			(center 0 0)
			(end 2.18 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "8d86a102-4571-4547-ad9c-2a9b4bcb86c3")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.26 0)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill none)
			(layer "F.SilkS")
			(uuid "5e5cad78-82da-4d37-9fed-e608895579a0")
		)
		(fp_line
			(start -3.04 5.8)
			(end 8.13 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e27846f7-2ebf-45bc-b247-96601f54331c")
		)
		(fp_line
			(start 8.13 5.8)
			(end 8.13 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dbd2b43d-334b-4e15-a97d-740fdbd71030")
		)
		(fp_line
			(start -3.04 -6.4)
			(end -3.04 5.8)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fb8c9799-930f-47fe-91ce-e2f2e04177e7")
		)
		(fp_line
			(start 8.13 -6.4)
			(end -3.04 -6.4)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "30ce088e-9745-4c6d-9b38-21eedacbac5f")
		)
		(fp_line
			(start -2.04 5.3)
			(end -2.54 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "db16fceb-7c63-4919-a9bd-e541d791c8b3")
		)
		(fp_line
			(start 7.62 5.3)
			(end -2.04 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2fec2921-8411-40eb-ab63-404782a419ce")
		)
		(fp_line
			(start -2.54 4.8)
			(end 7.62 4.8)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9b40652b-63bb-4d93-8168-4ad7d8147360")
		)
		(fp_line
			(start -2.54 4.8)
			(end -2.54 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "37d67937-d98e-4a61-8d60-b1b479844305")
		)
		(fp_line
			(start -2.54 2.3)
			(end 7.62 2.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a514a394-f3b4-4cd2-b7ad-b679a0740b18")
		)
		(fp_line
			(start 1.517 -1.273)
			(end -1.273 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aa58e981-7fdd-4d79-9a6b-09f8e6d6e4cf")
		)
		(fp_line
			(start 6.597 -1.273)
			(end 3.808 1.517)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9df05da6-c889-4fff-ae32-cec2418a60fe")
		)
		(fp_line
			(start 1.273 -1.517)
			(end -1.517 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b941774b-b269-420a-9006-7ded9c59333a")
		)
		(fp_line
			(start 6.353 -1.517)
			(end 3.564 1.273)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5cca6dce-d249-4daf-bb7c-6413a8e80e86")
		)
		(fp_line
			(start -2.54 -3.9)
			(end 7.62 -3.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f7f7b385-8539-48fc-8872-e48050924378")
		)
		(fp_line
			(start -2.54 -5.9)
			(end 7.62 -5.9)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bb673935-1270-4f34-a3dc-609f27d24548")
		)
		(fp_line
			(start 7.62 -5.9)
			(end 7.62 5.3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "64da2979-4d1c-4d59-a3a9-4287d7abdf3f")
		)
		(fp_circle
			(center 0 0)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "b598d053-6df4-4ca7-889b-cec379dca9ec")
		)
		(fp_circle
			(center 5.08 0)
			(end 7.08 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill none)
			(layer "F.Fab")
			(uuid "6f093fb0-62bf-42ad-84fe-b8f51059f265")
		)
		(fp_text user "${REFERENCE}"
			(at 2.54 3.1 -90)
			(layer "F.Fab")
			(uuid "bdc09678-e7f3-49a8-b26d-3da5457a959d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "/Triac Circuit5/High_Voltage_L")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "b769f2e0-6dff-4f13-8b0f-ebe77a0d9423")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/Triac Circuit5/High_Voltage_Out")
			(pinfunction "Pin_2")
			(pintype "passive")
			(uuid "4ee9e1e8-f457-4bd9-b124-e93e08bd6d91")
		)
		(model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-3-2-5.08_1x02_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 16 186)
		(end 16 16)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "Edge.Cuts")
		(uuid "0fa4f4fd-e8b6-41aa-9179-1b5a4d3dc51d")
	)
	(gr_line
		(start 16 17.4)
		(end 86 17.4)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "Edge.Cuts")
		(uuid "22245574-60f6-4507-a785-954d07a36d96")
	)
	(gr_line
		(start 86 186)
		(end 16 186)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "Edge.Cuts")
		(uuid "33c6702a-0f0f-478a-8be1-9cdee639639c")
	)
	(gr_line
		(start 86 16)
		(end 86 186)
		(stroke
			(width 0.1)
			(type solid)
		)
		(layer "Edge.Cuts")
		(uuid "48bbbf3c-60d9-4c7b-94da-9213207fa374")
	)
	(dimension
		(type aligned)
		(layer "Edge.Cuts")
		(uuid "46ae7f8b-54a5-4691-92d0-da888455968a")
		(pts
			(xy 51 17.4) (xy 86 17.4)
		)
		(height -2.5)
		(gr_text "35,0000 mm"
			(at 68.5 13.75 0)
			(layer "Edge.Cuts")
			(uuid "46ae7f8b-54a5-4691-92d0-da888455968a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
)
